(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 50.8 50.8)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "+5V")
  (net 2 "/Horloge Nixie/USB_D-")
  (net 3 "/Horloge Nixie/USB_D+")
  (net 4 "GND")
  (net 5 "/Horloge Nixie/I2C_SCL")
  (net 6 "/Horloge Nixie/I2C_SDA")
  (net 7 "Net-(D1-DOUT)")
  (net 8 "HT")
  (net 9 "unconnected-(N1-RHDP-Pad2)")
  (net 10 "/Horloge Nixie/K0")
  (net 11 "/Horloge Nixie/K9")
  (net 12 "/Horloge Nixie/K8")
  (net 13 "/Horloge Nixie/K7")
  (net 14 "/Horloge Nixie/K6")
  (net 15 "/Horloge Nixie/K5")
  (net 16 "/Horloge Nixie/K4")
  (net 17 "/Horloge Nixie/K3")
  (net 18 "/Horloge Nixie/K2")
  (net 19 "/Horloge Nixie/K1")
  (net 20 "unconnected-(N1-LHDP-Pad13)")
  (net 21 "/Horloge Nixie/OUT_LEDs")
  (net 22 "unconnected-(N2-RHDP-Pad2)")
  (net 23 "unconnected-(N2-LHDP-Pad13)")
  (net 24 "unconnected-(N3-RHDP-Pad2)")
  (net 25 "unconnected-(N3-LHDP-Pad13)")
  (net 26 "unconnected-(N4-RHDP-Pad2)")
  (net 27 "unconnected-(N4-LHDP-Pad13)")
  (net 28 "Net-(Q1-C)")
  (net 29 "Net-(Q1-B)")
  (net 30 "Net-(Q2-C)")
  (net 31 "Net-(Q2-B)")
  (net 32 "Net-(Q3-C)")
  (net 33 "Net-(Q3-B)")
  (net 34 "Net-(Q4-C)")
  (net 35 "Net-(Q4-B)")
  (net 36 "Net-(Q5-B)")
  (net 37 "Net-(Q5-C)")
  (net 38 "Net-(Q6-B)")
  (net 39 "Net-(Q6-C)")
  (net 40 "Net-(Q7-B)")
  (net 41 "Net-(Q7-C)")
  (net 42 "Net-(Q8-B)")
  (net 43 "Net-(Q8-C)")
  (net 44 "Net-(D2-DOUT)")
  (net 45 "Net-(D3-DOUT)")
  (net 46 "unconnected-(D4-DOUT-Pad2)")
  (net 47 "/Horloge Nixie/A_M01")
  (net 48 "/Horloge Nixie/IN_PHOTO_R")
  (net 49 "unconnected-(U1-3V3-Pad1)")
  (net 50 "unconnected-(U1-CHIP_PU-Pad3)")
  (net 51 "NX1A")
  (net 52 "unconnected-(U1-GPIO15{slash}ADC2_CH4{slash}32K_P-Pad8)")
  (net 53 "unconnected-(U1-GPIO16{slash}ADC2_CH5{slash}32K_N-Pad9)")
  (net 54 "NX2A")
  (net 55 "NX3A")
  (net 56 "NX4A")
  (net 57 "/Horloge Nixie/NX1BCD4")
  (net 58 "/Horloge Nixie/NX2BCD1")
  (net 59 "/Horloge Nixie/NX2BCD2")
  (net 60 "/Horloge Nixie/NX2BCD3")
  (net 61 "/Horloge Nixie/NX4BCD3")
  (net 62 "/Horloge Nixie/NX4BCD4")
  (net 63 "/Horloge Nixie/NX2BCD4")
  (net 64 "/Horloge Nixie/NX1BCD3")
  (net 65 "/Horloge Nixie/NX3BCD1")
  (net 66 "/Horloge Nixie/NX3BCD2")
  (net 67 "unconnected-(U1-GPIO0-Pad31)")
  (net 68 "/Horloge Nixie/IN_ENC_A")
  (net 69 "/Horloge Nixie/IN_ENC_B")
  (net 70 "/Horloge Nixie/IN_ENC_SW")
  (net 71 "unconnected-(U1-GPIO38-Pad35)")
  (net 72 "unconnected-(U1-GPIO39{slash}MTCK-Pad36)")
  (net 73 "unconnected-(U1-GPIO40{slash}MTDO-Pad37)")
  (net 74 "/Horloge Nixie/NX3BCD3")
  (net 75 "/Horloge Nixie/NX3BCD4")
  (net 76 "unconnected-(U1-GPIO44{slash}U0RXD-Pad42)")
  (net 77 "/Horloge Nixie/NX4BCD1")
  (net 78 "/Horloge Nixie/NX4BCD2")
  (net 79 "/Horloge Nixie/NX1BCD2")
  (net 80 "/Horloge Nixie/NX1BCD1")
  (net 81 "/Horloge Nixie/NX1K8")
  (net 82 "/Horloge Nixie/NX1K9")
  (net 83 "/Horloge Nixie/NX1K2")
  (net 84 "/Horloge Nixie/NX1K3")
  (net 85 "/Horloge Nixie/NX1K7")
  (net 86 "/Horloge Nixie/NX1K6")
  (net 87 "/Horloge Nixie/NX1K4")
  (net 88 "/Horloge Nixie/NX1K5")
  (net 89 "/Horloge Nixie/NX1K1")
  (net 90 "/Horloge Nixie/NX1K0")
  (net 91 "/Horloge Nixie/NX2K8")
  (net 92 "/Horloge Nixie/NX2K9")
  (net 93 "/Horloge Nixie/NX2K2")
  (net 94 "/Horloge Nixie/NX2K3")
  (net 95 "/Horloge Nixie/NX2K7")
  (net 96 "/Horloge Nixie/NX2K6")
  (net 97 "/Horloge Nixie/NX2K4")
  (net 98 "/Horloge Nixie/NX2K5")
  (net 99 "/Horloge Nixie/NX2K1")
  (net 100 "/Horloge Nixie/NX2K0")
  (net 101 "/Horloge Nixie/NX3K8")
  (net 102 "/Horloge Nixie/NX3K9")
  (net 103 "/Horloge Nixie/NX3K2")
  (net 104 "/Horloge Nixie/NX3K3")
  (net 105 "/Horloge Nixie/NX3K7")
  (net 106 "/Horloge Nixie/NX3K6")
  (net 107 "/Horloge Nixie/NX3K4")
  (net 108 "/Horloge Nixie/NX3K5")
  (net 109 "/Horloge Nixie/NX3K1")
  (net 110 "/Horloge Nixie/NX3K0")
  (net 111 "/Horloge Nixie/NX4K8")
  (net 112 "/Horloge Nixie/NX4K9")
  (net 113 "/Horloge Nixie/NX4K2")
  (net 114 "/Horloge Nixie/NX4K3")
  (net 115 "/Horloge Nixie/NX4K7")
  (net 116 "/Horloge Nixie/NX4K6")
  (net 117 "/Horloge Nixie/NX4K4")
  (net 118 "/Horloge Nixie/NX4K5")
  (net 119 "/Horloge Nixie/NX4K1")
  (net 120 "/Horloge Nixie/NX4K0")

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 087ab1b5-8f10-4d90-b5f7-da0eafa3689c)
    (at 116.84 78.74)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/e01ea40c-ec47-4225-9e8e-8942f38402fc")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 073b1f6a-6889-4f50-94d5-9f03f19a557e)
    )
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b212fa78-2133-4697-a97a-371c93a555b2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp af7823be-14b7-408f-8ae2-4f608b63de96)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 90a9b98d-039e-4577-82c4-947c803a9dc7))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f49ed84e-99a6-4fa1-b761-05f7829e0f93))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 514a5348-9727-4666-b365-55b61a4277ed))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8843b524-df8e-482a-a6ae-ba7e47caefe8))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 02168343-07d2-4294-83ef-80d508eb1706))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 369b9010-ee6c-4330-8a87-4e98f8ae70ea))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bca1a4f5-ae0d-4968-827a-fb75944c20b5))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 203ddebe-d138-4c43-b8d7-0a8e36af27be))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d26b305-66f1-4344-89af-a6e1948a872c))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 648c2609-280d-40bd-bf1a-08de9ac1598b))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "+5V") (pintype "passive") (tstamp bb38cc21-022d-4620-945a-54c91e17f2a2))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "GND") (pintype "passive") (tstamp 26b1a5c9-e591-4235-a002-8a5438f7fee4))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp 120db33d-d11e-4ab9-8c21-bed108456ee1)
    (at 145.8 115.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 610a3846-187c-4700-81af-de43361b7dc6)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6af5934d-1dc5-4fba-960e-a97e570a103d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb63c6c3-25a1-4d18-b86e-5017a821a3bf)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 3cd80b79-dc1c-4967-be90-6aa96b86a186))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 63d9542c-8d51-40bb-a07a-6f1b43a8fef2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 431e9ae2-c293-4ff8-ac5d-b9b3e8e4b5bc))
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 1457617d-5ced-4d0f-b979-e99a0b26e831)
    (at 90.25 48.3 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/9207a63a-9d04-457a-af85-e605b977a44d")
    (attr through_hole)
    (fp_text reference "R8" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 420720ba-4fb8-4a24-8258-419c3890648d)
    )
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 33bb778f-8568-413b-b83f-bc05a44473a8)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 83cb9858-09af-4912-8355-36f4abc76554)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1325cf75-48b8-412f-b0ec-c0ccf2c96774))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3cfa6591-6222-4a5f-abe9-b5485e240087))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d621c18e-62a1-4939-a367-298053004781))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fe178c6c-84d3-45c0-85f8-ea6839b75d80))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d5ecec6c-08e2-4648-a7c7-375f517ca8b7))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b1a50c52-f371-4dfc-ba18-76e4b26daec2))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c80663a2-56b9-4315-8382-607be7656fb4))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30151094-3672-4657-96cb-8f656ca62b82))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d838d20c-9518-4b88-8926-62d4d739c92b))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 105bba36-78d5-4dc6-b2ed-9bb371864598))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1f904383-6053-48db-b16b-39e8b00f55c4))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 727d60e7-d760-49f7-af41-8e81a0f758e0))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6cd9e212-432c-4eed-b2f0-fd179a87e239))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c8b897b4-ad8b-4323-b959-96349320f108))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e0de5532-d67b-4fbc-b267-b65f6cef9f19))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 69c51c06-bcb7-46bb-82d2-abfdc0a9ab0e))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pintype "passive") (tstamp 3700650e-b111-4c49-bf5c-61dc763de81a))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(Q4-C)") (pintype "passive") (tstamp c34ab31c-2510-4c50-9f9b-0a03cb9e36b3))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp 16836fe4-83f3-4952-9076-39bab15df500)
    (at 110.03 40.37)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/68506607-bff5-41c0-96fd-a704d99595a8")
    (attr through_hole)
    (fp_text reference "Q5" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0127308c-537e-4d1c-beab-c88591c8d7cd)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a9a4992d-39a1-44d1-ae52-0d3d30be8549)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 202d646c-2b2e-4035-b82d-4d8498b083f0)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dec94bc2-0a99-4c23-a7e0-e65192546645))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e42830ed-ceb3-4769-b25c-527238f60633))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ba14efdd-4c36-43da-a7dc-6ce0deafb7d0))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c943dda9-8fd9-462c-b780-811547c08ef1))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e59d9b04-25e4-4495-a1da-6dfe2c62745d))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3c3a3d62-19ae-4c6a-be6c-50a3c0b899be))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 762b2f95-20f4-4dab-9371-6b9c3c2e1c3f))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c0cc5036-de7c-49d2-a45c-db43800a63b9))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fe475909-caf9-460e-8bce-260efffca7a9))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8333b7d1-6787-4071-8e61-dd7692e9c285))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(Q5-B)") (pinfunction "B") (pintype "input") (tstamp 9bbff092-43b1-41a0-97ba-133a690a6f97))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(Q5-C)") (pinfunction "C") (pintype "passive") (tstamp a4dedd20-4298-4813-b738-1fb08974f216))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "E") (pintype "passive") (tstamp ce61eb15-6bb2-4b38-a3ae-8131db6dc283))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp 17ada81d-3c4d-491a-86bb-170864275c61)
    (at 132.03 46.59)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/123d2b82-2043-4b75-83d5-5f1b4ddd38ce")
    (attr through_hole)
    (fp_text reference "Q8" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b204506-733b-4a52-b085-37a3fbb14837)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3892424f-8ce2-4596-b412-fb35a57ba057)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4d9e26ab-8754-4fbb-9d3b-06462d4c8b26)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6950c4bb-345a-45e1-b7bb-96142c0e6ca3))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6f6bec94-e117-41a7-b81e-537533769991))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e1c8fcd-5f0e-43eb-bdcf-e7f7e086080b))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e148edd5-6824-41ac-af83-21e1a1e3dbe3))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b115e667-0cac-4ecb-9d66-be77966ee261))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bd8d4b7b-18c2-4f8b-ab94-d14fbdff2401))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b2d9b383-6514-4b31-9956-709cb0a50fb8))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c00b421f-9f3a-4329-ad0a-38c66f131ce2))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 961b66ac-a4b9-4809-b42f-b0cf44e502db))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2d99410-6a49-461c-8906-a1d71657b291))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(Q8-C)") (pinfunction "C") (pintype "passive") (tstamp 1f1aa3b8-f311-44aa-ab00-25afd0999a85))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(Q8-B)") (pinfunction "B") (pintype "input") (tstamp ab4d8f53-579c-41c1-8ec6-238a47a14f40))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pinfunction "E") (pintype "passive") (tstamp d8428fa4-63f4-4cca-b295-f0e300a8ca71))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 17d9b8b4-4197-4d7d-b36d-db9e33633ae4)
    (at 115.35 53.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/21430ac9-3e5b-4a1e-a9a5-64a87dd4510c")
    (attr through_hole)
    (fp_text reference "R11" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a3d8df9-559d-48f3-90d8-4e3d3f07b7e5)
    )
    (fp_text value "470k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ac21d6b-47ac-4165-923b-c06fe1a0f8f3)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 77a10b00-0882-4181-9247-78fbfdcaff1e)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 201a71f0-d17e-4a4b-b58a-533a7fe84373))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b69a48f5-7eb0-4845-ab79-250a661c78db))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c010cf30-bfd9-47e9-b3a5-2b873b7fca23))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 493408cb-df9b-477f-9f31-efd75d206bd2))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1ecbc0b5-13b6-4b98-ab56-9ef4383edddc))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c637fab-68da-4df2-b778-55c4c86a0084))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7886406b-55b7-425d-a5e2-a7e4686276d1))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d969fcbf-d678-4048-9f90-e05911e722b8))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 869f0487-a05b-4a1a-b96f-4b60f39105d3))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0107bba7-c6d0-4483-b2bd-5d0c58fe86c7))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5819ca29-6b7f-46b4-8138-7f8ca9a25ba0))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 64aa74a4-1941-45b1-b758-b0d139dba0af))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffe98144-6cab-457d-a972-edb70dbf6ed8))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c70674c-58d7-45cb-8fc0-b4321310a831))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bcb64268-1083-4d9a-9278-851f6b112470))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b4cd7cf-12ff-40a8-90bf-a9fe9a3e07ec))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(Q5-C)") (pintype "passive") (tstamp 1437d04c-e8f5-4258-a7ad-a2b764f3b970))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(Q6-B)") (pintype "passive") (tstamp 7c3adfcd-4887-4370-a6ff-e912ba12db1e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical" (layer "F.Cu")
    (tstamp 202a74b9-4421-4fc2-9165-dbf21c18a5ef)
    (at 148.59 85.725 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=5.08mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 5.08mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Photoresistor")
    (property "ki_keywords" "resistor variable light sensitive opto LDR")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0d92da0c-98ef-4468-a6f4-731ddbae0fc9")
    (attr through_hole)
    (fp_text reference "R17" (at 2.54 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ef66d74b-0b21-485a-ab71-1b30e6825a2e)
    )
    (fp_text value "R_Photo" (at 2.54 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a0b688c-ebfb-4f32-833a-e084b2d9111a)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2bd3c4c-c4d1-4cb2-8ba2-e98ae213783d)
    )
    (fp_line (start 1.37 0) (end 3.98 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c6715d6a-7953-4287-91e9-95796fc4a5db))
    (fp_circle (center 0 0) (end 1.37 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 573066c0-b16c-4118-83aa-93cffcf4004c))
    (fp_line (start -1.5 -1.5) (end -1.5 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 65b984a1-2c5f-43c1-8352-efdf8d64e5a3))
    (fp_line (start -1.5 1.5) (end 6.13 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 51ba26fa-f91b-4f8c-91e8-5f208696077a))
    (fp_line (start 6.13 -1.5) (end -1.5 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 01eebce0-346d-480b-a893-8e1785060101))
    (fp_line (start 6.13 1.5) (end 6.13 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 604b2f46-1280-4df8-8f77-5d200e67f113))
    (fp_line (start 0 0) (end 5.08 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp af75ff60-178d-4afb-b03e-c87afd752991))
    (fp_circle (center 0 0) (end 1.25 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 2ef3b60c-0aec-49a5-bcc8-5ba520ac6c58))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pintype "passive") (tstamp 2f637e81-b8c3-4b93-8970-c2601a51c4b2))
    (pad "2" thru_hole oval (at 5.08 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "/Horloge Nixie/IN_PHOTO_R") (pintype "passive") (tstamp 96830f7e-03be-4273-af70-fa03fa1a530c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P5.08mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 22abdfc4-ba34-43e0-b2be-8bd2c2076eb5)
    (at 148.59 76.47 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/959a1c7b-f39c-4c34-be81-e0dd61fc20ba")
    (attr through_hole)
    (fp_text reference "R18" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a718dd7c-cf3c-48d3-862e-f76adb6a2f1f)
    )
    (fp_text value "10K" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 707540b0-6b3f-4eed-b6e6-dbf4d287746e)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 398a8d3a-7a9c-4019-91d0-33d3d4127997)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0574048-7edc-4387-b36a-9ac4f3c48102))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 355260ca-adf3-4034-abcc-0a28f86cd254))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f134b448-01c9-4843-8860-6a88558e632f))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b1d9dab-dd71-4406-ba44-99b225ae9a96))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0193fffe-474d-4257-8247-31bd56f4038e))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a345f40-966c-4f66-889c-ed0470047d83))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 632bfc39-4950-4f66-bd67-1af611297f60))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cb543ab3-dc4e-41a0-8238-d9d60571cecb))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dcbfab3b-2bf1-4b8d-8ca3-1856bdbb5413))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b64bb646-033b-4290-8335-dbdda2845bf2))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc2f4d79-47a1-4a1f-b105-1c1ac5da02fb))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4f6ccd89-c6b5-4465-8f02-9a53093658dc))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bc636664-9a0d-4fa2-846f-959291999746))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2c960467-de80-4f1b-bd39-3a3ae7595952))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fadea38d-64ad-4a37-bf54-fe49fc993ac1))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f847cf7-1ee3-4df9-a2ad-2e2f16af6863))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "/Horloge Nixie/IN_PHOTO_R") (pintype "passive") (tstamp d44158cd-7d90-44d3-8450-69f3408d22cb))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pintype "passive") (tstamp e728157b-5e34-4d31-9d74-eb6e7f24e303))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp 22ea8624-cd70-48de-832b-f848bb1c4551)
    (at 62.8 67.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (attr through_hole)
    (fp_text reference "N1" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 525c323d-cd5d-446f-8a87-73db5ff6be92)
    )
    (fp_text value "IN-14" (at 0.1562 -10.0862) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp ffd53193-241f-441b-be38-a7e8405a7b8b)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp d762bbe2-5006-4b33-b06c-866502a093a3))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 2202a913-70a3-4cc0-a814-0978f4c2d8fa))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 0bc697fd-ed4e-4a36-8258-566fdc6ae584))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 4cbf6695-d049-4c17-b62b-49209b2ef18a))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp a82cecf9-aeee-4c4d-a401-ac22822debdb))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 7423cea4-2ecb-4927-85a3-e54c78cec3a4))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp f1abe772-debc-496e-9a4d-d7b1b8bd55d8))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pinfunction "A") (pintype "bidirectional") (tstamp 2d6bf537-ea1e-4d07-ba7d-6cf9cd8a9035))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(N1-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional+no_connect") (tstamp 5d9828e4-7f1c-438e-9351-f19c1218bd03))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp 11f14eee-99d5-4d5c-972b-d24d372b4332))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp 85007f62-d7ef-4cc6-85a4-3625e157dc80))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp bb24f932-6720-4a5a-8e2d-7e71bc579bd6))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp 574b65ae-7635-434b-90b1-d35a97ed7d59))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp ccb5145b-43e3-4704-9d17-9fe8286da12c))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp e13f382d-60fb-42ef-95b5-0772e8fc3bff))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp 27021830-6eb1-44f5-b571-83093570ddaf))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp 096c2647-db28-41e0-896b-6b767f4aab34))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp 03f8a145-cdfe-4ab6-baa4-e9e4b3963079))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp 5a45e9d8-1f3b-4207-9c30-2559564eddd6))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(N1-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional+no_connect") (tstamp 5c9d6a0e-87e6-42f0-8a72-6551ee67448f))
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 3bce24ba-64e2-44a5-92bc-fde16b260451)
    (at 62.23 115.57 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/c3280cc1-b9fe-4ecd-84d2-4de8d66c519e")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a7a7e98a-87cb-4c75-b672-fd53caae101a)
    )
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9d2161a-de06-423c-859e-decfc3baeed6)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 05ab5cd9-90d6-4eaa-9f86-cb108026077d)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9e2a1356-22eb-472e-8be3-82c62f5b1137))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2de842ee-3c89-4374-8230-fe02f83de711))
    (fp_line (start -1.33 1.27) (end -1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8de37a0b-a63b-4c24-a9be-7c402ebcb115))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp af03d97d-c524-4da2-a25e-6e711fe1414d))
    (fp_line (start -1.33 8.95) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ba614d58-816c-4183-9533-daae8f020285))
    (fp_line (start 1.33 1.27) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 82c2759e-ead3-4b3d-98bc-7b014e37cb1e))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ac5c2b1f-0511-4e9b-a212-5c356603699b))
    (fp_line (start -1.8 9.4) (end 1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1959a9a3-0e4a-4f61-9b0c-b0a59c5edcfb))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 511a3b9d-ba64-471c-b166-775fdfa7199d))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 64a0317e-0172-47bf-9ff3-0edb6d4b2c63))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c5dd23a-aec1-45dd-a88d-ad560c3669ea))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp edcc2c4d-13c4-45af-ab73-42e94b71d067))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41004812-2eae-4dfe-90bf-7d697da8a2c9))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb80e58a-dbeb-401f-bf35-4974351dcea6))
    (fp_line (start 1.27 8.89) (end -1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 253d7bd4-6d9d-4b2d-8a8d-c64d6ffd8972))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive") (tstamp aef3300d-ecf8-4b4d-a510-3777fb6a12c3))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/Horloge Nixie/USB_D-") (pinfunction "Pin_2") (pintype "passive") (tstamp 9ec60a40-8e54-433e-81a3-8e827d994d9a))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/Horloge Nixie/USB_D+") (pinfunction "Pin_3") (pintype "passive") (tstamp 7b50416d-ee4b-4299-b368-56b4889f6c6d))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp ff29d32f-7393-4fc7-a7d8-0659b58cf015))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 3d02bdd2-a6d2-4394-829a-6670310af6f9)
    (at 62.196 44.054 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/8be7a2ea-b82d-40b8-a825-92428c1d04dd")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 94051738-4399-492f-9a8e-c50ec6882ee2)
    )
    (fp_text value "470k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 954e57f1-0e80-4e28-9e37-35b4bd22be60)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a0f78759-219f-4ae2-9b7d-6f9e1bc92123)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1ca5f501-0549-4585-b1c0-91fdcd69653c))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a5d52b1f-f24d-4052-ad46-b657db161bf1))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 457aab2e-dbc4-4d45-8444-7129e15b3602))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a1dbe6f-969c-47ee-bd1e-feef3b3162a9))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 79040812-a207-4c4d-9c58-c1664cf85705))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f03f65ee-548c-43e0-a5f6-5e168b61ccfc))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp de04cfa1-317a-4731-a2b9-0f9aa88563b7))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b941b62-fb91-4986-bf5a-b0bdd0a28101))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b479a947-7854-49d9-94f7-8ccc7eb2ec95))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d901681f-034a-4162-ba40-b2c6e739d166))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9dedb1d-41df-4d8e-807d-5845495d0523))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 30b30230-4dfc-404f-896a-04523fd2a496))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a8c29259-4eb8-4554-a47a-b38a7fae990a))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 01d34d14-ed1e-45b6-94d5-f5991f06961d))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77a33a3a-0bd1-479b-95c2-fd718251da61))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0bb22f60-aa1d-40b4-974d-95bd636e7821))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(Q1-C)") (pintype "passive") (tstamp 9edf7c62-bc4b-4430-bef1-9aa4ac0b712e))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(Q2-B)") (pintype "passive") (tstamp 23a1ad39-35c9-453d-8f2d-2c17f9275851))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp 40a67ad3-831a-49e2-aff9-0c6cc4bcaa25)
    (at 138.8 67.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (attr through_hole)
    (fp_text reference "N4" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp e5318c26-5098-4fcd-8eb2-e4ba167c4559)
    )
    (fp_text value "IN-14" (at 0 -10) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp d2b9351b-486f-43ec-bce3-77853761e657)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp a230036c-4a6a-412b-8de6-05d5beb6a20a))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp fe298f74-989c-4df1-9ad9-64b1442f6ce6))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 9232ec21-e9c1-4765-938d-f86845b9cc71))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 35f1a105-b9b2-40f9-923a-cdc0aca94a1a))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp fd1f9c86-4d76-4bab-af39-0d5739106091))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 4507859b-b48d-417b-b526-9b49aa223ee0))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp a9908f96-ea24-4d97-bd92-1feb9401541b))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pinfunction "A") (pintype "bidirectional") (tstamp 05e9433d-deaf-4ee8-8618-61a374e0d3fa))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(N4-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional+no_connect") (tstamp 733bea87-eed5-43b7-9b3b-36dfa06e8afa))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp fc615abc-7fa9-43b6-a6dd-dd61b405e492))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp b40def4b-eaf9-45e3-80c6-aff77b668052))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp bed8354d-aeb6-4a3e-a3aa-4133d144d3f0))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp 6577efab-b29c-4745-a11b-6e89236fb9df))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp 8f62d8fb-d08b-4fe5-a7b6-94fd18a9e453))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp faf10cf8-dd99-4720-a542-61e758fdd562))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp 414ce39f-6122-4797-a614-f3c491dd7ab2))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp 03dde198-71c3-487d-a526-6a9ca1f9913e))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp 0d85cbbf-9673-4817-8f5d-cc12c22f96b2))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp b58798ba-9839-4762-bea6-2b47106b4726))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(N4-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional+no_connect") (tstamp 0506b9ba-5956-433d-a436-346ea4c5bf84))
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 417376b9-e89f-4dcc-872b-38a6432938ef)
    (at 85.09 78.74)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/86e998ae-f816-45bf-a877-a5766caf6510")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89a8f06a-41b7-4d31-bc11-562dcde91fd1)
    )
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 033f7f73-658a-4ce7-9437-3a9e513cd620)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp e7b17576-2344-4533-9c62-dc7d7167e017)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c25f3fa8-41c3-495b-8824-3c3136f9f9d3))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3f6c298f-90b4-47bc-a35d-ee8914160cb7))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2d8f1cfc-5fd3-482f-8f86-c57ab0afbc47))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 231fc20b-59d5-4f42-b7f6-6e83bac76f78))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 661003a5-ae5a-4e01-b812-c857da7bb87d))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1e925e38-cfe4-4e3c-8823-f6f4716a82b5))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 44698cdc-8a99-4591-b393-32a5f4777afa))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b67214ab-fe43-41a8-9f6b-6821cb88bdab))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c76688e9-53ba-4b5d-a3af-4c2f73c4d49b))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d2c58270-ad94-4b8b-95a1-53732d95f4d1))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "+5V") (pintype "passive") (tstamp f55dd8cd-ce11-4d7f-ac5d-f86d15e6f8c0))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "GND") (pintype "passive") (tstamp cf576b24-3fdd-4574-be96-36b9da1ba18e))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tstamp 41fbda8c-2d48-4585-b6f6-17e06c8b0de3)
    (at 62.8 67.8 90)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/ec147e4e-86f8-4c34-84ff-408c219efc16")
    (attr smd)
    (fp_text reference "D1" (at 0 -3.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c77e59f-5d94-441b-98d2-6c0a71a68f4e)
    )
    (fp_text value "WS2812B" (at 0 4 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca740699-50a0-4e6e-85b7-2fe1931b8193)
    )
    (fp_text user "1" (at -4.15 -1.6 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3791819b-5254-40dc-91f1-3f8ca54a1dbe)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.15)))
      (tstamp 98e9e9c2-68f1-4026-8a2e-83ce57576873)
    )
    (fp_line (start -3.65 -2.75) (end 3.65 -2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 956346d3-fa41-4181-92ed-5493ec80ffc4))
    (fp_line (start -3.65 2.75) (end 3.65 2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 63cbd06e-99f5-42b9-b4f7-96ff90a5d1cb))
    (fp_line (start 3.65 2.75) (end 3.65 1.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee976f95-891c-4c39-9cfb-68fab2031079))
    (fp_line (start -3.45 -2.75) (end -3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 75f90b6c-7beb-411f-ad62-96f69ed21e2f))
    (fp_line (start -3.45 2.75) (end 3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 96c36ba8-5739-458d-adf8-3e0c55b8bd41))
    (fp_line (start 3.45 -2.75) (end -3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5307353c-105b-440f-8143-40bafec6ec26))
    (fp_line (start 3.45 2.75) (end 3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9077e8f7-8b28-4fc1-b972-f4a801daf1f8))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e110aa1d-918a-46da-a991-1e6365b15f98))
    (fp_line (start -2.5 2.5) (end 2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ca8ba961-b021-4099-b827-dc13af66d398))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06e49138-2b54-4ccb-8841-7ef79307b3c8))
    (fp_line (start 2.5 1.5) (end 1.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 712555c4-8299-42fc-8b3e-30404a6b33b3))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 156d8bef-3110-456d-8f38-15f19aaf948d))
    (fp_circle (center 0 0) (end 0 -2)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp cb266b6c-60f1-4f69-b71a-c8cca72d341f))
    (pad "1" smd rect (at -2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in") (tstamp d7b668c8-9079-4c1c-a7be-78cd06f68747))
    (pad "2" smd rect (at -2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D1-DOUT)") (pinfunction "DOUT") (pintype "output") (tstamp 451bd86e-05f5-43da-8a52-3dfa3aa5bc96))
    (pad "3" smd rect (at 2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp fd470d97-4d9e-4dcb-b936-5ca5495299ee))
    (pad "4" smd rect (at 2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/Horloge Nixie/OUT_LEDs") (pinfunction "DIN") (pintype "input") (tstamp d745c3ca-5f07-4218-8528-06827132bfaa))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp 495ac295-a08b-441b-9d36-c3399edf2412)
    (at 55.8 55.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 519c88f5-c417-46a1-ab09-ad223f8bff37)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e9d0148-2f7f-4583-9023-3437aba5dac3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f6ebf08-e939-45c9-a4a8-4a4107b26f41)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 06f339d7-50c0-4602-bb31-dc7c61ae33c7))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 9b02427b-df53-4ec7-9eb6-46428f839448))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp 2dda3d03-b270-4d72-83c7-06e4912d6032))
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 4d2515dd-7058-4b5f-8f92-2ffe6290e328)
    (at 135.75 30.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/ed433585-dc61-424a-820c-37cda7e01adc")
    (attr through_hole)
    (fp_text reference "R15" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53131a47-7177-4b3b-bf72-890d6b1a2e64)
    )
    (fp_text value "470k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e2a37fe3-b236-4a91-b020-c1b3aba646c2)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6b7fdb0c-0109-44fd-807a-71436d9c029e)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cc5287a5-ff6f-4ef9-906e-8b87cdf5a80f))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 63fa5b44-c3c1-47d5-9d7b-2c21dfeff3e7))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c3fbc296-8ca0-494d-86a5-c10e5db5538e))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b8e06317-132b-4c68-8fec-67c361aa35d9))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6aeae7f8-4817-499d-a0b6-71c730182153))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2d29c09d-7ba3-4bac-b3fe-d4cca190879d))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d703ff38-5778-4303-9daa-30c8c03ee222))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0269df2c-a76c-4999-bcc6-08d3b371d066))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6b3a79d8-0d18-4341-acd7-19f59705e739))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 74736bd2-835c-46f4-9859-cd11ef99a7bc))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cade4b19-797a-4e1e-8e2b-0d60e2c0ace3))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 991bc336-07ca-4233-9442-e2a347d3f35a))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eeaf9968-b20e-4376-ae90-14c9641d32de))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f1f37c52-482b-4e7e-80c0-539b0fef5abe))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce1b8098-4e6c-4e4f-b7ac-dbb66acf7045))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5b79c54f-f466-4219-ba2b-b86e4795eb7f))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(Q7-C)") (pintype "passive") (tstamp f8c30d13-8602-4693-b391-35c69dea6ecf))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(Q8-B)") (pintype "passive") (tstamp 24ddaa66-f6b5-492a-b561-d85d3d8f11f9))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 506569ea-ef04-4198-854f-4203965c7528)
    (at 109.45 53.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/5b595f8e-9ce0-4344-b7f5-7126c012a731")
    (attr through_hole)
    (fp_text reference "R9" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7cf0bbad-7ded-43b4-b55b-05d0e10a027b)
    )
    (fp_text value "33k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b40989ee-a884-442d-a9bc-1ad3960d7b75)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp caffab35-89ac-4597-a6b5-c5a6264184b4)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a853c721-343d-497e-90d1-17a164878ad9))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 64b5ed48-ae43-451a-a692-612bd0026013))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b3e1502a-7039-4bc2-9620-3d89d5d8b346))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp faadb3df-3293-499f-9e66-d7b086deeac8))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ad790c7e-6c9b-496d-a551-fc08205c22e2))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 82910bb3-b615-4143-b71d-dfdd3dcfeb77))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7d3499f3-dd3e-4f93-8eaf-f0406e0f1a43))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c791c440-31fd-43ab-b177-2b603ea49bca))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d0293577-1765-4ffb-a9c4-4b653a5f9aae))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a7fd275-1c86-4cc5-8465-28ac4b840af3))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76e81e41-4cad-458e-9c1a-ca7ed58392eb))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1f1ae99-3832-45a7-835c-5fb264d45343))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 23ea44a0-fad6-4bbc-b898-f22e3a2c2bf0))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9cd3c7d7-2bc2-4199-941a-b51671cc484f))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3ba09013-5e19-4686-8dc5-0f807d615124))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8b4d12de-99fa-445f-8bb6-e3358ef28a6c))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "NX3A") (pintype "passive") (tstamp 1613fea6-d2d6-443d-848b-e1d1a01b72dd))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(Q5-B)") (pintype "passive") (tstamp f8b29950-16f9-4673-ad02-b6cc1c158172))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 506a9f0e-a489-404d-8b6f-76e30845ec76)
    (at 51.274 45.832 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/1669c59f-5ab0-4823-843a-fa1ab299c80a")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3a715335-773c-4d1c-9a6c-c5554e6e65e3)
    )
    (fp_text value "33k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d47e8a67-9ead-4618-95ad-d4a539fa31d8)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e6f072c1-9bab-4b45-a9bf-ef21be9d5547)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 512c7827-ded0-4929-82f1-e9d49fa8b52f))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 12f03561-e813-4a7f-ada9-2554926111fa))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cde8b2a3-eff2-4589-b170-39e3b6971a20))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 94622dd8-70fc-4c5b-81c1-5526cb2e8382))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d6db3623-6e79-482b-8e68-622677145658))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5554560e-543f-46f4-b112-2480ecd711f9))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a27308af-e1d7-49d7-b934-65aaadc7989e))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bbe457a6-7b54-4379-aa86-3dc1e2ed9d2d))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b7330cc5-9342-4224-8909-e11cd2ae5806))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 163944ea-b87a-493f-8946-b01d2bcd6cdd))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db759eae-4ae4-4fd7-b0c8-0c54d17e8dda))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2f3005bd-92c4-475b-91ad-5644ea56869e))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2168af3d-aff6-4fdb-8906-84a875b70841))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 51e88ee8-c4b8-42e3-af3c-e19bbd6947dc))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 18b50d05-b803-4bc9-ac51-ef93637c2e4c))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dfff361c-8de4-4264-b84c-84ca7dab0a96))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "NX1A") (pintype "passive") (tstamp 895bc160-91ac-4404-b8b6-abda17347409))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(Q1-B)") (pintype "passive") (tstamp b827f9aa-4fd1-42f8-a112-d7094cde6445))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 5f551a0f-26d0-4562-9b7c-97a9f48b2cb5)
    (at 66.26 44.054 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/02787926-227e-439b-a8b3-3510c1c1b9aa")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 583e028e-177b-473d-a760-42399a85ed04)
    )
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e30a7524-45a3-4c72-978c-d5410c8e8b95)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce7e3c16-4d3c-4f6b-93e0-c72e0d445515)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1348da06-2d78-460c-812c-3a366fb30532))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 74d15ea2-c414-47ae-8ad2-c1684362187d))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40e5784b-699e-4018-8f6e-6707d0cbaa14))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d6bc9bce-1251-4fcb-a090-f055bf17b7c1))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e18d997-bb70-4290-b1b3-2b175130185b))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 531c42de-e0c8-417e-b9ff-b07e45ca855f))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ac083155-d008-4ed5-aa4c-3091c348c3f6))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 760d503b-a95e-44f9-95e1-885ece308853))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3ec79e88-081e-4499-a4db-30df7126aa19))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4cddd7a7-b57d-4d62-9984-9f67cd6639a8))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db07f7f5-bf41-4eef-a001-69bfd34fd6ad))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 785c036b-7328-45bc-8c40-1ec02ecaec4d))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 89036a9c-13d0-4ada-9017-5ead7e3ac914))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc562f62-1004-4ef8-b484-a8f8a94a037d))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7d597bc8-0b55-49a2-9f5e-c3019b5c4d43))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc6c5cb1-7ae3-4dea-92e3-e308b9e07405))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pintype "passive") (tstamp 48ac24ea-7a1b-4771-a0c3-6560919cb16f))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(Q2-C)") (pintype "passive") (tstamp f62fbb62-a201-4ece-8c77-02a76e5f599b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp 635851a9-a24b-4278-beed-fe37664e46d3)
    (at 55.8 115.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 533b6270-ef72-4168-a135-07e9385184d8)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e4a28d3-f015-4209-85b2-8d4d3004d540)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 356ad0b8-706b-4ae7-bf83-2ed9b67ff507)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp bfceae83-813a-46e5-bd68-f2b474feea8b))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp cc5d37f8-159f-44e5-83a9-878d8863c119))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 01cf929e-46e5-4063-a2dd-25cb9e619b1d))
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp 74fb2fa8-62b0-43e4-8519-5f77640f35f3)
    (at 116.8 67.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (attr through_hole)
    (fp_text reference "N3" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 11012e8d-1c0a-4495-83cc-a460757011b8)
    )
    (fp_text value "IN-14" (at 0 -10) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 2e577400-89a2-4cf8-8cdf-78a4e41a35a2)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 177e4d1e-57c3-473a-9aaa-ac66f1fb94d0))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 9033f7c7-558b-475b-992b-c73854dbcd0e))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 3a29eb3f-1ec0-4c6e-96e9-9e95fa95654d))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 8e7b0875-7b6c-4a07-9516-ac6e5816cadb))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 300d0f3c-4975-4298-9395-f3866cc6ded7))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp f9a7dc4a-ff81-4ff4-8c81-7e78fea403c1))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp 43af299e-2e4e-4d49-8ee6-ec2e3979c35e))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pinfunction "A") (pintype "bidirectional") (tstamp d1b2f7a1-5e4d-4d18-bcfb-6a7d29e08444))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(N3-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional+no_connect") (tstamp 0c179683-158b-483d-941c-43ffe64638c9))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp 8907e7a1-ee30-4f1d-abcc-33bd59314e7f))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp 84bb1569-9ccd-4efe-ac50-eb8c9bd2ec97))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp 7eb021af-1672-4020-b879-e4e0d8dd00a2))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp cd0ab4c6-5dfe-428a-903f-38c40c58d8c7))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp 921b1fad-deed-45b6-82e1-3d1dc28cb420))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp 99229686-659a-4b87-b973-d1c898b2ac14))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp 025f991b-57ba-4b2f-8b9c-561c32a915d1))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp bd0935dd-d4c3-4627-8970-d76e90b72d7e))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp 40b3bea3-17af-4475-bbe3-7924762a8b6f))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp 5e5cac2f-4271-43f7-931d-d7b2bb9e0b5a))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(N3-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional+no_connect") (tstamp 2454ffc9-3e12-4601-b393-28b05d8ea880))
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 76b0619a-f2de-4a16-9b91-cbb5a1e7b754)
    (at 81.3 48.3 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/cc0c83d7-9b8e-4c15-829a-dc5dd86497d0")
    (attr through_hole)
    (fp_text reference "R5" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 48860163-4770-4bb5-b0b7-221e3845ffde)
    )
    (fp_text value "33k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 715d01c5-6da0-4fda-be23-641f7d64add3)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c0928c8d-9875-4701-92e8-60de9712dcb7)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3eb3fccf-1d2b-46b1-bafb-6fc774308382))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c36333cd-405d-484d-96de-652047850afc))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 18d80cd5-31de-45aa-aae3-4ffd462628bc))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 95f4eb65-bea5-485a-a46b-04d6e832c83c))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 207787fd-3a0b-4840-a7a6-ca397622fc92))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2c083d18-5c87-48ba-9fc9-a6f16a438167))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 63f43b7a-05b2-4bab-991d-ffbe40097161))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2acba259-b55e-4e69-931e-0784255845b7))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dea34a9e-c64c-4d72-96e6-a4acff3dc648))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c432cce7-2b69-4df5-a82f-2eef82fad4ae))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06d5571e-0de9-4941-8378-d807a484dcf5))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dbfc241e-f033-47aa-aab1-9bd449e0b44d))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a90f85af-2415-4478-b12a-40bc47e5c6af))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b029d83-66f1-452c-9cdd-fed9913a3804))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6a59543e-32e6-44c7-b2e0-7613ed22fbc4))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4a4cf1ee-3714-42bb-b458-6e0a87da7aa7))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "NX2A") (pintype "passive") (tstamp 347f92b7-0700-49e2-a83f-90c0668fa18b))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(Q3-B)") (pintype "passive") (tstamp d1cac2b9-2a3a-4d9d-a891-99b9c4cb9a9b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 7ec0f5d7-f2a0-462d-b13b-bd53ec78ef96)
    (at 62.4625 78.5075)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/798ce0df-a846-4b4b-a1f0-644b2ade44d8")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c2bbc9a-7cb5-438d-a47a-92b3251e4135)
    )
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d5188517-bf9b-4948-b41e-1ea90e4c8fc4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 48d91430-b2d0-4997-a7c8-7d2498ee7af2)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 65a283f4-d6a8-443a-9568-5cc81b73a09e))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a665dc3f-1fcd-4c37-9cd6-8fcda26087a6))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5f44714b-8de0-486b-887c-61045960ea30))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 640a2def-793d-4fe4-8c8d-b311970abd45))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7e92fb36-a92e-4904-aeb9-2dc44fc02624))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8bbccd70-9844-4c76-9ecb-f14c3ffac815))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e2c9c34c-b95d-453e-a31c-c44be78f23cd))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp edc35f9e-f3a3-4f76-9039-d472515c714b))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8b8934db-257f-4e9e-8454-5c3a4a5f10aa))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d8515181-43cf-4b50-b65d-f27061993745))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "+5V") (pintype "passive") (tstamp 8ff252a0-d32c-4a1a-a42f-7c89cb598094))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "GND") (pintype "passive") (tstamp 4a3cfa50-0ba1-4848-b3ce-477d6566d684))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 814fbc2b-f013-4c6a-870e-d158576691bc)
    (at 84.25 48.3 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0fc1bacf-e0da-4573-8c73-937df022e25c")
    (attr through_hole)
    (fp_text reference "R6" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ad1ced04-33c3-4912-b310-842d8e28ccc7)
    )
    (fp_text value "100k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6789b7a8-a5b0-4f4e-b5e4-008f8b824e9a)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3f6f1b8b-1bb6-4e10-a648-dc8e08571870)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp faddb9da-147e-4bf0-9ec6-399a83c13544))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2094fd9c-c1f0-4e39-9064-7091b6dc9a9b))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 958a91ea-a274-4548-965c-560a50000b1d))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc550c2f-4a14-48f9-afad-e48517f941fe))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 547171a3-781a-41ba-9ad6-1e1404ff734c))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 81ca0154-8570-4165-b919-7252bfad9f08))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0cc0bb43-2e41-462c-b42d-9fda9d0bcf6d))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a9938c81-6fb2-4154-aa3f-0406ff78ed2b))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2eb5c54e-2ccc-4d68-84d3-0f4a73352ca4))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cab15eef-97ac-4711-a0b0-739042b4cd13))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 930860fa-254e-4431-bea8-b7c03e454dc6))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d99ae741-c319-4e4d-bee3-c1cc81e9acf8))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0a41e57e-e463-4b85-80e1-854622fc5851))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b6276826-3b59-4d09-ac78-8653591452fc))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5e329b61-ec1e-4c50-a095-3e60ae085668))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed813cac-d4d1-4169-b0b2-471d23d80907))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(Q4-B)") (pintype "passive") (tstamp b4488dd1-0489-44eb-b779-89ae88ff1766))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pintype "passive") (tstamp 9f090bee-e215-412d-91d1-ee9f7c6713ef))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-16_W7.62mm_LongPads" (layer "F.Cu")
    (tstamp 8e38eba6-65c1-4507-b782-f4f5c385f66a)
    (at 106.34 113.03)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/6d2c34e7-c57e-4031-a9d6-887ecbf574b8")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 793c91a4-815b-4d5e-8495-b28fe51f7de4)
    )
    (fp_text value "74141" (at 3.81 20.11) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7bc8eb9a-0e7e-4eba-a078-e76bf9e9f69e)
    )
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cd0810a4-f9c4-4c64-a3a4-27b80b56f416)
    )
    (fp_line (start 1.56 -1.33) (end 1.56 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 55409333-947e-47d8-8bcc-8d13780090e7))
    (fp_line (start 1.56 19.11) (end 6.06 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8fdebd7e-b1d6-4287-bec8-e8d28b897e56))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ebaea0da-c6c8-417e-9171-496b45875c58))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6ec658e9-33e4-4d1a-993c-3f6d75ff4b9c))
    (fp_line (start 6.06 19.11) (end 6.06 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2cf7e0a0-9dda-44e0-8ba4-6cc7e07ec082))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 78025bc2-b34d-40ee-9a1e-6960c2cc0e97))
    (fp_line (start -1.45 -1.55) (end -1.45 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4c894be9-5517-4ec9-9ad6-17509dd94c09))
    (fp_line (start -1.45 19.3) (end 9.1 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6ad75234-1210-425e-8366-258f43a2678f))
    (fp_line (start 9.1 -1.55) (end -1.45 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9fa089ac-61e1-45ce-954c-4960b00cb778))
    (fp_line (start 9.1 19.3) (end 9.1 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9e59e710-eaa6-49fe-a577-265d12b8f749))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92148356-305d-4553-bb5b-5475b7801408))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37a6f047-d36c-47de-8ec3-b6448a2b437d))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2ada62db-4a27-468a-9352-5b7eb6d26cb3))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d07b1bec-f6c6-4f48-b850-062f9b532415))
    (fp_line (start 6.985 19.05) (end 0.635 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 26e5b291-7ba0-498f-86cf-a9749ed5ed2b))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "/Horloge Nixie/NX2K8") (pinfunction "~{Q8}") (pintype "open_collector") (tstamp 7b30ba15-2077-4e6b-afb8-c100cc2a0a83))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 92 "/Horloge Nixie/NX2K9") (pinfunction "~{Q9}") (pintype "open_collector") (tstamp 0b2baec1-55b5-452a-ab56-b4e637bd6bf4))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "/Horloge Nixie/NX2BCD1") (pinfunction "A") (pintype "input") (tstamp abb06162-bbf9-4859-a124-fd24f1a1b8ed))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "/Horloge Nixie/NX2BCD4") (pinfunction "D") (pintype "input") (tstamp 983057a1-735f-4b7e-ab98-1c0eb3f86a65))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in") (tstamp ed5733e1-90a9-4cf6-852d-022b622adfbd))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "/Horloge Nixie/NX2BCD2") (pinfunction "B") (pintype "input") (tstamp 24ea57a4-3474-4289-abfa-ae5811a4638f))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "/Horloge Nixie/NX2BCD3") (pinfunction "C") (pintype "input") (tstamp 94d4d86f-cc7a-413d-adea-980a3433ac39))
    (pad "8" thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 93 "/Horloge Nixie/NX2K2") (pinfunction "~{Q2}") (pintype "open_collector") (tstamp e795bd45-358a-4c6d-a7c9-ceb1907ce406))
    (pad "9" thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "/Horloge Nixie/NX2K3") (pinfunction "~{Q3}") (pintype "open_collector") (tstamp 369d4d2a-477b-4aad-88a6-57ca1430518a))
    (pad "10" thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 95 "/Horloge Nixie/NX2K7") (pinfunction "~{Q7}") (pintype "open_collector") (tstamp 5cbf6f25-8177-49d2-8bf6-67a64e72c33c))
    (pad "11" thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 96 "/Horloge Nixie/NX2K6") (pinfunction "~{Q6}") (pintype "open_collector") (tstamp 16d21c93-7292-4cd1-a0bb-c47d73b62eb9))
    (pad "12" thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp d1bf2b13-670c-4148-b21c-6a8bda0b2519))
    (pad "13" thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 97 "/Horloge Nixie/NX2K4") (pinfunction "~{Q4}") (pintype "open_collector") (tstamp 44e5bad3-4e7e-4695-bbbf-da3aa90a3ce2))
    (pad "14" thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 98 "/Horloge Nixie/NX2K5") (pinfunction "~{Q5}") (pintype "open_collector") (tstamp 8e93ec4f-4ab5-471a-8108-87c367d042fd))
    (pad "15" thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 99 "/Horloge Nixie/NX2K1") (pinfunction "~{Q1}") (pintype "open_collector") (tstamp f4addfbf-33a8-4539-b2e8-7d71625e85af))
    (pad "16" thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 100 "/Horloge Nixie/NX2K0") (pinfunction "~{Q0}") (pintype "open_collector") (tstamp ad2c3ec3-ab13-4d5b-9353-a8fb21ef48fe))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-16_W7.62mm_LongPads" (layer "F.Cu")
    (tstamp 911e050f-3ac8-4679-9cda-fc3c7c792de5)
    (at 168.91 95.25)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/8b25f833-d2e9-4600-b52c-ec42b879c6f9")
    (attr through_hole)
    (fp_text reference "U5" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c8a1eb5-9614-4264-9ddb-9eb57796cd72)
    )
    (fp_text value "74141" (at 3.81 20.11) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f4eedc86-c74c-4d4e-955e-8d02db6894f5)
    )
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3361afef-e4c8-4f22-801f-24b151737ca3)
    )
    (fp_line (start 1.56 -1.33) (end 1.56 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ef60ae9-edf3-4742-8142-b318cba97b43))
    (fp_line (start 1.56 19.11) (end 6.06 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e7fc6f52-e04e-4b59-91c2-bcadd2f98362))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4abe270c-0172-4de0-bad7-26a3988145d0))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9bf8e14-d9e9-4fad-9431-e2a5abd75d9e))
    (fp_line (start 6.06 19.11) (end 6.06 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8627c322-958a-45e5-b257-017a85d3983c))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 65344179-9677-45eb-a1de-de11fc526d34))
    (fp_line (start -1.45 -1.55) (end -1.45 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3b02fa57-f367-475f-9045-4d142dfb8fc7))
    (fp_line (start -1.45 19.3) (end 9.1 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a95bcffc-864d-4a9a-97ec-46a63361254d))
    (fp_line (start 9.1 -1.55) (end -1.45 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 97be4e68-df45-4fdf-b1da-65838e837b79))
    (fp_line (start 9.1 19.3) (end 9.1 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ffb4c6c9-7ded-4545-9365-77b89e07afbf))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dd13a308-0374-4e91-842c-f636f10c3a86))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cb158761-5c3c-4e13-904b-94e43b0d730f))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5c00ec40-b458-4105-b5db-fdc8ff951762))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b67a0d6b-9328-4e75-b08c-7e44d2a6268c))
    (fp_line (start 6.985 19.05) (end 0.635 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ffddcc4-f922-49f2-8871-6ae2326caa1b))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 111 "/Horloge Nixie/NX4K8") (pinfunction "~{Q8}") (pintype "open_collector") (tstamp 140efde5-889d-4630-a786-7bc0c236fbf2))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 112 "/Horloge Nixie/NX4K9") (pinfunction "~{Q9}") (pintype "open_collector") (tstamp faea3bb9-688a-44fc-b5d2-2a1a48a06c13))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 77 "/Horloge Nixie/NX4BCD1") (pinfunction "A") (pintype "input") (tstamp 5a60231a-0c1e-4ed4-8597-b3065dc231b7))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "/Horloge Nixie/NX4BCD4") (pinfunction "D") (pintype "input") (tstamp 1ec8653e-fefa-4f80-99e8-71b50abd67fd))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in") (tstamp 8f5181e2-adaf-4fa1-97b7-879ef8da820e))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "/Horloge Nixie/NX4BCD2") (pinfunction "B") (pintype "input") (tstamp 9ef740ff-f2cc-45dc-a8da-06a45b3f858e))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "/Horloge Nixie/NX4BCD3") (pinfunction "C") (pintype "input") (tstamp ca54df3b-ce57-4d2c-89f3-501f7a6dc86a))
    (pad "8" thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "/Horloge Nixie/NX4K2") (pinfunction "~{Q2}") (pintype "open_collector") (tstamp 65c68da3-cdfb-4c1d-adc1-a43753e570a1))
    (pad "9" thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 114 "/Horloge Nixie/NX4K3") (pinfunction "~{Q3}") (pintype "open_collector") (tstamp f98ea8a1-e6d2-448f-a7c7-30be9a2afb3e))
    (pad "10" thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 115 "/Horloge Nixie/NX4K7") (pinfunction "~{Q7}") (pintype "open_collector") (tstamp a1ec0374-feaf-4df0-8520-f7752fd33d0e))
    (pad "11" thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 116 "/Horloge Nixie/NX4K6") (pinfunction "~{Q6}") (pintype "open_collector") (tstamp 9dd47057-0920-4e00-b9ef-f67beedb022e))
    (pad "12" thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 21076f71-0c2e-4caa-8ca2-3925333786b1))
    (pad "13" thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 117 "/Horloge Nixie/NX4K4") (pinfunction "~{Q4}") (pintype "open_collector") (tstamp 8af73fe9-945b-4ec8-9572-53055e5d4695))
    (pad "14" thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 118 "/Horloge Nixie/NX4K5") (pinfunction "~{Q5}") (pintype "open_collector") (tstamp 04608d27-60c8-4113-9f20-80c2cff9ae9e))
    (pad "15" thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 119 "/Horloge Nixie/NX4K1") (pinfunction "~{Q1}") (pintype "open_collector") (tstamp 75f18c7e-6565-4c81-86cc-79424d87ae6a))
    (pad "16" thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 120 "/Horloge Nixie/NX4K0") (pinfunction "~{Q0}") (pintype "open_collector") (tstamp bbabb1b8-d566-4734-ad30-383f84154af3))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp 926ab641-c28a-4ca8-91d3-e5f0aa0c7fac)
    (at 64.228 44.054 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/8b7b34c9-cb78-4fe8-bacd-da5c7b644dcd")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.37 -90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 217ce879-5ac8-4729-a990-528cde172a28)
    )
    (fp_text value "100k" (at 5.08 2.37 -90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ccfb906-5738-48e1-8d18-208edadccfad)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 -90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 810b62e7-b61c-4eff-80ac-c93a61c2ea0a)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8e55f0f-6238-44a0-8342-f2b45d6fee0b))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9942c28-ca1f-4628-83b6-784f12e30348))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9979e321-1469-4548-a825-ba552bbdb960))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cd15db90-f5b6-46f8-ab96-aada36b9fb22))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff4c7136-c0d2-44d1-b2a8-35f773dc5d02))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d1d6f12b-9bc8-445d-b638-4b2f6080f273))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e656d6b4-6b09-4890-b0f0-cbe4302dfcd2))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 41cfb06f-bbd8-406d-99d0-a9693d4e1b55))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5191e213-0059-404c-ab1b-be0f3bd36016))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f4d96815-8bcf-4a64-b2cb-f9421595e422))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e6fdfe25-4d40-498e-a779-4ee6c1a34200))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2f5d27a-5d8d-43c0-84f6-581f320d1b99))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 02644c66-c8cd-4700-9138-9ef60f049301))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bfa1cecf-dc9d-4100-9f51-04f9ed73d594))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9593760e-fa7f-40e4-af13-35f0ba0a7166))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5591a33d-23b0-4e81-9c7e-49e8654c2d15))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(Q2-B)") (pintype "passive") (tstamp f5774729-dfd4-4684-921e-67d79d6d818c))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pintype "passive") (tstamp 69e323bd-5cce-467d-93c9-5d2fa1dbf805))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tstamp 9352cbc6-b26c-47bf-bd3f-5696b1019e29)
    (at 138.8 67.8 90)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/e3a7e6bc-4f0c-42b6-8482-cc63a2145bc9")
    (attr smd)
    (fp_text reference "D4" (at 0 -3.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 79db28b0-110f-45b8-b3cc-04b2f0940074)
    )
    (fp_text value "WS2812B" (at 0 4 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 64e7d843-91e1-4186-a76c-72720afa493a)
    )
    (fp_text user "1" (at -4.15 -1.6 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b8108d9e-6246-482d-98a5-69f97b1fbbff)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.15)))
      (tstamp 3ee9af2b-b00d-4e8c-8c00-f66ebeb4ba27)
    )
    (fp_line (start -3.65 -2.75) (end 3.65 -2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 087e54b1-794d-44f7-82bb-0266521642c3))
    (fp_line (start -3.65 2.75) (end 3.65 2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ebab61be-febe-4a52-b273-69dbbf95c560))
    (fp_line (start 3.65 2.75) (end 3.65 1.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7adf7db3-af28-4dc2-8a2f-9f143bd06011))
    (fp_line (start -3.45 -2.75) (end -3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 963beeef-3803-4ed0-9fb5-4713b80d2076))
    (fp_line (start -3.45 2.75) (end 3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9de8ce27-1478-4027-bd7a-ee0026624a2a))
    (fp_line (start 3.45 -2.75) (end -3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2d787939-27e5-44e4-9100-aee1c8dbb129))
    (fp_line (start 3.45 2.75) (end 3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b7f37348-24db-4c90-a8e9-8ff8e692c96b))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e0112578-36af-40dc-a0cc-a0e533754525))
    (fp_line (start -2.5 2.5) (end 2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0391e205-6635-4728-ae3e-b6f54c6df63b))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3938b66c-7c9e-41ef-85a9-d3351e52e318))
    (fp_line (start 2.5 1.5) (end 1.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42ca287b-f299-4fec-a342-7178fc88a8aa))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d2767f5-bce0-41cd-afb9-81d42e26d3d0))
    (fp_circle (center 0 0) (end 0 -2)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp f6205855-eccd-4ba9-bbf2-f36854f30913))
    (pad "1" smd rect (at -2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in") (tstamp 70ede652-1460-47c8-a36b-832970dfcc47))
    (pad "2" smd rect (at -2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "unconnected-(D4-DOUT-Pad2)") (pinfunction "DOUT") (pintype "output+no_connect") (tstamp 50c38bc5-46c3-4587-b606-013d377748d7))
    (pad "3" smd rect (at 2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp ac3a8542-5d65-458c-9d22-b6739016469c))
    (pad "4" smd rect (at 2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(D3-DOUT)") (pinfunction "DIN") (pintype "input") (tstamp 838eca58-c999-4685-83e3-b8acfd374efc))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 9eb0a42d-f859-4d47-9f0c-1b6daf82fbfa)
    (at 138.43 78.74)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/74a814b0-47b8-47f3-a174-6d18665a2960")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.68) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3f8f8bd-4b7d-429b-ade2-74fd93b19a7d)
    )
    (fp_text value "0.1uF" (at 0 1.68) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp caaaee62-c533-46c3-bfe4-99a00f14373a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 86611ea4-7d57-43bb-bd1e-b98b0aa4e7f0)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 563fac29-275e-47d0-9da7-ca7e1a9f160b))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f1d71f86-05e3-4f65-8ef8-67c03fb79344))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 33d5c3f7-df3b-4462-8a03-ba997ce3ad9b))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b83feb93-1126-4c66-a186-64b5e966792a))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c14d4b21-2f0f-450a-b8ec-ce6b716717d6))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b415fd3a-5b6e-4f5f-8065-98e276212ba0))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bf7eee8f-8e0b-4511-bcd4-c92862714b9a))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fba71c89-5b5a-4e88-8147-976ff8b59615))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6cc623bc-bf18-48b7-bb8c-5a1fe98a2b7a))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae48c103-7d5b-4458-9a31-feb4e7c8a934))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "+5V") (pintype "passive") (tstamp e8bea1bd-f580-45f0-b973-75810a920e77))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "GND") (pintype "passive") (tstamp f8a29c68-8694-4e84-99e7-455e5c9bd697))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp b94f43cd-8503-47e4-b7a2-430951935a61)
    (at 129.85 30.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/65ed49d1-b91d-4bcb-8c37-7c05504ef579")
    (attr through_hole)
    (fp_text reference "R13" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7a55f11e-e10e-4653-9039-d4d7962789c9)
    )
    (fp_text value "33k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 168d6eb4-ffeb-4b39-a3f9-00eb80bb7ad3)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a6670e23-3e4c-4666-90b8-284085e54383)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp af8bf81f-47ce-442e-8694-9ed178193ff1))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b8fd33fd-c587-4476-a723-9c67ff49f78c))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5ce649a7-4c37-40ac-b03b-a1662b6ecb04))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c964af3-ce53-41fb-b1bc-2834b472636b))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5b687976-a718-4899-a62b-a56e13345588))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0e183689-32b7-45fa-a941-06111ea7e2b3))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c2426d08-45e6-4734-aeac-a546468029d2))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6113b173-862a-4fd3-9481-4a3e2208fb70))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 639e4556-e853-4c40-9923-7b4ecf10dd74))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 52130513-738b-4524-85a6-c54923859dfa))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ad3f81e4-21ea-4333-ac47-7cbd524e7862))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 16f89131-e3e9-452e-90d2-397e9cbf4d9e))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dceca2f6-3640-4f1a-b889-685b61d2e442))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4be566a1-4616-4b41-89fa-a5c1ad0034a3))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f9c86f3a-dade-43f7-b342-d902be40839a))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c7a2e4fc-db54-4cb9-884f-fcc7d647c950))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "NX4A") (pintype "passive") (tstamp 74e139cd-276e-4a8f-a827-e3a423b07081))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(Q7-B)") (pintype "passive") (tstamp 77429955-8936-4edb-97d5-635b409f7253))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" locked (layer "F.Cu")
    (tstamp bec607ae-169e-4bf5-a782-f0065fb0abf5)
    (at 147.32 96.52)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch")
    (property "ki_keywords" "rotary switch encoder switch push button")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/ce68a31a-568b-4e57-b0bb-55bda0e65ee5")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec5c8797-7245-4a23-b6c3-fc9a732976d2)
    )
    (fp_text value "Rotary Encoder" (at 2.54 5.08 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9a50774d-cded-4a43-a95e-5819c641479d)
    )
    (fp_text user "C" (at -3.81 3.175 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
      (tstamp 682baed3-31a2-4089-8efa-49bdb6cec4e2)
    )
    (fp_text user "SW1" (at -5.08 8.255 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
      (tstamp 6d38d17d-a593-418a-940a-9c4886fbb4f2)
    )
    (fp_text user "B" (at -3.81 5.715 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
      (tstamp 8428616e-1fb9-42d1-9eea-a7faa589ad9f)
    )
    (fp_text user "A" (at -3.81 0.635 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
      (tstamp cb67356d-292c-4510-8fa4-57449f2d5bcb)
    )
    (fp_text user "SW2" (at -5.08 10.795 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.1)) (justify left bottom))
      (tstamp f4fec678-6447-476f-9b6c-c3882c1b2e90)
    )
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2e00bb91-cc6e-4694-a41e-800677a199e5)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4ef88dff-9a45-4410-9d3e-85f4d982ce77))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c30141a7-a858-4b61-8bcb-edd201e36f04))
    (fp_line (start -1.33 1.27) (end -1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e048fb97-423a-4eb4-80de-5762a69e88c5))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 98eba678-63f4-4abc-9f39-e2eadb6ee572))
    (fp_line (start -1.33 11.49) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2735f14e-472f-43bc-9b6d-68369e700270))
    (fp_line (start 1.33 1.27) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b17cb6c2-6450-4117-aef8-3fe1a5f1997f))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e59a34a-5732-4edf-ba74-69cf55c16195))
    (fp_line (start -1.8 11.95) (end 1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8d6495b9-bee7-4bc9-9c2f-a4fa1f73cc50))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 461d0a08-3504-4489-a1e0-42eb84a74d5a))
    (fp_line (start 1.8 11.95) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa0008b7-265c-4213-a6a0-3d67e76e645f))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7dd3c5ab-a200-4100-b0bf-9ec492b758b5))
    (fp_line (start -1.27 11.43) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e4b30f6-aa71-4566-8283-ad557f6708ae))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8ecb680b-25c3-4882-a55a-f074dd84d4a2))
    (fp_line (start 1.27 -1.27) (end 1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0bd7f3bf-9a07-4a18-ab65-37f70705ae64))
    (fp_line (start 1.27 11.43) (end -1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d3ec1912-54a9-4b0a-b506-c993ed300ae2))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 68 "/Horloge Nixie/IN_ENC_A") (pinfunction "A") (pintype "passive") (tstamp a35b4b89-0a29-4768-91a2-653c5ca02412))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "C") (pintype "passive") (tstamp 3799580e-c07e-4786-9ddd-2928f3486387))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 69 "/Horloge Nixie/IN_ENC_B") (pinfunction "B") (pintype "passive") (tstamp 73a491d3-9844-4960-9ab8-4ca45826e0e7))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "/Horloge Nixie/IN_ENC_SW") (pinfunction "S1") (pintype "passive") (tstamp cb2955e0-ab7a-4a4b-bb1e-c806223a1510))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "S2") (pintype "passive") (tstamp c8fca5ab-0a52-4495-b0fa-123ed7bbadaf))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp becdf325-898e-44a2-b4c5-be0e6d69b3cf)
    (at 68.8 44.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/03787509-3523-4bfb-93d3-cfd32cc89e4b")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 20a36615-25af-4459-83ba-caceafaff349)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp abaeed44-a279-4b15-a6fc-aade46a348c9)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e5d4b99f-fd7d-472a-948b-632e168c206b)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c0910c76-2849-4960-a9e3-6cf895f8e306))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8df30c57-823e-4415-a165-1c9497b06995))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8cc558b-7866-467b-8949-849f4d895297))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b60e2aa4-c8bf-4cb9-a36f-f6fcb36e328d))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3946a17b-4e52-4180-97a1-9830cd3c2950))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2c3180f2-5f35-4f08-803f-9dd385be8963))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 47364369-12a4-474c-92df-34397ba039ae))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f644af84-eca7-44ab-9265-faaaa34048be))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2fb18495-b0b5-416b-99a5-c1ae9b5daead))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 95826be1-f4b0-432d-a425-6f9cc49dea22))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(Q2-C)") (pinfunction "C") (pintype "passive") (tstamp 0f174eac-8367-4fcb-9aab-68e79ad2a1e8))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(Q2-B)") (pinfunction "B") (pintype "input") (tstamp cbef73a7-0ab7-4c0f-8c7a-2a93337195a4))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pinfunction "E") (pintype "passive") (tstamp 2c717ec9-375e-4900-b285-4a81338c4309))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp c755475e-894b-4882-8ce6-374469c9ce22)
    (at 132.8 30.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/f8a24ec2-4c2e-4169-ae3e-69c8f18a80cc")
    (attr through_hole)
    (fp_text reference "R14" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 133959aa-27e6-4706-b399-a738bbe96562)
    )
    (fp_text value "100k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 79f62399-fb36-4a4c-92d8-da39081ec5b0)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 961619d8-e1f9-4026-afd4-6061d384cde1)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 461af53b-7a26-487a-a975-44b269216362))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0885609-078f-4c5b-9819-47da7d5c82e6))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 72272831-132a-4da7-95c5-5883afaf43e2))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f96708e2-8e61-4c61-886a-b128c52504d3))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e4c44a23-82dd-4010-ba4b-fda7891f4e20))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f50c504a-fcaf-413c-a709-d81c65730a29))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d4c660c1-bb88-427a-a023-77566ce4026c))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 05791ccc-0cdc-4c65-a96e-81cda4d8f03f))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 965a0b72-8ca7-4318-824d-8ba055d246bb))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30831ff7-251f-4b37-8dba-d61b9c8d9468))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed27fae3-e909-4723-974b-575f85772126))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56371bed-da81-4c07-81e9-c7d991a28473))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5290fba9-9101-460c-9b7d-0c8db53c8ac6))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15c34cd4-663c-4e5b-88d2-d143859f90b5))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f96c2d1a-6a7e-45af-99f0-2afb61d25eca))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6e48dd44-18d2-40d6-bf83-40103a38005b))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(Q8-B)") (pintype "passive") (tstamp f759fdf1-120e-456d-8271-103c247452c2))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pintype "passive") (tstamp d6e5d3a9-d04b-49d3-b345-fbaa9e229e03))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp cac71a15-84f8-4d9e-8de8-d62242d2768b)
    (at 87.3 48.3 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/d5f17e5b-2b4b-4896-9943-499373ca0d64")
    (attr through_hole)
    (fp_text reference "R7" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp abebea87-3918-44f3-a8aa-2aad802edb26)
    )
    (fp_text value "470k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 380e6d32-3158-4848-ac48-da6c0e831bca)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8649283f-6204-4c59-8dc2-4468e9e037a1)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1f66fa38-736f-4893-b725-e2ef923eb171))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2269377a-bf78-448e-9867-8eafb60eef42))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9e8ac52-1395-47bf-b242-10cd1c14c68f))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b6b373d-9219-4023-81a2-62413ee1c8bb))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8c4cfc1-6953-4419-8984-ee0913be4905))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4d9ae99d-128e-4c5d-87d7-eb0101b7f6bf))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d46b5d31-a89e-48ca-a7ae-6f5de576d03b))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e4b457dc-ff92-49a1-b9af-91d935c2ec97))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 216c1fde-e487-4b22-93ef-ffcfa3c1d530))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 765540bd-cfff-4861-9a70-4955c25d1c14))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92e8d4f4-7d95-4088-bf1a-52f2471d3c52))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2da8f596-48ac-4b0f-9fb2-7562ff8411b0))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0be84bf8-c9c0-4215-8b18-cf8ce5801493))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 55d0066e-02a0-4655-9e4c-a8926d1cc762))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 88102875-df2e-4e36-b70e-0bb7275f4be8))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 119cf6b2-b303-477d-89ce-1fd10627f8f9))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(Q3-C)") (pintype "passive") (tstamp d6df796f-fc23-4e0a-9b96-a6c98eaaf972))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(Q4-B)") (pintype "passive") (tstamp e978912f-d6b4-4cc2-b399-eaa13ea500e5))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-16_W7.62mm_LongPads" (layer "F.Cu")
    (tstamp d04826e6-8d91-468c-ba7e-52ae431663af)
    (at 117.94 113.03)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/2d1c6471-ceba-4767-ae21-b198a857b702")
    (attr through_hole)
    (fp_text reference "U4" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0f5cf5f6-405a-45af-919a-4df1f6b1c138)
    )
    (fp_text value "74141" (at 3.81 20.11) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da95f9a3-b27c-4d84-89fa-9e0d8b9ebfb1)
    )
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7ebfb61e-c050-45c5-9988-cf6725205a84)
    )
    (fp_line (start 1.56 -1.33) (end 1.56 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9bfc07e4-725f-429e-abb7-1e39b338aa14))
    (fp_line (start 1.56 19.11) (end 6.06 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8ab0e6c8-974b-4b26-870e-7db12511a2b9))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5362c1a2-afb6-4844-9535-c7a19b76f955))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 08c688b6-237b-46ca-a04e-9cb11fd34b2d))
    (fp_line (start 6.06 19.11) (end 6.06 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8c53f84-54de-4e40-b71e-03c10f3a9662))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8853cd7e-1e3f-44b1-ac40-1479ae4883fe))
    (fp_line (start -1.45 -1.55) (end -1.45 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3c2e0062-a5fc-4a66-810d-68efa22e2574))
    (fp_line (start -1.45 19.3) (end 9.1 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fc5c0f34-f0b0-4de3-9b77-00038cb59448))
    (fp_line (start 9.1 -1.55) (end -1.45 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 22130c40-29c6-4d0e-9d8d-dbfc5d85623a))
    (fp_line (start 9.1 19.3) (end 9.1 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4e3179de-18dc-4f0e-987c-b5bb987910bd))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e41cddbf-bbd0-414c-acdb-7cbc182f5fd8))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7a8d0cab-81b0-4a58-9263-0a259c5839fc))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa4d18fb-ab7c-46d3-ad70-834b69ee0fd1))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ec5d66a3-fed9-4790-88c1-b1b3a69aaa37))
    (fp_line (start 6.985 19.05) (end 0.635 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1603ffb9-9d39-4fa4-9939-0515c965d776))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 101 "/Horloge Nixie/NX3K8") (pinfunction "~{Q8}") (pintype "open_collector") (tstamp 9479ed37-e011-4102-a428-d2594942a0fb))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 102 "/Horloge Nixie/NX3K9") (pinfunction "~{Q9}") (pintype "open_collector") (tstamp ecd0b32b-c0ed-4416-8320-b77d76601686))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "/Horloge Nixie/NX3BCD1") (pinfunction "A") (pintype "input") (tstamp d464dd55-b5a4-4ac6-b2f9-f158d8358ea9))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 75 "/Horloge Nixie/NX3BCD4") (pinfunction "D") (pintype "input") (tstamp 289cef0d-ec78-4576-bb4b-ce3b3b708df0))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in") (tstamp 6b1ffcde-72ed-4042-b2eb-d1313cc5e031))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "/Horloge Nixie/NX3BCD2") (pinfunction "B") (pintype "input") (tstamp 6eeda14e-0c32-490b-bc7d-5e584c9dbf0a))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 74 "/Horloge Nixie/NX3BCD3") (pinfunction "C") (pintype "input") (tstamp abc0267f-0aa9-407f-aff1-3a86cd5d916e))
    (pad "8" thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 103 "/Horloge Nixie/NX3K2") (pinfunction "~{Q2}") (pintype "open_collector") (tstamp 778354e4-fdaa-4ab0-b4c7-c92903729909))
    (pad "9" thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 104 "/Horloge Nixie/NX3K3") (pinfunction "~{Q3}") (pintype "open_collector") (tstamp 4f3eb438-7fa7-43a6-9299-5fabc63f687e))
    (pad "10" thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 105 "/Horloge Nixie/NX3K7") (pinfunction "~{Q7}") (pintype "open_collector") (tstamp 58af6ad4-f31a-4dd2-a4c4-f4ce4ce939be))
    (pad "11" thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 106 "/Horloge Nixie/NX3K6") (pinfunction "~{Q6}") (pintype "open_collector") (tstamp 921fe194-bc6f-4fa9-8ea6-9173dfc9310b))
    (pad "12" thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp ecdf2df1-1cf1-4658-8aa3-219bb4d7549a))
    (pad "13" thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 107 "/Horloge Nixie/NX3K4") (pinfunction "~{Q4}") (pintype "open_collector") (tstamp 96996ffd-b68b-465b-a882-27e7af484d65))
    (pad "14" thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 108 "/Horloge Nixie/NX3K5") (pinfunction "~{Q5}") (pintype "open_collector") (tstamp 090c4eb8-acbb-4076-a931-f793fc24a46c))
    (pad "15" thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 109 "/Horloge Nixie/NX3K1") (pinfunction "~{Q1}") (pintype "open_collector") (tstamp 57bb152f-e9de-4939-b863-68a22b735289))
    (pad "16" thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 110 "/Horloge Nixie/NX3K0") (pinfunction "~{Q0}") (pintype "open_collector") (tstamp dd7737c5-5885-408d-9f63-e07093b44b4f))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp d1ff2b0c-d43e-412c-a359-d5bcdf929f01)
    (at 78.75 115.57 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/72e95360-3d9d-4402-abf9-895236b95029")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f8d63f3b-cbc9-41ac-a349-1b536c12bfb3)
    )
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b59d4d70-94bc-46fb-aec6-532a8f4f0b12)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9b8d0548-2552-49ed-a63a-431c709b04c2)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a3ded92-ef89-4096-9bb1-b76d3a7dc2fc))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58c59389-2379-4278-b25b-579711179441))
    (fp_line (start -1.33 1.27) (end -1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7675d05-4d1c-4b84-8e6e-2d240b20caef))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5a71011-609e-429c-88ec-cb76dff65c29))
    (fp_line (start -1.33 8.95) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e1aea274-0b73-42ce-9528-39cb730a309e))
    (fp_line (start 1.33 1.27) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6f913d5b-055b-40b7-8060-77a694c1baae))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 26934796-9ed5-42d6-9f2d-28208ad554ed))
    (fp_line (start -1.8 9.4) (end 1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7f8323d9-ead8-459f-8e51-647efd9fb86c))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8200d21f-1e91-4d6f-bebc-fda7e16dd3cb))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32aec78e-f72c-49d1-bb3a-043c37a60fae))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1a3e70e2-0e21-4433-aaef-3170f383f2c0))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 59651f78-ffc5-44b9-8027-c93d3ed53641))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 12a78812-5390-489a-bd14-b32022b45e1c))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b87af3c-66de-443b-919f-e32bf638ffb0))
    (fp_line (start 1.27 8.89) (end -1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aed3f282-8298-456c-8a9b-e3e194a1fc07))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/Horloge Nixie/I2C_SCL") (pinfunction "Pin_1") (pintype "passive") (tstamp 7e10e1fe-04e1-40f6-a8ed-42bf50b8e1a8))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/Horloge Nixie/I2C_SDA") (pinfunction "Pin_2") (pintype "passive") (tstamp a0a9e55d-d486-4498-a520-8c79726fb2d0))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_3") (pintype "passive") (tstamp 5f237042-5d03-45dc-a220-1f81572079d3))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp 56c44e5c-0636-4aed-b971-62440c173614))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp d3df2ed5-cf4b-436e-8bd5-11af4bfbbde6)
    (at 110.03 46.16)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/487425bd-d3d6-47c4-a1c2-69de23b17acc")
    (attr through_hole)
    (fp_text reference "Q6" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 03dd43c8-edeb-47b7-9df5-0b8c0ed2bf9e)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 334f7507-094f-417c-9e2c-e5cfd65c541b)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3aedb8ea-7028-421b-8c51-cf7bda86d042)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 25020d0b-fc39-4ec1-b186-51f6f3fbfd0f))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7b49255-b7bd-44a4-84a3-90fa7af28b2b))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 663c1e8c-1658-49cd-bc80-546f4d3e24a5))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0e21e371-4423-4355-977f-f0d904b1013a))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 57e43ebc-cfc7-48f1-a165-2ab56770a8ef))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 43f60382-b2e9-403e-b463-4c876b1ced05))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bc05d8c5-5b0b-40c9-bc73-a53470ff1bed))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0dd1ede6-eb15-470c-8f7b-55376acbbdad))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b86db821-04c4-46bc-bf96-d052a3936de3))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 28b0d636-ef4e-4351-91ae-517c6c889793))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(Q6-C)") (pinfunction "C") (pintype "passive") (tstamp d44a1a6a-afc6-4422-b222-0d93e8131348))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(Q6-B)") (pinfunction "B") (pintype "input") (tstamp 7780c589-423e-4711-b17f-8a586a346cc6))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pinfunction "E") (pintype "passive") (tstamp de8d7ade-b6d3-4f1a-b588-f06d290f20f3))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp d94cafbe-a1fb-40b7-9b4a-17eda3a1d979)
    (at 112.4 53.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/1359a25a-6345-46da-83c7-a255fa7a8a82")
    (attr through_hole)
    (fp_text reference "R10" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 654298ca-ea06-4346-989d-4d26d580501c)
    )
    (fp_text value "100k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 842453f7-482f-451d-a857-a44b5f9dc2ba)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a8ca0544-919e-46ac-b0ff-37cc9b9dd3c2)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b985cd3f-2784-4f0a-bc42-9b83fd31b923))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 432a3a6b-1cd9-4029-9834-5a03127371f5))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 598205d3-243d-4898-a93b-f738a49a4eaa))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 973e9ed3-7b3d-4a10-885b-34bc7f99f131))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 854b359f-0833-4f03-9b2a-c9c0520d7016))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8667aec-760b-4dd9-a5f3-80a752428e92))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ee37048d-123e-4db0-9f64-101e791f29f9))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 778dc273-5b03-4969-856f-9bc7bbaf905a))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 876f7f8f-db1c-4912-83f3-8ec5cfd3944f))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f58a3d8b-02ee-40dc-9322-2181cc2886ec))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 268d8409-bb98-448b-9450-1a9119ea251e))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0547be8e-06c4-46fd-85d8-64b6ad8cc8b9))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86f58dc9-3572-4faf-9a48-c3fbb71c628d))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ed4de373-b818-4e64-856b-bea0e6e4f8ae))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ca308004-2f6f-45f6-94b4-883cc2fb78db))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 552ce0dc-31a8-44ed-98b4-08ca2abeffcf))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(Q6-B)") (pintype "passive") (tstamp 546d0b8f-7899-4de7-afaa-ac2dce1f8e86))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pintype "passive") (tstamp 3c80c195-a6c8-4aa9-96a7-518be8285505))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "PCM_Espressif:ESP32-S3-DevKitC_Laurent" (layer "F.Cu")
    (tstamp e42da164-b181-4ee3-81e2-5e6b335f90d3)
    (at 97.71044 134.62 -90)
    (descr "ESP32-S3 general-purpose development board, based on ESP32-S3-WROOM-1 or ESP32-S3-WROOM-1U,It has all the ESP32-S3 pins exposed and is easy to connect and use.")
    (tags "ESP32-S3")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "ESP32-S3-DevKitC")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/2dc24073-c3ed-4178-abef-7de8f85194b1")
    (attr through_hole)
    (fp_text reference "U1" (at 12.7 -2.1 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 660a38af-faf2-458d-aa90-e0e3e7a859c8)
    )
    (fp_text value "ESP32-S3-DevKitC" (at 11.42632 29.46128) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f2a5fee-cf8f-4a4f-9e6c-cd0147c96760)
    )
    (fp_text user "GPIO41/MTDI" (at 24.13 15.24 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 0043433f-4f14-41eb-8794-e449161ccac3)
    )
    (fp_text user "GPIO35" (at 24.13 30.48 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 097bba40-37ad-46bb-b5cb-3f7bac0690c4)
    )
    (fp_text user "GPIO39/MTCK" (at 24.13 20.32 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 0fca0238-e78c-442d-924c-6b67862aa472)
    )
    (fp_text user "GND" (at 1.52032 53.33728 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 169975c1-b7bb-414a-93ef-e8c79b19f89c)
    )
    (fp_text user "GND" (at 24.13 50.8 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 19c45262-a9fc-4bb0-b5e0-1127f230c1ee)
    )
    (fp_text user "GPIO42/MTMS" (at 24.13 12.7 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 1b170fef-950e-4bc0-aa74-aa25b66275fc)
    )
    (fp_text user "GPIO48" (at 24.13 38.1 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 1fa974c7-46a1-4bfa-84d9-d1d2aa341141)
    )
    (fp_text user "GPIO21" (at 24.13 43.18 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 20328e93-c9ec-4d48-99e3-90fd90f4f1fe)
    )
    (fp_text user "GPIO14" (at 1.27 48.26 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 237e35b9-202b-4c9c-ae2a-574bcae42738)
    )
    (fp_text user "GPIO4" (at 1.27 7.62 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 26d8c125-7603-4cd0-b963-c262e3d484ac)
    )
    (fp_text user "GPIO19" (at 24.13 48.26 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 2954277d-7e96-4b8c-b7ce-a42d3b636198)
    )
    (fp_text user "GPIO6" (at 1.27 12.7 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 2fe9bccc-8fba-4c90-bfc8-429521d0f978)
    )
    (fp_text user "GPIO7" (at 1.27 15.24 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 3757b654-c3ea-4132-adac-0c2a2b6173a5)
    )
    (fp_text user "GPIO1" (at 24.13 7.62 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 392fe927-f5a3-4d28-8f88-9236ee6003fa)
    )
    (fp_text user "GPIO43/U0TXD" (at 24.13 2.54 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 3ed03ce9-6844-42bd-8444-a7ec14ff1f83)
    )
    (fp_text user "GPIO38" (at 24.13 22.86 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 4da4f179-b9fe-4fb4-8b10-4400943869f1)
    )
    (fp_text user "GPIO2" (at 24.13 10.16 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 4e928add-82e2-4fd5-9d13-2dd5504277f3)
    )
    (fp_text user "GPIO40/MTDO" (at 24.13 17.78 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 53acc318-8b32-4043-a5b1-a0fd8479d3b6)
    )
    (fp_text user "GPIO9" (at 1.27 35.56 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 552d3265-e06a-46b0-844b-a3d301bdaab7)
    )
    (fp_text user "5V" (at 1.52032 50.79728 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 5bca517b-c8c4-4328-aebf-8682e3cf787a)
    )
    (fp_text user "GPIO0" (at 24.13 33.02 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 5fd6392e-ac13-4413-8f72-f0a110c4692e)
    )
    (fp_text user "EN/RESET" (at 8.88632 5.07728 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 60ae0f7b-74a6-4b8a-a334-57629233598e)
    )
    (fp_text user "GPIO36" (at 24.13 27.94 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 64dc3ff4-e67f-4fb5-b79f-e6b17819bc23)
    )
    (fp_text user "GPIO45" (at 24.13 35.56 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 6aac1b05-64ef-4fb8-afca-e7047208e019)
    )
    (fp_text user "GND" (at 24.13 0 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 6b4aee0d-8afd-40a8-b4e5-f7ecf8180aea)
    )
    (fp_text user "GPIO47" (at 24.13 40.64 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 6bcf7411-5678-44c3-a22c-c694e170bef8)
    )
    (fp_text user "GPIO5" (at 1.27 10.16 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 7641c984-0cf0-4cd1-9ce2-598970da582f)
    )
    (fp_text user "GPIO17" (at 1.27 22.86 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 8274c290-edaa-4d2e-874d-eaa23e13196d)
    )
    (fp_text user "GPIO8" (at 1.27 27.94 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 851dfd53-9940-4611-bd7e-85218b2a1397)
    )
    (fp_text user "GND" (at 24.13 53.34 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 939f3f8b-5aae-4797-ac47-84b1c22b1960)
    )
    (fp_text user "GPIO11" (at 1.27 40.64 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 98b07867-813d-4f6d-b632-3a142a17e4f8)
    )
    (fp_text user "GPIO16" (at 1.27 20.32 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 98fcd3d5-d912-42a7-8c98-e905b0feb20a)
    )
    (fp_text user "GPIO46" (at 1.27 33.02 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp b7a8dd81-4e58-46af-802a-b16b27ba22b8)
    )
    (fp_text user "GPIO15" (at 1.27 17.78 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp bd80feb5-9c2e-45f2-9552-88ab70c8d736)
    )
    (fp_text user "GPIO18" (at 1.27 25.4 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp c25c746a-d24f-4b4a-9631-ed8ae9c70c09)
    )
    (fp_text user "GPIO37" (at 24.13 25.4 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp c9408f33-e025-4dec-a5d8-d8734cf8261b)
    )
    (fp_text user "3V3" (at 1.27 2.54 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp ca36409f-b9d6-4b40-9a3a-7a8b83c49657)
    )
    (fp_text user "GPIO20" (at 24.13 45.72 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp e1b96867-3a41-4472-b3ad-6505cade76c3)
    )
    (fp_text user "GPIO13" (at 1.27 45.72 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp e21fb41d-0918-48f0-bb35-18412f392d95)
    )
    (fp_text user "GPIO10" (at 1.27 38.1 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp e6edd6f1-28ed-4360-b21f-b8a03fcc0386)
    )
    (fp_text user "GPIO3" (at 1.27 30.48 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp e70de6b3-fe34-40fe-bdef-f518a00652b8)
    )
    (fp_text user "3V3" (at 1.27 0 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp eb204f2d-8b8c-40fe-b956-4f65a6a68e04)
    )
    (fp_text user "GPIO12" (at 1.27 43.18 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp f0cf3cc7-26a2-4d65-9603-5fc482df84b1)
    )
    (fp_text user "GPIO44/U0RXD" (at 24.13 5.08 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp f596bfcf-e118-4ae5-b071-97c8ec2e408c)
    )
    (fp_text user "REF**" (at -0.00368 -0.00272 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0a60eb07-3bd1-4597-9400-aa0a82b912f8)
    )
    (fp_line (start -1.5 55.114) (end 26.899999 55.114)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5cf94802-8885-4447-a98d-29daa8861ab1))
    (fp_line (start -1.499999 -1.1) (end -1.5 55.114)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6fd8b4f0-ccd4-453f-89a7-ae4ee6126b1e))
    (fp_line (start 2.46012 -7.01312) (end 22.98332 -7.01312)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d5b3e699-15ed-4d57-9c5a-732ed949945c))
    (fp_line (start 2.46012 -1.12032) (end 2.46012 -7.01312)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c2684ed-91cb-4c8b-b5f8-3e0659b04ff3))
    (fp_line (start 22.98332 -7.01312) (end 22.98332 -1.12032)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6df2e4f5-ef46-469d-b3c0-ce5c9cf86e0d))
    (fp_line (start 26.899999 55.114) (end 26.9 -1.1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 29bbe88e-343d-469e-b54c-071136a8189a))
    (fp_line (start 26.9 -1.1) (end -1.499999 -1.1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a5931c1-ff43-45da-9bac-db15909d4386))
    (fp_line (start -1.25 -0.85) (end 26.65 -0.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 35e1eb40-3765-4863-8bfe-b36efd099b34))
    (fp_line (start -1.25 54.864) (end -1.25 -0.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b29035bf-df59-4b1e-b732-3b3d3c626de5))
    (fp_line (start 26.65 -0.85) (end 26.65 54.864)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7c7bbada-a256-42b4-aca5-fe8989df5257))
    (fp_line (start 26.65 54.864) (end -1.25 54.864)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 19b4cd11-aa6a-414b-970f-bd12066ab6df))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U1-3V3-Pad1)") (pinfunction "3V3") (pintype "passive+no_connect") (tstamp 395a3d57-1d5d-4a82-8720-23dad5ecdbf8))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U1-3V3-Pad1)") (pinfunction "3V3") (pintype "power_in+no_connect") (tstamp 6983c89f-53da-4ac5-a024-6cea21bc66a0))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(U1-CHIP_PU-Pad3)") (pinfunction "CHIP_PU") (pintype "input+no_connect") (tstamp 0bc582eb-bf88-4094-915c-0bc38c01d4ac))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "/Horloge Nixie/NX1BCD4") (pinfunction "GPIO4/ADC1_CH3") (pintype "bidirectional") (tstamp f4c3bee0-9bdc-4cba-b5e2-3b0aad3a0aa2))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "/Horloge Nixie/NX2BCD1") (pinfunction "GPIO5/ADC1_CH4") (pintype "bidirectional") (tstamp 22914ef9-26c0-4049-b10f-9137f5a4acab))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "/Horloge Nixie/NX2BCD2") (pinfunction "GPIO6/ADC1_CH5") (pintype "bidirectional") (tstamp 007af0df-6657-4942-a52a-95b4aa9ccfab))
    (pad "7" thru_hole oval (at 0 15.24 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "/Horloge Nixie/NX2BCD3") (pinfunction "GPIO7/ADC1_CH6") (pintype "bidirectional") (tstamp 4b285a38-52c5-4f9d-b279-22c73c948680))
    (pad "8" thru_hole oval (at 0 17.78 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(U1-GPIO15{slash}ADC2_CH4{slash}32K_P-Pad8)") (pinfunction "GPIO15/ADC2_CH4/32K_P") (pintype "bidirectional+no_connect") (tstamp 8612850d-89c9-48ad-9610-63d83ed0ee7f))
    (pad "9" thru_hole oval (at 0 20.32 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(U1-GPIO16{slash}ADC2_CH5{slash}32K_N-Pad9)") (pinfunction "GPIO16/ADC2_CH5/32K_N") (pintype "bidirectional+no_connect") (tstamp 47d8f21d-9098-42ed-bb69-26eecace0dfb))
    (pad "10" thru_hole oval (at 0 22.86 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "/Horloge Nixie/NX4BCD3") (pinfunction "GPIO17/ADC2_CH6") (pintype "bidirectional") (tstamp dc7fab85-5574-489b-b9c2-e91a22486036))
    (pad "11" thru_hole oval (at 0 25.4 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "/Horloge Nixie/NX4BCD4") (pinfunction "GPIO18/ADC2_CH7") (pintype "bidirectional") (tstamp 84c6bcee-6693-40f2-80c7-daff8333e933))
    (pad "12" thru_hole oval (at 0 27.94 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "/Horloge Nixie/NX2BCD4") (pinfunction "GPIO8/ADC1_CH7") (pintype "bidirectional") (tstamp 409efd6b-a54a-4a33-97a6-98399287ddc8))
    (pad "13" thru_hole oval (at 0 30.48 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "/Horloge Nixie/NX1BCD3") (pinfunction "GPIO3/ADC1_CH2") (pintype "bidirectional") (tstamp 14c6cf76-3ab8-4237-b6e4-817a174bf977))
    (pad "14" thru_hole oval (at 0 33.02 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "NX2A") (pinfunction "GPIO46") (pintype "bidirectional") (tstamp b133539c-a09d-4794-96ef-f2d5843b55b2))
    (pad "15" thru_hole oval (at 0 35.56 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "/Horloge Nixie/NX3BCD1") (pinfunction "GPIO9/ADC1_CH8") (pintype "bidirectional") (tstamp cc85ece5-bb27-4fc2-aa6b-a3eb6e08b3d8))
    (pad "16" thru_hole oval (at 0 38.1 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "/Horloge Nixie/NX3BCD2") (pinfunction "GPIO10/ADC1_CH9") (pintype "bidirectional") (tstamp 50bd6b00-5248-45be-ad80-d78364b6ff74))
    (pad "17" thru_hole oval (at 0 40.64 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 74 "/Horloge Nixie/NX3BCD3") (pinfunction "GPIO11/ADC2_CH0") (pintype "bidirectional") (tstamp 5e49655d-82dc-48b5-9f06-1afc473d8dc2))
    (pad "18" thru_hole oval (at 0 43.18 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 75 "/Horloge Nixie/NX3BCD4") (pinfunction "GPIO12/ADC2_CH1") (pintype "bidirectional") (tstamp a82ca284-e641-42ba-9c82-684f1b574720))
    (pad "19" thru_hole oval (at 0 45.72 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 77 "/Horloge Nixie/NX4BCD1") (pinfunction "GPIO13/ADC2_CH2") (pintype "bidirectional") (tstamp 27f5ae95-1d39-4e0f-b2b5-dc5f2c15d98e))
    (pad "20" thru_hole oval (at -0.00368 48.25728 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "/Horloge Nixie/NX4BCD2") (pinfunction "GPIO14/ADC2_CH3") (pintype "bidirectional") (tstamp 0797c203-c9fe-4e5b-af2f-56d341ac2b7e))
    (pad "21" thru_hole oval (at -0.00368 50.79728 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "5V") (pintype "power_in") (tstamp eae1e5b3-2bc8-4279-9866-723f628408a5))
    (pad "22" thru_hole oval (at -0.00368 53.33728 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive") (tstamp e4019ef4-7dc1-4e3e-8654-a34f3965be50))
    (pad "23" thru_hole oval (at 25.4 53.34 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive") (tstamp ac53bc98-394c-457e-bb83-66b5d991dd6b))
    (pad "24" thru_hole oval (at 25.4 50.8 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "passive") (tstamp b631bf39-4074-4738-8565-b61f3221e935))
    (pad "25" thru_hole oval (at 25.4 48.26 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "/Horloge Nixie/USB_D-") (pinfunction "GPIO19/USB_D-") (pintype "bidirectional") (tstamp e09be15e-0570-434a-9eeb-7af0f541d38e))
    (pad "26" thru_hole oval (at 25.4 45.72 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/Horloge Nixie/USB_D+") (pinfunction "GPIO20/USB_D+") (pintype "bidirectional") (tstamp 37d5bb5a-05cc-4213-9d59-d682c320b9a5))
    (pad "27" thru_hole oval (at 25.4 43.18 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 48 "/Horloge Nixie/IN_PHOTO_R") (pinfunction "GPIO21") (pintype "bidirectional") (tstamp 0f57a140-ec7d-414b-8c86-46f2a90937e2))
    (pad "28" thru_hole oval (at 25.4 40.64 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "NX3A") (pinfunction "GPIO47") (pintype "bidirectional") (tstamp 29316593-33bf-4f00-a043-f398322b049f))
    (pad "29" thru_hole oval (at 25.4 38.1 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "NX4A") (pinfunction "GPIO48") (pintype "bidirectional") (tstamp 96a0bcbc-99ab-4d5d-86ca-aba653edb83e))
    (pad "30" thru_hole oval (at 25.4 35.56 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "NX1A") (pinfunction "GPIO45") (pintype "bidirectional") (tstamp 72a88ddf-466e-462a-a8ba-b4a3b513842c))
    (pad "31" thru_hole oval (at 25.4 33.02 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(U1-GPIO0-Pad31)") (pinfunction "GPIO0") (pintype "bidirectional+no_connect") (tstamp 84d4af96-7bc1-42d3-aa8e-cc21df6ea77a))
    (pad "32" thru_hole oval (at 25.4 30.48 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 68 "/Horloge Nixie/IN_ENC_A") (pinfunction "GPIO35") (pintype "bidirectional") (tstamp 24b92d46-6573-4150-8271-5cedb13c4edd))
    (pad "33" thru_hole oval (at 25.4 27.94 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 69 "/Horloge Nixie/IN_ENC_B") (pinfunction "GPIO36") (pintype "bidirectional") (tstamp 6a6a9f81-66a4-4118-a9a7-b22d25157c72))
    (pad "34" thru_hole oval (at 25.4 25.4 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 70 "/Horloge Nixie/IN_ENC_SW") (pinfunction "GPIO37") (pintype "bidirectional") (tstamp d05d4529-18e9-4200-b94d-54b2ce10ff4a))
    (pad "35" thru_hole oval (at 25.4 22.86 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(U1-GPIO38-Pad35)") (pinfunction "GPIO38") (pintype "bidirectional+no_connect") (tstamp 643a06e4-81de-4031-80d1-313abe8b807d))
    (pad "36" thru_hole oval (at 25.4 20.32 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(U1-GPIO39{slash}MTCK-Pad36)") (pinfunction "GPIO39/MTCK") (pintype "bidirectional+no_connect") (tstamp 6cd9c116-cab0-4330-8f55-88dd410dcc73))
    (pad "37" thru_hole oval (at 25.4 17.78 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 73 "unconnected-(U1-GPIO40{slash}MTDO-Pad37)") (pinfunction "GPIO40/MTDO") (pintype "bidirectional+no_connect") (tstamp 0865147f-5613-414e-be5e-d6cab91d6034))
    (pad "38" thru_hole oval (at 25.4 15.24 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/Horloge Nixie/I2C_SCL") (pinfunction "GPIO41/MTDI") (pintype "bidirectional") (tstamp ff74b996-1627-450b-bbc6-614063690a99))
    (pad "39" thru_hole oval (at 25.4 12.7 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "/Horloge Nixie/I2C_SDA") (pinfunction "GPIO42/MTMS") (pintype "bidirectional") (tstamp f1533ab9-de37-42a7-9454-240a4e8e0404))
    (pad "40" thru_hole oval (at 25.4 10.16 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "/Horloge Nixie/NX1BCD2") (pinfunction "GPIO2/ADC1_CH1") (pintype "bidirectional") (tstamp f4fbc014-e345-4f04-9843-14fa7fc15ddc))
    (pad "41" thru_hole oval (at 25.4 7.62 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 80 "/Horloge Nixie/NX1BCD1") (pinfunction "GPIO1/ADC1_CH0") (pintype "bidirectional") (tstamp 943a5c23-6bbd-425f-a600-73d92046863f))
    (pad "42" thru_hole oval (at 25.4 5.08 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 76 "unconnected-(U1-GPIO44{slash}U0RXD-Pad42)") (pinfunction "GPIO44/U0RXD") (pintype "bidirectional+no_connect") (tstamp 240b0cd7-bc2f-489f-a838-cd577f98a2fd))
    (pad "43" thru_hole oval (at 25.4 2.54 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/Horloge Nixie/OUT_LEDs") (pinfunction "GPIO43/U0TXD") (pintype "bidirectional") (tstamp d4fc4f3f-7337-48f6-9fb5-f51877cc2451))
    (pad "44" thru_hole oval (at 25.4 0 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 14d7ab14-e0f5-4047-a763-c1598ee10de3))
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp e63a5714-417b-47df-aea3-e3f0db317f01)
    (at 84.8 67.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (attr through_hole)
    (fp_text reference "N2" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 223407a3-3f3a-4f0b-b46b-d279d8039ce4)
    )
    (fp_text value "IN-14" (at 0.4062 -10.0862) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 25c8375c-e5c4-4fc2-9f2d-453e113eb1d6)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 826a6a5b-0a7c-456a-a818-b91e32f7d2b1))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp f44ade3b-bfb2-4f6b-bde0-0c3d306ca215))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 94832b05-d036-407e-afcd-03d98a10dc5a))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp e82baa14-8b3d-421c-a918-41d588038a97))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 590d357a-1738-450f-adaf-2ac030ea9ac1))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 31117ec2-4b5e-4afa-a045-d47423a08663))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp 41740711-6acf-4067-a1c3-d482be084916))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pinfunction "A") (pintype "bidirectional") (tstamp 242fd2fc-5d3c-4ed4-93d0-c039985c9893))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(N2-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional+no_connect") (tstamp b4e16d05-4e2c-4894-acde-73050783bfad))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp 3420e46f-7083-4aab-83c1-bcedeb4f3870))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp 6fe42420-ab3d-4118-a43d-746d556f470b))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp 509f7996-e54a-425b-94cb-4970765329a4))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp 39d1c7a3-22f1-46d0-a54c-cf5b48554f24))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp 5c63fcef-457c-447a-83be-3268caf12ffe))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp 308b2ed9-10b2-472d-b5d3-7ad1d5ce07eb))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp 37c49039-835a-45b1-a1de-980df7ef946f))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp 6f50d81d-226e-4dee-81a7-ffd635cbee72))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp c5287cac-2a90-473f-bd10-e5dc27dc5b30))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp d13973b1-8b0c-47d8-a75a-8df7fa074f5c))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(N2-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional+no_connect") (tstamp b11a6c51-7d4a-4b38-8f96-29794de6c2a2))
  )

  (footprint "Package_DIP:DIP-16_W7.62mm_LongPads" (layer "F.Cu")
    (tstamp e7ea5d10-4ef6-4ff7-bce3-998e2861e8d1)
    (at 101.6 86.36)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/6ac4e9c3-16ef-4bd5-ab18-adfbda188a45")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6d6af38d-f4a1-4eaf-a2bc-fd910d58b92d)
    )
    (fp_text value "74141" (at 3.81 20.11) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5ecd0e04-0657-46c9-ad9c-4db05d4b45a5)
    )
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aa5f4413-3850-423d-9227-33ff4c85e546)
    )
    (fp_line (start 1.56 -1.33) (end 1.56 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9f1f2952-94bb-423f-bab5-ad55ad0c385d))
    (fp_line (start 1.56 19.11) (end 6.06 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3b023c92-95cd-49b2-b6c8-aec7abefc051))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 65470870-f8f9-4ca4-a7f5-52e5717117ba))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 691db443-53b4-4568-b4fc-d4e68b0a8695))
    (fp_line (start 6.06 19.11) (end 6.06 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d16e2fea-f3be-4ca3-ac31-ac1cf43bf033))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 13cdf6c2-e6d3-4dc3-85f5-911258ed4a0a))
    (fp_line (start -1.45 -1.55) (end -1.45 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fae24599-e11c-4faf-8c84-c31aaee61078))
    (fp_line (start -1.45 19.3) (end 9.1 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d4bfff02-0c67-4b07-a501-7433f1c243b8))
    (fp_line (start 9.1 -1.55) (end -1.45 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ba6f89c5-ed63-4331-93c2-dfd1cad7bc09))
    (fp_line (start 9.1 19.3) (end 9.1 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a80dba8b-1fe3-4011-b8ea-037593aeebf1))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f5ca0cc5-e785-4f39-b815-f09d49487a10))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9b08fb4f-dd49-4ede-818c-b19a4fb7ebf9))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d50ae00-9722-48ad-904c-8969d755dbfd))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2ad26ab1-00f5-4fee-ae75-4cb48608b403))
    (fp_line (start 6.985 19.05) (end 0.635 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c9a229ce-ee5c-47c8-879f-6acfb062b63e))
    (pad "1" thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 81 "/Horloge Nixie/NX1K8") (pinfunction "~{Q8}") (pintype "open_collector") (tstamp c8d2eebe-8e29-4639-bbe6-e742966100e3))
    (pad "2" thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 82 "/Horloge Nixie/NX1K9") (pinfunction "~{Q9}") (pintype "open_collector") (tstamp 64a2af88-e7ff-4f6c-9961-e0eebd654e8e))
    (pad "3" thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 80 "/Horloge Nixie/NX1BCD1") (pinfunction "A") (pintype "input") (tstamp b8f1dc1c-caf7-45a5-ab8e-df96064e3c6a))
    (pad "4" thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "/Horloge Nixie/NX1BCD4") (pinfunction "D") (pintype "input") (tstamp 274280ad-224c-45fe-b475-e3e4fec54b4d))
    (pad "5" thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in") (tstamp 6cc02d48-2d14-4279-95e4-f88fa2e722b8))
    (pad "6" thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "/Horloge Nixie/NX1BCD2") (pinfunction "B") (pintype "input") (tstamp 1d8eebcc-bf26-4483-a31b-70ebe28a52e5))
    (pad "7" thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "/Horloge Nixie/NX1BCD3") (pinfunction "C") (pintype "input") (tstamp fb311608-3416-458b-83f0-f3eb21891b9b))
    (pad "8" thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 83 "/Horloge Nixie/NX1K2") (pinfunction "~{Q2}") (pintype "open_collector") (tstamp 31f1880f-887d-461f-9f68-90d4f63a8703))
    (pad "9" thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 84 "/Horloge Nixie/NX1K3") (pinfunction "~{Q3}") (pintype "open_collector") (tstamp 70ec2b6a-69b9-4ce6-b580-db6d793785b2))
    (pad "10" thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 85 "/Horloge Nixie/NX1K7") (pinfunction "~{Q7}") (pintype "open_collector") (tstamp 7e06b021-512b-4053-81c7-192d3c49d7c3))
    (pad "11" thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 86 "/Horloge Nixie/NX1K6") (pinfunction "~{Q6}") (pintype "open_collector") (tstamp b5cc8296-a18b-44ce-9a59-d192630f2c90))
    (pad "12" thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp a0f8c95c-8c94-4618-b225-2cbcc8b64528))
    (pad "13" thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 87 "/Horloge Nixie/NX1K4") (pinfunction "~{Q4}") (pintype "open_collector") (tstamp 4466a9e5-109c-48e2-983a-32aefb6cbb08))
    (pad "14" thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 88 "/Horloge Nixie/NX1K5") (pinfunction "~{Q5}") (pintype "open_collector") (tstamp 7c2eca7f-e163-48cd-95a6-21add395e4ff))
    (pad "15" thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 89 "/Horloge Nixie/NX1K1") (pinfunction "~{Q1}") (pintype "open_collector") (tstamp d3874876-5dba-4d7a-967b-75c2f2994795))
    (pad "16" thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 90 "/Horloge Nixie/NX1K0") (pinfunction "~{Q0}") (pintype "open_collector") (tstamp fb2310bc-9269-4b5b-bed6-1005f3bb1c28))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp ea68b619-67a1-40e4-b31f-965b2b5d9b9c)
    (at 132.03 40.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0ca726e4-7b2d-4fba-9c3f-fa1046cb65f2")
    (attr through_hole)
    (fp_text reference "Q7" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c6e3b9b5-e6e0-49f9-bb04-f9f4ade859e9)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0c43ce4a-611d-4c88-8feb-e0db8b0126a9)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 526e96bd-2c84-488b-91b8-b8c6bb390c9c)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d0d16848-316e-437e-b937-5d8f5a50b4f9))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 20f7b9d7-4784-4509-b543-b935c5577299))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5261fbb-a7d7-471e-89a5-4361eb369f72))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bcd28ebd-a4f8-423c-85bb-9def51dd88b3))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 53743ef9-007a-4628-bce8-0dc8f88e2bf3))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32f4815c-0a4e-412a-8562-9084266e321d))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 51469418-b80b-4206-aef1-86627787e3b1))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 92960cb3-fb18-4a75-ac25-55d1d2ee9c65))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 921ac109-9cb4-4780-b619-8ede1b913681))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d76583d-44b4-4e1a-b182-5d2d519f5554))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(Q7-B)") (pinfunction "B") (pintype "input") (tstamp 2aac40ae-1d3f-444b-a659-356260990d37))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(Q7-C)") (pinfunction "C") (pintype "passive") (tstamp 67223643-d353-4c3e-8e1c-2500f4b59557))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "E") (pintype "passive") (tstamp bd629e56-a449-41e9-8a52-55289b7914e0))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp ec49fc01-ed41-4572-9157-8a3dcfdabcba)
    (at 138.7 30.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/8efa8390-0fb2-43f9-a2ff-1010f64758ea")
    (attr through_hole)
    (fp_text reference "R16" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f7b4c0af-7589-46b2-8d9a-588e4055eb59)
    )
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c549dadb-1516-4d06-ab9e-133c8453d398)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4ce65be6-aaef-4aa5-b1a1-f75c33897b71)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d3dfc68-acdd-41d2-b0bf-a4ff2ac0becb))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c2e9d0da-eba1-4386-a23f-cae94c6f27f0))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d3f12c38-b197-448b-bb36-57633c7b92da))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec908954-cbc4-4708-9a2f-6d8912e29d5c))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4daf09bd-080e-4ac5-a0ab-1ab94916720c))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0016a62c-c7d5-4bbd-b2d3-c8648ab020f9))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 86e9a7e1-c3d9-4167-901b-582ee02f9cbe))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 69281d27-4c37-457a-b0ee-bfdf259057c2))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d24be73b-75fc-4bb2-b8c9-e11b2e51e2db))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 78fc89cc-8464-4935-b853-475ffc3f6ce2))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c32cf494-9010-4700-92c0-195790936051))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a030134b-3f02-49a7-9ea5-a32db94de820))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8f111be9-0757-449c-a1fd-a1e85fe6212c))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b7742052-1276-46fe-aa8f-c6cabd264701))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a6c1a724-e53c-4697-bc60-b6661756a8d2))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a9994667-9df3-418b-98f5-b244116fbf8c))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pintype "passive") (tstamp fc612fc6-caa3-4f16-b159-8d3c84837764))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(Q8-C)") (pintype "passive") (tstamp a6ae5685-1739-46fa-9701-97731d8d198d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp ede73228-26cd-4a7a-87d6-f0bbb64f89bc)
    (at 55.084 44.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/63bc0011-29e7-4bc3-8003-22d7bd5fe3f4")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5978fb46-7029-4995-a9dd-8254a9ecec67)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ffa776c1-4996-4ea2-9657-f2fc79b1d85e)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f55a3ed4-a562-4c50-9172-7c6e5a37f666)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa83a3df-b249-41a1-98cb-18df257ead17))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a53c4f7d-d612-4112-974a-96685326316e))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5fc56b50-54ab-4ce4-88b1-1e68f6cc5ba7))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 25cc983f-1c2b-413a-a69f-b30edf2637aa))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 32aa7486-94a5-4294-af6c-39557ec22d1f))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 076c41fc-1f48-49c6-ac36-e17123b0b03d))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp abe2c5b8-608d-40ef-a293-5a7ac735f8ff))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b2331534-fb95-4056-88e3-e398b42380c1))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0f7bc59b-845e-47b7-a404-68c31f4a0716))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1f9142c5-c20f-4de8-85a5-0a686a535b69))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(Q1-B)") (pinfunction "B") (pintype "input") (tstamp 9f48bce6-1fd9-488f-9124-b6548757bff0))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(Q1-C)") (pinfunction "C") (pintype "passive") (tstamp eb20dbda-dc16-469d-8a90-a0f942451668))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "E") (pintype "passive") (tstamp 55318af4-1de3-4338-8c2d-4edfe7844a30))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp f274e8c4-1938-41f6-b441-6dbe8df2db8f)
    (at 80.53 42.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0f18661e-c1ab-4cfa-9ad7-0c6b5dc8e354")
    (attr through_hole)
    (fp_text reference "Q3" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed6293e2-1e7d-479a-b35d-6b910d006df6)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 50f273e3-f093-4c4f-be02-92662ca52d26)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4190198d-7e08-4b95-a418-edfee2edb26e)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c377cb0c-32a5-48cb-b926-256de505e174))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a4c02f2b-cccc-461f-a1e0-eeec0b2040d1))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e05e2f99-5713-4761-b99b-ce3478bf32ac))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 59a0211b-3843-4c32-b643-f9e4f4819532))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9be79425-a066-48ee-8910-113d1c55f519))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c68571f1-fa1c-4050-a2c9-f4278f9cbf01))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c8f91a74-aba4-4f16-a562-3b9f9e71d21b))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7b3e6560-fed5-4fa3-a399-ff7118b19f62))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c224adca-323c-4f2a-b760-4aab76394b4d))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43c7d8e9-a774-4d47-8f6c-45740dc14a40))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(Q3-B)") (pinfunction "B") (pintype "input") (tstamp febc112e-280f-43c3-a78c-d2f6317817ca))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(Q3-C)") (pinfunction "C") (pintype "passive") (tstamp 79636a6b-c55a-4c8f-a744-01a1d94ab122))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "E") (pintype "passive") (tstamp 9d96d241-65c2-467d-a47c-002e75d7233f))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp f3279155-4a66-44cf-b129-6dcfa57de93e)
    (at 88.63 41.784)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0c193db8-2f74-442a-af78-e641792bf8f2")
    (attr through_hole)
    (fp_text reference "Q4" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0357bd81-78ac-4c5b-a796-abc536e4ed32)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb29f57c-2543-441e-9d3d-e24ce2f5766b)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d915b15a-359e-4a50-bc66-e0a55a5627dd)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da22cfc2-c66b-4148-bfaa-d35654323e9b))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 73820ad4-0902-41b2-8eff-d714ce989d64))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0300a2d-02ef-4384-9103-9ab2474fe241))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a3f2f5f9-9437-4496-9dd5-e9adf0a1c67f))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6a345b9f-983d-4f1b-8150-ff4b9d14c8a2))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c5b3cd4b-6a26-4874-aa53-20d2d359545f))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f298187c-5c42-4473-b22c-7d9f67b4c4de))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f2a4e401-8633-41d1-9fa8-126d95d82850))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6b3424d4-21b4-4caf-9d10-780d975485dd))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a306296d-e13f-4050-86b3-956381cd4aad))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(Q4-C)") (pinfunction "C") (pintype "passive") (tstamp 21453c37-ff94-4eb9-b552-8f44b319a115))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(Q4-B)") (pinfunction "B") (pintype "input") (tstamp 40977e15-79eb-4bd6-89a8-0674d8a7da45))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pinfunction "E") (pintype "passive") (tstamp d74756a4-14a3-47e3-a5d5-be7605fc42b9))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tstamp f4f600f5-80f0-408e-ba6b-c30e67e513b9)
    (at 116.731 67.7138 90)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/920cc3eb-a9aa-4c86-83b6-03eae4e08e3b")
    (attr smd)
    (fp_text reference "D3" (at 0 -3.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da58b796-12e9-4475-b8cb-15cef56fb212)
    )
    (fp_text value "WS2812B" (at 0 4 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 72d8a4e7-0585-4b69-a4aa-29eaa5aa524c)
    )
    (fp_text user "1" (at -4.15 -1.6 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fad72673-5d14-4433-a314-0c08ad85741c)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.15)))
      (tstamp de2fd491-3485-45fb-83c0-0234fded7237)
    )
    (fp_line (start -3.65 -2.75) (end 3.65 -2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc98753f-229d-47e5-a26c-55ca43638988))
    (fp_line (start -3.65 2.75) (end 3.65 2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 66685ea6-43a2-4bc1-8434-5269676819f7))
    (fp_line (start 3.65 2.75) (end 3.65 1.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f17332c9-3031-47ee-9a99-5197c91d9b90))
    (fp_line (start -3.45 -2.75) (end -3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 39d5efb3-0d83-4fb3-b5a0-60e472bd28a3))
    (fp_line (start -3.45 2.75) (end 3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4d4b2a3b-4f5a-4304-ae3b-353e76f285e8))
    (fp_line (start 3.45 -2.75) (end -3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 328565ec-0d38-44ff-8d0b-4d637a81d262))
    (fp_line (start 3.45 2.75) (end 3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b76dcf9a-86e6-4556-a32c-256bfd5b782f))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5c750abd-d996-4611-b532-9ca096a18713))
    (fp_line (start -2.5 2.5) (end 2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4be67ccc-9dbc-4cb0-8455-02011c8d2b98))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a942e661-c85a-4221-9445-21f605dfa7ca))
    (fp_line (start 2.5 1.5) (end 1.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c54cbee-d8ed-4f33-9bf6-ca88c6e268ee))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1bc5975c-de19-4239-82e8-ad9a59af21a7))
    (fp_circle (center 0 0) (end 0 -2)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 4ba730aa-9c96-40b6-a38a-41d45bce4ab5))
    (pad "1" smd rect (at -2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in") (tstamp 244c66b0-1a2b-41f1-8a51-d969c1107322))
    (pad "2" smd rect (at -2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(D3-DOUT)") (pinfunction "DOUT") (pintype "output") (tstamp 17f56a84-6b7d-44e7-bbf2-5ccc18c38054))
    (pad "3" smd rect (at 2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp b491b922-515e-41b8-9e1f-71e0085b8cac))
    (pad "4" smd rect (at 2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(D2-DOUT)") (pinfunction "DIN") (pintype "input") (tstamp ce572f2e-3ee3-479d-b295-b2a77a9eb8e3))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tstamp f58632e1-deab-4e63-8c98-27eb64dceee7)
    (at 84.8 67.8 90)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "RGB LED with integrated controller")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/1f0ae004-3394-4213-98c8-a30115430518")
    (attr smd)
    (fp_text reference "D2" (at 0 -3.5 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 742233cf-0fdf-4844-8110-0b2d1e02c61d)
    )
    (fp_text value "WS2812B" (at 0 4 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bdf6ed8f-99e0-45fc-ae46-7790dbc4e73d)
    )
    (fp_text user "1" (at -4.15 -1.6 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 63c02cf6-81a4-4cb0-83a7-bad123ee97d7)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.15)))
      (tstamp 9972449b-dc9d-418b-ac48-f403fc0038cb)
    )
    (fp_line (start -3.65 -2.75) (end 3.65 -2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1ce72c22-a1ce-41e2-b831-bbad9bf06db1))
    (fp_line (start -3.65 2.75) (end 3.65 2.75)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8fc4eded-5575-4651-b130-8a8906cd1b05))
    (fp_line (start 3.65 2.75) (end 3.65 1.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdc8eb3e-07b5-4f21-87dc-6795cf184b61))
    (fp_line (start -3.45 -2.75) (end -3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 39cc8417-aa00-4e72-9d40-7bb249cd1dc3))
    (fp_line (start -3.45 2.75) (end 3.45 2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4cca8361-c442-478d-8a3a-3a14fbe43127))
    (fp_line (start 3.45 -2.75) (end -3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f716929e-7a01-497d-b74a-bee4fb80ebd3))
    (fp_line (start 3.45 2.75) (end 3.45 -2.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8800e96e-c3bb-41f7-a48b-1fd79c4e2b87))
    (fp_line (start -2.5 -2.5) (end -2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 66bdaa51-107b-432c-9e9a-f72c231ca440))
    (fp_line (start -2.5 2.5) (end 2.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8eae3422-4c6d-4079-8580-f0ed1ac40ca5))
    (fp_line (start 2.5 -2.5) (end -2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db25afe7-4f42-4d78-81c1-af8046a5651b))
    (fp_line (start 2.5 1.5) (end 1.5 2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 54da61d1-c14e-45ec-8472-0ab63e75378f))
    (fp_line (start 2.5 2.5) (end 2.5 -2.5)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d56cdb9c-98b9-4bd3-936c-feaf97c3cf92))
    (fp_circle (center 0 0) (end 0 -2)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp c77c4bcd-6f24-4a12-8775-41c14238c68c))
    (pad "1" smd rect (at -2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in") (tstamp 276f3ed0-0e76-48f6-9090-7c817627c73c))
    (pad "2" smd rect (at -2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(D2-DOUT)") (pinfunction "DOUT") (pintype "output") (tstamp 95f4b1b5-1a7a-450b-800b-a47cde5381e6))
    (pad "3" smd rect (at 2.45 1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "VSS") (pintype "power_in") (tstamp e453e436-6095-41cd-b1cc-2863fef3decd))
    (pad "4" smd rect (at 2.45 -1.65 90) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(D1-DOUT)") (pinfunction "DIN") (pintype "input") (tstamp 52a88a66-be1b-49d6-b951-60c8adb9c766))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tstamp f69a6716-eba7-4ac1-a3c7-8464804a78b8)
    (at 118.3 53.8 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/199e4760-ddb9-4a86-87ab-c5ff873dfc88")
    (attr through_hole)
    (fp_text reference "R12" (at 5.08 -2.37 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9b872c61-99bf-4ab0-a54c-b2128d013773)
    )
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3aca2c29-e961-4235-a427-a0e2a2cb7bd1)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8611260a-daf5-445d-98a2-0146e96bc5b0)
    )
    (fp_line (start 1.04 0) (end 1.81 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e69ea32c-d6c6-4f37-8395-1fc53517235a))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42b6f01c-d218-4c44-b31d-c08c1c3375ae))
    (fp_line (start 1.81 1.37) (end 8.35 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f30e2588-53e6-4c9a-b2b3-46f214f744a2))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2918dd6d-6026-4427-9285-8c7cf486f9a2))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc2b0eea-7d9f-4124-a204-6defca47a79a))
    (fp_line (start 9.12 0) (end 8.35 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d090a6d-2cc4-4e30-807f-c513530bb415))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bc9b48ac-ed2f-4bd0-8baf-309be868fc19))
    (fp_line (start -1.05 1.5) (end 11.21 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 95084e95-94a8-460d-92c9-360b2a0ad96e))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e470e94c-07d5-413a-88d7-6236759ac826))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ae088f42-f0e2-40ff-a686-1fdcb7e77918))
    (fp_line (start 0 0) (end 1.93 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e2048d6-8c1b-4782-bd7c-8237aeb0fdfc))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 686e6c40-d217-418b-9b7c-f60a5f4ffd1a))
    (fp_line (start 1.93 1.25) (end 8.23 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 58fbbd02-7eec-43bb-aa95-3390bd382ec4))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1f80709-17a2-433a-a32f-9e437f20828f))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d91d3acc-7edb-423a-ab56-76105b553405))
    (fp_line (start 10.16 0) (end 8.23 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 82c42484-d375-4bf3-9f33-bdee368e00e4))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 47 "/Horloge Nixie/A_M01") (pintype "passive") (tstamp d4834a53-5ebf-4ae8-b908-1785fc80839e))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(Q6-C)") (pintype "passive") (tstamp 8a2a24a4-ad62-432e-988e-18042fba8155))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp feeddce8-11da-41b9-bdab-11f00f192777)
    (at 145.8 55.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fd563363-7a17-4f8c-87a2-d2679d06de9c)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fdf22a3d-14a9-404d-914d-53f6b4388b68)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19036cc9-b417-45c3-8465-55f9ee5ec199)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 65b7b46d-b04b-4b4a-99f7-6b70673492da))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f8cc41a2-f219-4b9c-8458-7e47f98fa7f8))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 31bf90e7-5aec-49f7-aa00-ba4d65d19694))
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp fff31730-ae9f-4022-af55-fb522b97199d)
    (at 26.67 62.23 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/4b33c1bb-b6ce-41da-b1a7-444dddb36773")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ae7797e0-59d4-4e81-90be-bfc5b3242dc4)
    )
    (fp_text value "Conn_01x05" (at 0 12.49 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d810348-c7f4-4f28-b494-d64b7183e79b)
    )
    (fp_text user "${REFERENCE}" (at 0 5.08) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 315375a4-a983-4064-bf01-2499e7ad7fd5)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5d6e13b5-2cdf-4525-bde3-b65e205882c1))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7699d943-e977-4a10-b3b3-b20d76632430))
    (fp_line (start -1.33 1.27) (end -1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ea45f2e-ea31-414e-9988-4b2c52e48047))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 23bb54c2-1fd4-4288-8dcd-bd3f7daa42f0))
    (fp_line (start -1.33 11.49) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6a641b62-384a-42e1-829e-56414aba2aad))
    (fp_line (start 1.33 1.27) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3108e16d-c03d-4a82-9d4d-b3da0b66e8e5))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3a703df4-b25e-47f5-9739-69eb57d6c7cf))
    (fp_line (start -1.8 11.95) (end 1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ebba5cda-ab35-4600-b055-21e3de91d0f0))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 330bbc69-ef52-417d-b4d9-549e70fdc0ed))
    (fp_line (start 1.8 11.95) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6c68dfe8-cb7c-4025-bcb6-5ee2b0f43a53))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d2de3b27-8f8a-480d-a2ae-6d926229f7ef))
    (fp_line (start -1.27 11.43) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8934c9aa-f5fe-41f5-9d06-09669a6fa4d9))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7f401548-40b7-4ff4-986d-e173b8730be6))
    (fp_line (start 1.27 -1.27) (end 1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b95a94ac-89a6-494a-9451-e1567f0a8bf0))
    (fp_line (start 1.27 11.43) (end -1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bf0af519-7bc7-4ac9-bd19-f8105b0d58a3))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive") (tstamp b8a36177-c33e-4a9b-a643-35528a88c06b))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp 0847eba0-2eda-40ec-a45a-87992541efde))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp 05d1af23-eb60-4f22-815d-3118d006a4f5))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp 359ab67d-9bb0-47c5-918e-d17d72036ca2))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "HT") (pinfunction "Pin_5") (pintype "passive") (tstamp e5db6488-8af5-4e02-b081-1dd896b4c95f))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 50.8 50.8) (end 150.8 120.8)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 978ab02a-4d02-4f36-9c71-6b032c574b96))
  (dimension (type aligned) (layer "F.Cu") (tstamp 695fff3d-1e75-4196-aa04-10fc05075efa)
    (pts (xy 50.8 42.8) (xy 150.8 42.8))
    (height -4)
    (gr_text "100 mm" (at 100.8 37) (layer "F.Cu") (tstamp 695fff3d-1e75-4196-aa04-10fc05075efa)
      (effects (font (size 1.5 1.5) (thickness 0.3)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 10404ab6-f20f-48d5-a5b9-c84f81ea443d)
    (pts (xy 48.8 115.8) (xy 48.8 120.8))
    (height 3)
    (gr_text "5 mm" (at 43.8 117.8 90) (layer "Dwgs.User") (tstamp 10404ab6-f20f-48d5-a5b9-c84f81ea443d)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5))
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 22c28744-5d7e-4bf8-8048-23db71a5565d)
    (pts (xy 48.8 55.8) (xy 48.8 115.8))
    (height 3)
    (gr_text "60 mm" (at 44.65 85.8 90) (layer "Dwgs.User") (tstamp 22c28744-5d7e-4bf8-8048-23db71a5565d)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 33737eb9-0750-447a-8981-ee77596297d5)
    (pts (xy 42.8 120.8) (xy 42.8 50.8))
    (height -2)
    (gr_text "70 mm" (at 39.8 85.8 90) (layer "Dwgs.User") (tstamp 33737eb9-0750-447a-8981-ee77596297d5)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 696cb32d-76f9-483d-93ea-19fa109940ca)
    (pts (xy 48.8 50.8) (xy 48.8 55.8))
    (height 3)
    (gr_text "5 mm" (at 43.8 53.8 90) (layer "Dwgs.User") (tstamp 696cb32d-76f9-483d-93ea-19fa109940ca)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5))
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp f5243de0-5dc3-4a59-8fa6-89f61ca630e3)
    (pts (xy 50.8 122.8) (xy 150.8 122.8))
    (height 5)
    (gr_text "100 mm" (at 100.8 129.3) (layer "Dwgs.User") (tstamp f5243de0-5dc3-4a59-8fa6-89f61ca630e3)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5))
  )

)
