(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 50.8 50.8)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "unconnected-(C1-Pad1)")
  (net 2 "unconnected-(C1-Pad2)")
  (net 3 "+5V")
  (net 4 "/Horloge Nixie/USB_D-")
  (net 5 "/Horloge Nixie/USB_D+")
  (net 6 "GND")
  (net 7 "/Horloge Nixie/I2C_SCL")
  (net 8 "/Horloge Nixie/I2C_SDA")
  (net 9 "unconnected-(J2-Pin_4-Pad4)")
  (net 10 "HT")
  (net 11 "A_M10")
  (net 12 "unconnected-(N1-RHDP-Pad2)")
  (net 13 "/Horloge Nixie/K0")
  (net 14 "/Horloge Nixie/K9")
  (net 15 "/Horloge Nixie/K8")
  (net 16 "/Horloge Nixie/K7")
  (net 17 "/Horloge Nixie/K6")
  (net 18 "/Horloge Nixie/K5")
  (net 19 "/Horloge Nixie/K4")
  (net 20 "/Horloge Nixie/K3")
  (net 21 "/Horloge Nixie/K2")
  (net 22 "/Horloge Nixie/K1")
  (net 23 "unconnected-(N1-LHDP-Pad13)")
  (net 24 "A_M01")
  (net 25 "unconnected-(N2-RHDP-Pad2)")
  (net 26 "unconnected-(N2-LHDP-Pad13)")
  (net 27 "A_H10")
  (net 28 "unconnected-(N3-RHDP-Pad2)")
  (net 29 "unconnected-(N3-LHDP-Pad13)")
  (net 30 "A_H01")
  (net 31 "unconnected-(N4-RHDP-Pad2)")
  (net 32 "unconnected-(N4-LHDP-Pad13)")
  (net 33 "Net-(Q1-C)")
  (net 34 "Net-(Q1-B)")
  (net 35 "Net-(Q2-C)")
  (net 36 "Net-(Q2-B)")
  (net 37 "Net-(Q3-C)")
  (net 38 "Net-(Q3-B)")
  (net 39 "Net-(Q4-C)")
  (net 40 "Net-(Q4-B)")
  (net 41 "Net-(Q5-B)")
  (net 42 "Net-(Q5-C)")
  (net 43 "Net-(Q6-B)")
  (net 44 "Net-(Q6-C)")
  (net 45 "Net-(Q7-B)")
  (net 46 "Net-(Q7-C)")
  (net 47 "Net-(Q8-B)")
  (net 48 "Net-(Q8-C)")
  (net 49 "H10")
  (net 50 "H01")
  (net 51 "M10")
  (net 52 "M01")
  (net 53 "BCD1")
  (net 54 "BCD4")
  (net 55 "BCD2")
  (net 56 "BCD3")
  (net 57 "Net-(U2-3V3-Pad1)")
  (net 58 "unconnected-(U2-CHIP_PU-Pad3)")
  (net 59 "unconnected-(U2-GPIO15{slash}ADC2_CH4{slash}32K_P-Pad8)")
  (net 60 "unconnected-(U2-GPIO16{slash}ADC2_CH5{slash}32K_N-Pad9)")
  (net 61 "unconnected-(U2-GPIO17{slash}ADC2_CH6-Pad10)")
  (net 62 "unconnected-(U2-GPIO18{slash}ADC2_CH7-Pad11)")
  (net 63 "unconnected-(U2-GPIO46-Pad14)")
  (net 64 "unconnected-(U2-GPIO9{slash}ADC1_CH8-Pad15)")
  (net 65 "unconnected-(U2-GPIO10{slash}ADC1_CH9-Pad16)")
  (net 66 "unconnected-(U2-GPIO11{slash}ADC2_CH0-Pad17)")
  (net 67 "unconnected-(U2-GPIO12{slash}ADC2_CH1-Pad18)")
  (net 68 "unconnected-(U2-GPIO13{slash}ADC2_CH2-Pad19)")
  (net 69 "unconnected-(U2-GPIO14{slash}ADC2_CH3-Pad20)")
  (net 70 "unconnected-(U2-GPIO21-Pad27)")
  (net 71 "unconnected-(U2-GPIO47-Pad28)")
  (net 72 "unconnected-(U2-GPIO48-Pad29)")
  (net 73 "unconnected-(U2-GPIO45-Pad30)")
  (net 74 "unconnected-(U2-GPIO0-Pad31)")
  (net 75 "Net-(U2-GPIO35)")
  (net 76 "Net-(U2-GPIO36)")
  (net 77 "Net-(U2-GPIO37)")
  (net 78 "unconnected-(U2-GPIO38-Pad35)")
  (net 79 "unconnected-(U2-GPIO39{slash}MTCK-Pad36)")
  (net 80 "unconnected-(U2-GPIO40{slash}MTDO-Pad37)")
  (net 81 "unconnected-(U2-GPIO44{slash}U0RXD-Pad42)")
  (net 82 "unconnected-(U2-GPIO43{slash}U0TXD-Pad43)")

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 03c1d73b-a424-4839-a8ed-ce058d18497a)
    (at 168.07 38.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/ed433585-dc61-424a-820c-37cda7e01adc")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 82088aa0-a54b-4e4e-bbed-7f935bc892c4)
    )
    (fp_text value "470k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp deea3aa7-fea6-4769-8788-b5172ec13c0e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp d875626a-abd8-44c6-9e1a-e70e63babd48)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c6a8986b-f3cc-4dbe-b970-b84e017d1681))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d00cfb84-7246-4d5b-ba81-6f6b34874d9f))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ede2a9ea-d2f3-4135-aa7a-15ee926bc97a))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5e294a33-cf29-4438-bd66-d4d2ee43b73d))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a6358597-f0f0-49da-a3fd-c5f2f312b4a3))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0b7833eb-2247-4f69-bd2d-d07898f78ff2))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5d44160d-8929-4eb2-b36c-9343065ab8f2))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 04ffe3b6-8065-470a-afd9-f926d685e7ba))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c6be426-8879-4f42-9a12-48ae4d5c4707))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4842f601-95cf-47bd-8b5e-d81646422e54))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 48 "Net-(Q8-C)") (pintype "passive") (tstamp f1ba3649-3f71-408a-96fb-2c772bd50ae6))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 40 "Net-(Q4-B)") (pintype "passive") (tstamp 85991d5a-2cfc-4ce2-83aa-f8687d14201f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp 120db33d-d11e-4ab9-8c21-bed108456ee1)
    (at 175.8 115.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 610a3846-187c-4700-81af-de43361b7dc6)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6af5934d-1dc5-4fba-960e-a97e570a103d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bb63c6c3-25a1-4d18-b86e-5017a821a3bf)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 3cd80b79-dc1c-4967-be90-6aa96b86a186))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 63d9542c-8d51-40bb-a07a-6f1b43a8fef2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 431e9ae2-c293-4ff8-ac5d-b9b3e8e4b5bc))
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 14086cd0-5c99-4d2a-8dcb-a84368cc0cc3)
    (at 175.8 97.18)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch")
    (property "ki_keywords" "rotary switch encoder switch push button")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/ce68a31a-568b-4e57-b0bb-55bda0e65ee5")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp da1655b5-d178-4a28-a178-4b4fa87dd101)
    )
    (fp_text value "Rotary Encoder" (at 0 12.49) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9cd4a54a-24bc-4e5d-bd1e-c60c2be10c31)
    )
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp effbff79-9bb9-4325-a056-adcba554a8c6)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1b43c841-c0ce-4744-9108-ac367daaa7f6))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7644dd1d-45a4-400e-9fd6-797ac3fdb826))
    (fp_line (start -1.33 1.27) (end -1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0406fabc-ffb6-4772-95a5-837446f5b22f))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7557c2be-a469-40eb-9744-aaefe7e823a3))
    (fp_line (start -1.33 11.49) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1f38303c-dd96-4730-9e2e-7a87a6facffb))
    (fp_line (start 1.33 1.27) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3808be78-24b6-44bc-ad63-8bef0497fb57))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 04e666c3-b785-4b94-abec-480c5a489a28))
    (fp_line (start -1.8 11.95) (end 1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9f27ca16-7dbb-4e0d-9baf-92e16d52d124))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2546f9c6-fb2f-4a7e-8ef7-f6c69c758642))
    (fp_line (start 1.8 11.95) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f9f5398f-1e04-42bd-ab9c-7175b3a25d5c))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 512f6f48-102f-4b6b-a92c-6aca55593c4a))
    (fp_line (start -1.27 11.43) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b072664d-83e2-43ac-a1f6-2703a936282a))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3c401b01-af8c-487e-9871-97017204f597))
    (fp_line (start 1.27 -1.27) (end 1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d375c99c-f2ae-4989-8975-8c716e4173b5))
    (fp_line (start 1.27 11.43) (end -1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bb8184a5-e93a-4781-96ad-3de2614e3729))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 0909de09-322a-4126-837b-24ebb5365fd2))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp d24df2c0-20fd-41e9-b498-75e2c2af4bbc))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 5520a6ec-47e7-487e-b4b2-d6ce60d93dc9))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 667aa0de-d7cd-4077-a531-ecc3e2f1fdd6))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask") (tstamp 415046af-efb2-4845-aec9-093cbc869175))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tstamp 1820000d-4951-4760-81fc-b14190c7b2a4)
    (at 61.8375 36.8)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/ad549f04-e2cc-423b-9b39-42f4b3aa5e16")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 357b1efc-df78-4de9-ad11-11458edb0863)
    )
    (fp_text value "0.1uF/16V(10%)" (at 0 1.68) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a638f07b-de90-43f7-b775-d84625adb476)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 08ca02a9-18e3-4a81-ac51-59b6d6fc5efa)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 644e47e6-2233-4358-97c3-52df15967b08))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 75aef6f6-b881-46c4-979e-39f897e88355))
    (fp_line (start -1.88 -0.98) (end 1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e6c9df49-078c-496c-b41a-49fbc127b022))
    (fp_line (start -1.88 0.98) (end -1.88 -0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8a14d4f7-1497-4275-bbae-5604c121e3c8))
    (fp_line (start 1.88 -0.98) (end 1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2014f954-3232-4415-9166-ea153f9f9144))
    (fp_line (start 1.88 0.98) (end -1.88 0.98)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e39b8687-a474-4333-b6b8-2829833367a2))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f961c9a9-23a1-4172-94ec-be0f435e10df))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 650f0956-a972-45c3-b49c-b7d784a49e10))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37e03bf8-0a29-4984-8e71-4b5074644d85))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fc6ee60b-60c0-46fe-9f7f-da5a5eaea68b))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "unconnected-(C1-Pad1)") (pintype "passive") (tstamp 6ca3695d-9dca-4f38-9d27-b10015c5f09c))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "unconnected-(C1-Pad2)") (pintype "passive") (tstamp 3ab42f84-d1fd-4d7c-b162-1b708b4c4e74))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 1b339db9-2fdb-48f0-b0da-90be6a889b54)
    (at 53.8 99.72)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/c3280cc1-b9fe-4ecd-84d2-4de8d66c519e")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f16f536f-39b0-47d4-8f79-878b71798764)
    )
    (fp_text value "Conn_01x04" (at 0 9.95) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 93f06435-29aa-4a38-9d49-a7fef021f7b5)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1b0bd750-18d4-4e03-92e0-194d00732722)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 182dc54c-19d8-4ca9-ac0e-2c5beab4c250))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d12c5914-a930-4478-8281-9ddc46afd480))
    (fp_line (start -1.33 1.27) (end -1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2add4168-74ff-4f01-89a6-c383aff5975f))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 594c1093-0c31-44fa-847a-ac62bc988f60))
    (fp_line (start -1.33 8.95) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 19d49d66-b530-4167-bb44-f356ad1e718f))
    (fp_line (start 1.33 1.27) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6cab6491-a7c0-426d-9c33-683b47bdb543))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e1c07fcd-baab-487a-a71e-81680a26c591))
    (fp_line (start -1.8 9.4) (end 1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 609de0f1-c89f-4316-8337-72bc6d4beeeb))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3dec8838-baf3-4015-9a90-02ee6ab4a621))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4624c968-2d02-43b4-9cfc-e7dbc5444708))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d1390fd3-d998-4842-b65c-442dd2f408b5))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5937d786-c4c6-483e-9b38-bfb9bc8542b7))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c90d6058-9bbc-4b52-af5c-7e89a8e2f527))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eaa7b9ed-1924-4ae6-994c-46614410e961))
    (fp_line (start 1.27 8.89) (end -1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp db29a6b1-6678-4c01-a4e7-07c617f2cea6))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive") (tstamp 93d86284-1e15-4c20-b117-5799ceb5da72))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/Horloge Nixie/USB_D-") (pinfunction "Pin_2") (pintype "passive") (tstamp 56c7e0c5-3eec-45c1-b89e-112e42c692db))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/Horloge Nixie/USB_D+") (pinfunction "Pin_3") (pintype "passive") (tstamp 7c4122d9-c101-4ef3-8a97-c0679d219f69))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp e3c97b5c-5ae3-40f8-a912-5f5bf5f6e018))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp 1d03a62a-98b3-4842-875a-807380ecc511)
    (at 153.8 64.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0d165883-6a0d-4726-8dfc-8b4476c221d1")
    (attr through_hole)
    (fp_text reference "N4" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 08f813c6-a0cc-4156-9d6c-3f2f36a0686a)
    )
    (fp_text value "IN-14" (at -7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 7e701589-7899-49b5-a103-d45970121f21)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp f97f1786-fa25-422a-a158-96475263c8e2))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 943a991b-c933-4d7d-a732-0813d7133efe))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 074dd4ee-3d7b-4e51-87b8-face2fb37780))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 6d3f1b7d-548c-4613-b7a1-61d4ca4ac908))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp ae53a385-f55c-4efd-aa81-e3286bbb45b2))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 3603e99f-fcaf-44e3-9b49-a9a66ade9dab))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp 1860eb77-e882-4479-af01-b6a484f4211e))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 24 "A_M01") (pinfunction "A") (pintype "bidirectional") (tstamp af2d21ae-b10f-44e9-8166-adb58ec53a64))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(N4-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional") (tstamp 073d8e91-6799-434b-b6fa-d58c4d5a93c4))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp 81a71689-8c49-4fcc-a202-58b6544da96f))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp dc4d8759-57b4-474c-a0f9-2128e5d61d9d))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp 272186d7-2109-4d08-a653-63cbd9ffeb48))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp 731107f3-0696-4b71-a823-1383eb470d8e))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp 3ac0cb76-5861-4d58-ba33-d2a44f2e4d9f))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp 5ea75d5c-17a8-49ef-9ea5-212732fd586c))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp 30ee4bd2-28aa-42de-83ea-859452735f79))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp 5bbaa1d5-1001-4cf4-a5de-448555e5482c))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 21 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp fda6f81b-aaa9-49d8-ad2c-8bb0710065c9))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp 9f1d8b94-4120-4565-af04-a1a4990373a2))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(N4-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional") (tstamp 8d349b3c-f250-44f3-bc76-d2a1da7f8cc6))
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 2b8c78bf-b55c-4c7c-8b2c-112f65221e76)
    (at 141.8 43.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/17c7e2af-2bfe-4c77-b09a-49abbd35dac7")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 00f33fdd-d9b4-4c82-b08b-5f68d0ef4a95)
    )
    (fp_text value "33k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a0162259-22c4-4c58-9245-ed9cd713c1b7)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 8f7cb10f-0ba8-46e0-892b-cefd22bce67a)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7992c380-4104-4db2-8013-89729cae4a6c))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 605de9db-b621-4c9d-9d63-d49aaf8a79f9))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 40e1b7f6-b3d8-4c9c-b1db-4855ed6b8348))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 77a65bdd-b735-4709-95e6-336bb8676009))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 839f31d9-9b60-4020-979e-51666412a528))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bcc1653c-0071-4501-8236-f61eef746d86))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 73029300-7226-44e1-81d7-1571adead679))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 54b66cbd-4350-427d-823b-376a106af61c))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 63920efa-14b6-4f07-8ce8-dd21f123e54d))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2153e61c-a80e-467b-84ed-1f651c0bbb06))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 51 "M10") (pintype "passive") (tstamp e7f2faf3-bbc3-4550-b26f-1867407f4f3c))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 45 "Net-(Q7-B)") (pintype "passive") (tstamp ef89e5d0-90c8-40a8-b2db-bf2cb400182c))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp 3eeb062a-5715-4678-b751-928f010d2770)
    (at 96.8 64.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/3dd673c3-8cc3-4fce-a61c-238f44e125c2")
    (attr through_hole)
    (fp_text reference "N2" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 10324090-67b3-4f8b-8e66-c1a281d9f6ad)
    )
    (fp_text value "IN-14" (at -7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp d7250cfb-be25-4c30-82ea-182e63ea6022)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp d03bd75b-2f1b-4b93-b1cc-7ad8c2615adc))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 703a68dc-388e-468a-8592-381a3923ec72))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp ec78be3d-c18d-473a-b1db-e2478a04b45d))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp a7030654-99ea-497b-8279-03526692dc9a))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 616fc285-3aee-4425-895c-ac1f06a44011))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp f3033a58-4bd1-48b3-8bf9-b5fe0ca10180))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp 04351685-6a93-49f4-8d80-74aca9d43b8a))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 30 "A_H01") (pinfunction "A") (pintype "bidirectional") (tstamp c4936809-fd2f-41fa-b07f-415def71d9b9))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(N2-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional") (tstamp 93ad48ac-f707-4c9f-875e-8b074b1f237b))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp d94369cd-5612-434c-91e0-8c0cbe67cddf))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp ac6be136-4b7f-48b3-a063-051fd040e063))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp 29b884d8-80b1-4659-882d-7ca83b2ecf99))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp 9cc815e8-8f36-4b20-98f9-fb69905ea42f))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp 1fc9c568-304a-4f7d-a888-2848a22d58ef))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp bf912d3e-90ef-43a3-9379-b5b8101cdb5f))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp 35eff4b1-e70a-4a6b-9b7f-4bea676e690b))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp ad95269e-ebad-41b4-816f-313a3de8ba73))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 21 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp 4adfc86c-8b01-4e0a-a68e-273852171c56))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp 208ceaf6-960e-43dc-b6c6-9884d3a9974f))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(N2-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional") (tstamp 9f7568fc-aaae-4e27-a975-de8579f9ead8))
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp 434d8480-f234-4f68-81f1-fcb7f3498d21)
    (at 115.53 34.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/da133bcb-7ee6-47e8-9fcf-d9db21dff1e9")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0f7b5273-8f08-4ff9-ab7b-a0676572bf4c)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ada2ace-da25-455c-be2a-a9e88719d00f)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fcbe59b7-46db-415d-8d4d-9d4893d9cdb6)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 53289832-70fa-45af-b5b7-906b39324f84))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2e463caa-fcc8-43f3-8d7f-34acb74299e3))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6bfcb286-d752-4ba6-9d20-26cbdc57d4ac))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ef90cadb-bcb7-43ce-808b-83b4110ba565))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c06a66cf-a2bf-4680-8d5c-76933353aaa3))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6095e362-2e4a-4c43-961b-16c936480f8d))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c4f4ff87-06ac-4198-abac-a88536bdcc25))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 27446626-6c2e-4426-b454-a1f8f237d163))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d0a89d87-fbe5-418d-8f5d-41470df91638))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 84bb850b-a217-49aa-b94c-98ddac041c3f))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(Q2-C)") (pinfunction "C") (pintype "passive") (tstamp 0a3bb8a4-4617-46ab-a337-42e01e50dff6))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 36 "Net-(Q2-B)") (pinfunction "B") (pintype "input") (tstamp 8ad420b8-b108-4b1e-bda2-86b81fa79c48))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "HT") (pinfunction "E") (pintype "passive") (tstamp 12faeb6a-a508-4ec4-a0f9-7feaf4fee8bd))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp 44a6a605-b0d6-42fe-be15-5a1b4916cd40)
    (at 81.26 41.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0b056c6b-2d1a-4d51-ab37-01bb8d29d266")
    (attr through_hole)
    (fp_text reference "Q5" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 12f38216-5fc7-4a7f-8ad0-776073b49071)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b0ed92a5-bf60-4d67-8172-b1b3f8300a8f)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 714738e1-2b5f-4396-a05a-75e74201756c)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09afecbd-02b6-45a1-b810-061cbdd21fd4))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ad3c4331-1652-4bca-9c50-0c1dd7e2d5a7))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6fc77ba-4cc6-4c8f-bd48-a3ee7dbf2219))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 914498c4-dfa5-4341-a8f4-bfc1aaac0106))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a8977189-c847-4ec6-b455-484b638a72a4))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d0bca896-5fee-4202-959f-8832788e7ac5))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fd92ced9-d4c3-4573-b279-ee540fee4295))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ee6da1cf-ebc2-4e93-9229-d34741ff8d4c))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f7c510c9-7f86-4699-8a1c-9bad43bd7a6b))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fa94d2db-5fc9-4fe4-a766-3641ea7fade9))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(Q5-B)") (pinfunction "B") (pintype "input") (tstamp e9cc6ed5-0b75-4ede-8253-fba73bb0f5b6))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 42 "Net-(Q5-C)") (pinfunction "C") (pintype "passive") (tstamp d3e10bc7-5c2b-4f44-9d68-b2a515757734))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "E") (pintype "passive") (tstamp 2963a91a-23ba-46ee-8228-35d7b26cbef4))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp 495ac295-a08b-441b-9d36-c3399edf2412)
    (at 55.8 55.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 519c88f5-c417-46a1-ab09-ad223f8bff37)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e9d0148-2f7f-4583-9023-3437aba5dac3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6f6ebf08-e939-45c9-a4a8-4a4107b26f41)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 06f339d7-50c0-4602-bb31-dc7c61ae33c7))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 9b02427b-df53-4ec7-9eb6-46428f839448))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask") (tstamp 2dda3d03-b270-4d72-83c7-06e4912d6032))
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 53dc7a70-08d7-4782-8dfe-51bec0cc8da4)
    (at 74.8 33.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/7d5180f3-1588-49b5-9e1d-5c806166562f")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dbbc9ea2-f233-44c8-af9e-8837a92fcca0)
    )
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bd32c9fb-b833-4a92-a288-8d4968f73230)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 2ec40b71-f86e-48d1-b9b9-e46b798a0a1f)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 04fbdc1b-28cc-4d39-8d4d-2dd0ac0281f7))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 874b8db0-43ae-4a8a-88f0-1385d0cf62ad))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c09a2f93-af1c-495a-a12a-e5e19e90a1a9))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6f731572-b068-4a2e-a864-8a68dea63086))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dacf6cca-01cc-4792-9689-bc68049f5a6f))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a376bf4a-0e93-4a71-9466-b4cf92eec9f8))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 77f4d86e-d1c5-4c61-b720-dc8b805e1349))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ddad0417-9862-4550-868a-6126e852e96f))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5fdf96ba-4f3f-49fd-9e77-3fe967218ed8))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4ced76af-9a8d-4cb0-b569-f33b67e70535))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 34 "Net-(Q1-B)") (pintype "passive") (tstamp e7b458af-4378-43f2-b366-54f28c4ad0f5))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 10 "HT") (pintype "passive") (tstamp 82bdfe01-781f-4161-9258-870ee7ec2bc1))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 5eb426ba-c8f9-4a31-ac1e-0d9e29532100)
    (at 74.8 43.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/71c96234-fd80-422d-a5f7-c08e580d5673")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1f975e34-4887-477b-a388-202549136679)
    )
    (fp_text value "33k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bc8444de-db7f-4f01-827d-0510d02b8d70)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 8bcce116-b2ae-48ee-bb0c-816dd6519b8d)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c391498e-de13-48a9-8c3d-d75b91421f89))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a62f4050-7175-4b77-9e1c-79fd0a38551e))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d753f96e-6a14-4506-8270-25caea55abec))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ccda3c0f-e922-4810-9c3a-99a07e8a041d))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0ea280a1-6187-499b-82aa-7bdca943fbdf))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 21d9ba1a-aed6-40a9-aebb-66406a2c0993))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a02cc05a-8b4b-4651-bd14-8b92557f2efb))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c2cb327-8dd5-43a0-95d2-ca140271ab48))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b4a62374-16dd-4053-9a2b-eadd2f03ba6c))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae2d0401-3e46-4cd9-9359-c8523a3003d8))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 49 "H10") (pintype "passive") (tstamp 91543719-0b57-4328-aa8e-2d89d224bcfe))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 41 "Net-(Q5-B)") (pintype "passive") (tstamp c13e208d-7e17-411b-89d4-14a7f6628654))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp 635851a9-a24b-4278-beed-fe37664e46d3)
    (at 55.8 115.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 533b6270-ef72-4168-a135-07e9385184d8)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e4a28d3-f015-4209-85b2-8d4d3004d540)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 356ad0b8-706b-4ae7-bf83-2ed9b67ff507)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp bfceae83-813a-46e5-bd68-f2b474feea8b))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp cc5d37f8-159f-44e5-83a9-878d8863c119))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 01cf929e-46e5-4063-a2dd-25cb9e619b1d))
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 639ada5d-df11-4f65-95e2-e777747dca8c)
    (at 167.8 44.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/65ed49d1-b91d-4bcb-8c37-7c05504ef579")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c693698-bc3a-4081-a6bb-d9d51aff0e42)
    )
    (fp_text value "33k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ddc40eb0-abf2-401f-8aa5-a246406eb942)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 9127c6bd-56e7-4184-b4a5-0e14c94dd0cf)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 020d7c00-5f27-4d76-ab9f-55f52b421270))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58bc3a32-5c33-4aa0-803f-c4c3dc7c9a60))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp aea6c054-672c-4214-bc90-f016ca822e7e))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6fc971bc-e0e0-4a7f-a802-d5a36f0e728e))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp da568eee-31be-4c2e-9412-f20bbd28c406))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4ea43a72-143e-4901-8abb-6a7875180b18))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f94d53fd-3562-46e9-8672-ed357893f1e6))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8ca5c03d-503d-4246-91cc-64ae64f24bf8))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e71d38f7-f469-416b-a967-609d288fe24d))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b24d489b-fcb5-4339-babb-4b6ca3ec4a87))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 52 "M01") (pintype "passive") (tstamp ed17122c-c302-44d9-a02a-d3b5fda9e08a))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 47 "Net-(Q8-B)") (pintype "passive") (tstamp 2c97037c-dcc8-4545-872a-6868661137ad))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp 6838833d-d544-48e8-b235-052da2c5feb3)
    (at 81.26 33.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/9e23d8e5-2d36-445b-a30d-c426fbbc1edd")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5e906154-a1ea-4653-953b-bb9180eb8d41)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 265cbe0b-3b1f-4f8b-afae-cfb49184233a)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 16ab088a-cf58-4f66-b104-7c2863444074)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 616d0f06-7d07-4d4c-8c8d-902d2bc7ca50))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cf9e8448-b493-42a8-8f32-df2ca5bd518f))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 391a39ce-5d75-4a82-851b-6f988481a486))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d5cc1e85-3e07-4acb-b24e-6aff5f3fb9f7))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c3cf9c4e-c49f-4206-9114-a789eda28473))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp db410175-e6af-4165-a9de-eab56f5df476))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7cabbd57-def9-4d0d-8934-71d5798a0f41))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 10308090-eeed-4cee-8211-ffb2950cec7e))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 33d29d93-56f1-4669-b88e-15a27c0d0658))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9a97ea1a-301c-48ca-b18f-54020fc97ee9))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(Q1-C)") (pinfunction "C") (pintype "passive") (tstamp 7ff3a238-f2a4-4f99-9cf6-a841049d607e))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(Q1-B)") (pinfunction "B") (pintype "input") (tstamp 547d5d2c-5f94-44e5-a3a2-76fff02f7707))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "HT") (pinfunction "E") (pintype "passive") (tstamp 2ebd91d8-bd15-443e-91df-5af034ed0c2d))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 6b9fbe98-95fc-427e-a2cb-90e7697bcd2f)
    (at 110.07 39.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/62caa4ad-c636-4600-9a27-db169be6e93e")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2927dabe-73c4-4081-ba0b-35545f8bf064)
    )
    (fp_text value "470k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 76b8a4a6-4b34-4aac-9c1a-a0814e36b76d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 8c687d2c-9cb5-4297-8e89-bb2e7e802181)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 361e2790-bdf6-4e63-91a3-5dc1d1de8f70))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eda1acd8-4297-415c-bc00-2c337bd3ca60))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1b24011e-e8fe-4cbf-a4d6-0e49a9dc77c0))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0711266b-24f9-4be5-8d72-20681f7ece18))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 30d596a7-1d45-4f49-9207-0e7b7e06effc))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8d68e0c2-10e8-413d-aebc-9a9653a9428b))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cfe95862-806a-43f1-938c-b68dc15b1063))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b971314d-b465-4718-a0a6-db99c4d6c710))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a4c5cb0b-de8a-4e97-a667-4a3cc6761393))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8a351858-4058-44c5-9005-ded49f0301af))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 44 "Net-(Q6-C)") (pintype "passive") (tstamp a1061d5d-23c3-4862-b094-cf3a3611442b))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 36 "Net-(Q2-B)") (pintype "passive") (tstamp a642cdd3-b09a-4086-874c-d32eef751ae0))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 6d1246eb-4d83-4c43-a8d3-7cda15da09d6)
    (at 181.07 34.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/8efa8390-0fb2-43f9-a2ff-1010f64758ea")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 84ca6486-0a3f-492f-bc71-a03f814f5cbc)
    )
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c0a745f4-96ea-4c2a-8926-22e81d2dd4ab)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp b7820043-0de2-4067-ad06-4257dbaedba7)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c1215d2-ebf1-4a1e-b9f9-4dc6819138f4))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8715f6ec-e9b4-4ee6-9de0-8260bc970290))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 703acbaa-5c09-4144-817b-c0eed3a48b40))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d40105b8-7716-496d-ab75-c7ddd7cdea76))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7c00a124-c1aa-4979-ac63-58e04e5badaa))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6d3cebf1-987a-4af2-969c-246dd18da2c3))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 493c487a-f0aa-4fc7-8d81-de9a84e6fa89))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5f76086-00cb-4341-856c-cd4cf082c8e2))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bddf536d-f2bd-403a-943c-08d16f20ceed))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 45a1e2e7-7572-4bdc-b906-c541d5522daa))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 24 "A_M01") (pintype "passive") (tstamp e572440e-7c9c-44b5-ac75-b9819a967c2c))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 39 "Net-(Q4-C)") (pintype "passive") (tstamp 3a88feb8-e9f0-4728-a7e4-7a7809619d3b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 711ca88d-9260-4393-8e18-8006446fbe55)
    (at 110.07 34.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/51fa228e-dbad-466e-96ff-110ef72a8038")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 28ddfc0a-3597-4fcb-878e-8eb993586d43)
    )
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b72efe5f-4558-4912-8d20-033454601ae5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp e87683f2-3b72-4696-afe7-6d46f2c77560)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e759023a-4685-43a0-8a11-f053d8c4e1cb))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6200231f-dd8d-4bad-a02a-dd4c396bddbd))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f6853d57-faff-408a-a4e0-966e75c94e0c))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8ca559c5-5bd1-45a1-b6d8-bd51b7f7cdda))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cf976696-d81f-4f48-b4c3-3051602049a3))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 280e8a17-ac77-47ce-bc88-1a0bd07a8698))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9902a61a-9533-4510-ba5d-3f9a9e3a3e27))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 548efa3f-038f-4b6d-82f2-114acfb3825a))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f7d2bd0a-028b-48c4-8267-39896682baa6))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b5b90f0d-b92f-4292-84d0-511849875f8d))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 36 "Net-(Q2-B)") (pintype "passive") (tstamp dc9cd572-3d85-4293-ab92-2ddd6ae3461a))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 10 "HT") (pintype "passive") (tstamp a54d5634-80ea-4015-89e5-809b3769c9c4))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp 7932480f-f178-40dd-bf4a-be22beb56155)
    (at 127.8 64.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/43b1aa7c-f1cb-4972-a401-0455ef625bf1")
    (attr through_hole)
    (fp_text reference "N3" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 097c249e-02bd-4091-ba68-fa55fc37ff78)
    )
    (fp_text value "IN-14" (at -7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 3b0d44c5-8c9b-4e90-9a6c-10b9a8d5e744)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp be880c23-599e-480b-a93b-4c3a88255d14))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 51d080bb-aaac-49c5-9d88-01ebcc2d1e01))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 6d71597f-0ec8-4dde-98ab-fcb58b1dc6ec))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp eb06818e-d013-4af4-bde0-33a3ebea168c))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 4b93775e-4909-4d99-9e70-2de9d0d44734))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp 21a45617-4ecb-442a-bfb1-3e9a6bf6d7e2))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp 9d7b24fe-5804-4f2a-b6c0-a69215a63274))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "A_M10") (pinfunction "A") (pintype "bidirectional") (tstamp 8d4ece43-742b-407d-b2d9-6b5a420ba62c))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(N3-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional") (tstamp c3bd0778-1275-4823-98a1-e22e21c823ae))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp cc0171c3-016d-48e1-9024-219ad7018ae9))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp 0c5b2d4e-3e38-4070-9275-0dea1b1f479c))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp c0f5d293-2f73-4902-8bcc-750b23e83be1))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp 124fdfa0-6672-44b5-aa03-b62695b1bcfd))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp 38e660c3-2718-4bc4-8c01-a34157c4fda3))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp e46f168b-a326-4ac0-8553-8512753cec6f))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp 556e3e8c-e255-4838-b377-94b316f65fba))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp 58d1a8ce-0033-439d-bd09-736c9106454b))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 21 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp ed21e153-777a-4513-be6f-0d089b6cbd2e))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp e6d34676-80d9-433f-a45e-809d0b3a7752))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(N3-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional") (tstamp 6b333e23-7531-46dd-ad4f-5e9ad103782a))
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp 9bda447d-0157-4877-b982-da3bb79f08e8)
    (at 110.07 44.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/d18c936c-3c06-4302-98e7-e7cd267f3d01")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 544987bd-f561-48b6-b5d8-2f94e9a171ce)
    )
    (fp_text value "33k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92ed2bb0-ea2e-415a-a44b-c77670862931)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp b06f90c9-b944-4583-a58e-e3279abc2474)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5100dacb-7363-458b-a225-e205d7c47a46))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42300a70-beaf-45d5-a548-d2fb939339a6))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a66772ea-0c5e-40c8-a1e0-8504040830dc))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1d9bc05a-baca-4312-8531-f1df3bf98753))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 15155d10-420a-4e4f-8129-50b4ecba34e6))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2fc70ddc-9edb-45a0-9c25-4b32ad2183e7))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7a960b33-1fab-44fb-888c-121a57e44fa8))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bcfc0b11-641f-4787-b658-da13ae67774a))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 68d2dbac-8e18-4470-a92e-e455ae415d98))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 65254cd9-1f73-4153-a422-e28026b03254))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 50 "H01") (pintype "passive") (tstamp c1eda21f-a738-44b7-892b-82f870e78be4))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 43 "Net-(Q6-B)") (pintype "passive") (tstamp 0bf2defe-9eb2-4ea0-874a-c4a13724dcc5))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp a62ed3d5-9ed1-405f-a316-4b3a54d7f90c)
    (at 148.8 43.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0abfce8a-f9c6-4bad-8628-7b58d1307e9a")
    (attr through_hole)
    (fp_text reference "Q7" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d562b432-f7f3-4eaf-b48a-20bf5f5f7443)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6687afd2-9105-4e04-b026-1be3df7171b6)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5c09635c-11f2-4fc8-9b93-b7116ad1fe7d)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 30f68073-06ed-4eb6-8b7c-86854dc4eec4))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f3dc1acf-fd71-4312-9868-6c11f2b29299))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 17e9fdf3-577c-4aa5-b265-1f26b7b2bf1a))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0cf46e6e-1b7a-47cb-b1f3-11807c4048ff))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3c7bd944-0a85-4895-a371-9842ea34a4a4))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 77ee693b-23da-4912-ba8c-54c9aee02936))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 73e2fd86-6f39-4f13-a80f-677ab6693318))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2459959e-c07e-41d9-8485-758d57f3131b))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb50c6b6-200a-4f2e-b88b-f6a93e9c4373))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ad1c6986-82d3-4b1c-a21b-9d8c58858c18))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(Q7-B)") (pinfunction "B") (pintype "input") (tstamp 2cd2f477-2244-43a3-986a-7f2564a12940))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(Q7-C)") (pinfunction "C") (pintype "passive") (tstamp ab4acb68-4c28-4124-9542-2eb75b336d2f))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "E") (pintype "passive") (tstamp c4e8e300-d34b-4312-9e97-316c612a6fcf))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp a696e630-6652-4fa8-86cb-89b1fa16f8b1)
    (at 89.8 33.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/155d6e0f-1301-43d6-968c-e4defe42f7c1")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9a77423c-da8f-4594-af48-a801e7b9f59a)
    )
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6b9a8648-0188-46ca-8734-34e828b1b0dd)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 270d3245-6657-4ffa-8b9d-7ef4d88e8f72)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e038fbfe-889b-450c-8ae1-5a5f21487bb2))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d7000a26-48e3-4c68-aad5-9d184798d125))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4efb655c-ef78-4b1b-9ce0-216d1da9ab4e))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 61ed0e11-092f-4298-abe0-cd224ce9afdb))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 63ee1ee1-3328-41c3-9adc-ba181655a891))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 073beb25-3116-4e79-81df-bc94bcb8e419))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp afc3906f-286f-40fb-93d2-12b7f59b8f34))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e84dc148-3361-4618-9f00-a47ffa60ac3b))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 09705f0a-6013-45cc-8f42-9ae4180b6009))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eb6de761-de45-4a0c-91ac-ccbe35a374cb))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 27 "A_H10") (pintype "passive") (tstamp b1fa4310-15be-4364-917a-06ef35959b34))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 33 "Net-(Q1-C)") (pintype "passive") (tstamp 887d4b98-420f-4290-b65b-90ee1343f81b))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp a9f27c33-0991-4201-b70c-3a98853bc38e)
    (at 115.53 42.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0d98cd7b-3337-4399-94be-20b9758f36b3")
    (attr through_hole)
    (fp_text reference "Q6" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f976b81e-5aaf-481f-ae12-5312bba53f4c)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 969d627e-6013-433b-972f-d009f4814a7a)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d1e31291-31ca-4cc1-9396-e2931b8bfad3)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8a897d1c-3b12-44cb-be99-8290c4e6a1d5))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 53464699-6dbd-42e6-a71f-da8ad7b636a9))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4b06393f-d210-4356-9001-eb18fbb708b7))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c6ebc824-fa87-4faf-b1a5-a21a70bf23cf))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b4e2221f-db47-4406-a4c5-bf846112914f))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp eadd5fd9-5430-4ffa-ba26-fa06aea949cb))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a7c3fc9-32cc-4c45-a7a3-a0b75d39f9ed))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1aff3309-9fa8-458d-96cf-39cd1fd804b1))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e07cc84-202f-4b92-b079-606b2779b540))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a4e734c5-e69d-4499-9122-106a52d822e8))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(Q6-B)") (pinfunction "B") (pintype "input") (tstamp 88b9b0b2-b0a7-4d19-9c26-e2f585be21c8))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 44 "Net-(Q6-C)") (pinfunction "C") (pintype "passive") (tstamp a0e6f014-0080-4a52-880c-35891a06227c))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "E") (pintype "passive") (tstamp 6573b64a-6025-43e1-892b-c3b72fe79b79))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-16_W7.62mm_LongPads" (layer "F.Cu")
    (tstamp b1b0a109-64ef-4db2-92cc-9b6c66f60b0c)
    (at 138.42 112.88 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/a41e7841-5907-44d7-b827-ec3e7cbcf2b0")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 59ce0b63-3829-43c7-8552-617817b74246)
    )
    (fp_text value "74141" (at 3.81 20.11) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 33f54382-2d0e-437e-9105-8281e33c48cc)
    )
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 849ca24e-e0c2-420a-bd8d-d096e871e3d8)
    )
    (fp_line (start 1.56 -1.33) (end 1.56 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d0fbf506-3d5f-4ddf-83c5-d6249de4c067))
    (fp_line (start 1.56 19.11) (end 6.06 19.11)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fc5b2b52-a2f1-4345-a3a0-aa2059fe42b0))
    (fp_line (start 2.81 -1.33) (end 1.56 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 38206cd2-b832-4461-99dc-27d1c6a9f383))
    (fp_line (start 6.06 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 16439285-ebc4-4f13-a69e-3308b9e79984))
    (fp_line (start 6.06 19.11) (end 6.06 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 66218cba-9f86-432e-957a-54dc022e5299))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85632a91-1154-4cd4-bdfb-e403658a1cf1))
    (fp_line (start -1.45 -1.55) (end -1.45 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b74c657c-548c-4e1a-8b6f-c693f4b7a088))
    (fp_line (start -1.45 19.3) (end 9.1 19.3)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d9cfc870-bea1-4537-9c86-3c3e8d6ded8c))
    (fp_line (start 9.1 -1.55) (end -1.45 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c360f048-04d3-4e06-b1fc-85f73678fc7a))
    (fp_line (start 9.1 19.3) (end 9.1 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e608bae3-9ded-4aae-a309-51e51a354e39))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1be21fe5-366e-48b6-aa44-6a986ac48210))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f2072096-830c-4773-acde-4a8bafa58129))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5a77b1b-e867-4106-92b5-bea0c2a45092))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8567d546-fb9c-482f-9775-5eea3f14c7f3))
    (fp_line (start 6.985 19.05) (end 0.635 19.05)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c5cea7dc-1d1b-47d5-b3a9-70455078ff74))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K8") (pinfunction "~{Q8}") (pintype "open_collector") (tstamp 4855e9a2-e2f0-41ff-ae8a-f40081322fa0))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K9") (pinfunction "~{Q9}") (pintype "open_collector") (tstamp 18173ddb-acd6-41d2-ad7b-67cb1c0cca0e))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "BCD1") (pinfunction "A") (pintype "input") (tstamp 17d7d190-0f28-41de-8f4d-cf2de173d3e6))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "BCD4") (pinfunction "D") (pintype "input") (tstamp 0e7efcff-48cb-4876-95cc-785b01b9e48f))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "VCC") (pintype "power_in") (tstamp a349411b-2651-4b6c-aec1-13a15d23fa27))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "BCD2") (pinfunction "B") (pintype "input") (tstamp 3bd6c29b-d8a3-4180-9a61-c65ebf7dd1a4))
    (pad "7" thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "BCD3") (pinfunction "C") (pintype "input") (tstamp 3f25bba7-26b3-4a6f-b1a4-af61fe09efb0))
    (pad "8" thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "/Horloge Nixie/K2") (pinfunction "~{Q2}") (pintype "open_collector") (tstamp 9ceb8493-885d-4eb8-bd38-9954d24f644d))
    (pad "9" thru_hole oval (at 7.62 17.78 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "/Horloge Nixie/K3") (pinfunction "~{Q3}") (pintype "open_collector") (tstamp adeb6873-e6b6-4738-8b07-495eb2485e36))
    (pad "10" thru_hole oval (at 7.62 15.24 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K7") (pinfunction "~{Q7}") (pintype "open_collector") (tstamp 624d692f-9d74-4986-b29c-322be6dd18d4))
    (pad "11" thru_hole oval (at 7.62 12.7 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K6") (pinfunction "~{Q6}") (pintype "open_collector") (tstamp 4138fbd9-1299-4b41-97e4-066c5ba10d9e))
    (pad "12" thru_hole oval (at 7.62 10.16 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in") (tstamp b46473e5-3f0d-4f3e-83f8-a934ca850d16))
    (pad "13" thru_hole oval (at 7.62 7.62 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K4") (pinfunction "~{Q4}") (pintype "open_collector") (tstamp da503f6c-a5b6-4ab2-8d6a-3deb764e2edb))
    (pad "14" thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K5") (pinfunction "~{Q5}") (pintype "open_collector") (tstamp 7bf7e805-f7ec-490d-b259-dc12d895e35c))
    (pad "15" thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "/Horloge Nixie/K1") (pinfunction "~{Q1}") (pintype "open_collector") (tstamp 4c3a0609-759e-4293-ae51-02179c5bcf00))
    (pad "16" thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K0") (pinfunction "~{Q0}") (pintype "open_collector") (tstamp 3b403bce-9825-40ac-bdcb-e69ee0763ab2))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp b205df96-ea0b-4e24-a668-c5e9e52b38f6)
    (at 141.8 38.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/923ecead-61b5-44e2-a663-efdc3bd79964")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f79ae6f-265c-4a29-8cd9-16714f00905e)
    )
    (fp_text value "470k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3e89a28c-100e-48b7-a210-b003663aab98)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 06755384-5971-4959-90ac-65c0314348e6)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff123b5f-473f-49dd-83e9-c525e2ec87ed))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b63fc7cb-4393-4117-b81b-66120abcd772))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e68e2f99-877e-4c3c-a1a8-989bafa3a3cc))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0a9fb40d-26ef-4718-b817-c7caeff47a30))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6d012365-17a1-4a9a-814d-b9ba3bccf0c0))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 679b26b9-15c1-47d3-aca5-af34a121ceb1))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3fd6e65a-070c-4b8a-b590-5fb11396d060))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6dc61d24-a742-4d16-a7ee-a70488fffea6))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a261680e-9fbb-44bb-95c9-f3e4ffe58a26))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4fbe2781-76a2-42bc-9d59-72d6d94b3735))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 46 "Net-(Q7-C)") (pintype "passive") (tstamp 1659b243-c46f-47a8-a063-b1361abc1e58))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 38 "Net-(Q3-B)") (pintype "passive") (tstamp 5cd5382e-76eb-46c8-89da-97a7aac565f4))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp bb3a9a90-62b3-46d2-a210-7dac0d45138a)
    (at 53.26 88.8 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/72e95360-3d9d-4402-abf9-895236b95029")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 70752f55-bfc9-48f4-bd9d-7db199b9ec9d)
    )
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b10e1e9a-fcba-467a-b811-06875d132306)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 52215d53-0dc6-4605-8450-762466b61cbd)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b1b4291-16d4-4cca-a4d3-1d9ec0771697))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2a58e9b-5528-44d0-b392-30d37495722a))
    (fp_line (start -1.33 1.27) (end -1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cbec1778-9032-4633-9f28-7a56dd1dfd65))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 93623db6-e95c-4673-af5e-892a1be4e36d))
    (fp_line (start -1.33 8.95) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49d43b9c-a3ad-45d4-8a0c-1ee398bfb42f))
    (fp_line (start 1.33 1.27) (end 1.33 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b14a0b96-1238-46f7-88d0-d23a8d3a301c))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 35d33e7a-9203-4cb2-b524-60540879569d))
    (fp_line (start -1.8 9.4) (end 1.8 9.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 139dc40b-6834-48d2-92c2-1351451990cf))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp becc6221-8c66-4f84-91ea-578345753339))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c2006f3c-1027-4c7a-816c-9a159281f23c))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c5dc199d-8e46-45be-98dc-544df9ea176f))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d50b6582-fe55-41e8-93d0-5556222a469d))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 950ec52d-53e9-4a7c-9848-dd74435727f3))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 90c8f29c-b01e-4589-a695-a18abc5fca8e))
    (fp_line (start 1.27 8.89) (end -1.27 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3891fb5d-9864-442c-8401-d7829fa70315))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/Horloge Nixie/I2C_SCL") (pinfunction "Pin_1") (pintype "passive") (tstamp bec8cc33-c276-48cf-9ba7-d9e345826c7a))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/Horloge Nixie/I2C_SDA") (pinfunction "Pin_2") (pintype "passive") (tstamp 622b79ed-1d88-4e64-a984-821a11ce0c74))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_3") (pintype "passive") (tstamp 366f42ac-cd63-45d6-8b63-c54416a6cc2a))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(J2-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 28667c45-610f-4fc0-9929-023c20a86a48))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp bb58b852-c618-4bcd-a3a0-cacbdb60026c)
    (at 174.8 70.18)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/4b33c1bb-b6ce-41da-b1a7-444dddb36773")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 00cd04d5-59a4-4c33-a781-bfd09006428e)
    )
    (fp_text value "Conn_01x05" (at 0 12.49) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d459f446-3194-43ec-a20d-f45b8a369b4b)
    )
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 714c682a-0692-4818-b6de-95279e270b1a)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dca9705a-221c-4f17-b442-cb7cb4da4b52))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e3d7de0-1e32-4e77-aca8-82544dfee32c))
    (fp_line (start -1.33 1.27) (end -1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b5974f72-bac1-4f63-8370-55323e17409a))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0d683518-7104-41e7-968e-f0879e121b49))
    (fp_line (start -1.33 11.49) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8496c53-d355-4fdd-bc8d-f60b2595bf3c))
    (fp_line (start 1.33 1.27) (end 1.33 11.49)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51902860-16ef-4e43-81c0-9ceb9feb6030))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 137ad572-2fb1-45bd-90fc-392027a00e5e))
    (fp_line (start -1.8 11.95) (end 1.8 11.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b5368c0a-4b02-448b-b486-e95e24a6d473))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 62821abf-0dbb-4529-9d22-f288e1447746))
    (fp_line (start 1.8 11.95) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1c12d257-7b3a-4e83-9906-e7b9cc955c9e))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 379e67b7-6812-4976-a7f5-08303d981c98))
    (fp_line (start -1.27 11.43) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 758139cf-a112-46ba-95c6-c3d22f9fc5a7))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60513073-84a5-4331-8a9d-e3ab7cf7146c))
    (fp_line (start 1.27 -1.27) (end 1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2c017a2-5d8c-46c2-a0ff-bca0e5fc3cb4))
    (fp_line (start 1.27 11.43) (end -1.27 11.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ac805b0a-5456-44ea-aeba-b33282790886))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive") (tstamp dc32fddc-487a-4012-8fe0-9d8f63120aeb))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp db9b3b85-09c3-4ee8-9cd3-ae1e93937a5c))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp 96cbf9ce-3d71-4f64-8251-d49955ea6b52))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_4") (pintype "passive") (tstamp 59283e9e-f267-4378-b23e-7d2babc02f21))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "HT") (pinfunction "Pin_5") (pintype "passive") (tstamp 8f7ab84e-4b34-4df4-9abb-8b5ab402214d))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp bd456dc9-c376-412a-a00b-7fcf3f347c54)
    (at 157.8 33.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/9d76a504-3fd0-4fc2-8167-bdce7a5fa0bd")
    (attr smd)
    (fp_text reference "R7" (at 0 -2) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 433424d1-47c3-43d6-ae3b-f9b8cfc81aa0)
    )
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ab4192bf-3efe-46db-aeca-e7db8b366fa4)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp c53a5b77-6d02-4af1-8f05-bcfe8578c654)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 11c0ab6d-2567-49eb-848d-1558c18b4834))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 730fd5d7-fd51-4a4f-bd2d-2fdf52fa4434))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c0ec45af-74d2-4199-8831-9bb35399fe14))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bc091514-9f9b-4149-beb6-3e2403717fff))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp be41381e-80d3-4d82-b661-e96bb64b26d1))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 178a3b1b-a82c-4afb-a612-a2cf4309f39b))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 57b3e37e-fc52-405e-b05b-54aa6ad57e39))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2433d2ed-d86c-4ae4-8c7b-e61524d90797))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ecbff061-bca0-46c7-973a-ea664dae2084))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 33ca5143-313a-4f7f-b549-d01e937393f8))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 11 "A_M10") (pintype "passive") (tstamp b84949fa-a697-4e6a-ad92-47d33b6648d6))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 37 "Net-(Q3-C)") (pintype "passive") (tstamp ef7215f3-998a-454f-8155-e754d20d1567))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp c15f3874-a7d6-439b-9c96-5880c73087c7)
    (at 148.8 35.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/e5514aba-40cd-4d04-aaa7-a34b84f957ee")
    (attr through_hole)
    (fp_text reference "Q3" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b784cc06-8ecd-4a31-a6aa-b46c56e7196b)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 087d06cd-1b2c-4b46-a7bc-19f8f6b49ac9)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4a1239df-a632-4a9b-89f3-a451480538d5)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 93e7596a-3737-4643-a059-4fa3b28d45a3))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp acb85e26-6923-4498-9e5b-b807d2212a90))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3463de27-44dd-4980-81ae-2b98accac2f9))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 72334eb9-8a6d-4ed7-aa15-769257dddc37))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f17a9ce6-94c3-47ca-92f7-838448af1692))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ab538e3a-34aa-4a9b-9353-ace7cb8902b0))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c57f7808-9721-4a2b-9e00-3d6edaa9a7e3))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8a9efffa-7777-4bc3-9341-cfdddef66821))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 17e4693b-f230-4252-b7af-456720090f4e))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60586388-f5d6-4cd1-a744-dd4db7fbe46f))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(Q3-C)") (pinfunction "C") (pintype "passive") (tstamp 086760e6-6829-4807-8f06-7a1724185bd1))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(Q3-B)") (pinfunction "B") (pintype "input") (tstamp 8eb37062-be9b-4093-93e0-e97961122cd6))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "HT") (pinfunction "E") (pintype "passive") (tstamp 1d7685f5-14c2-4e25-b053-52445b36ce31))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp c3c1260a-60cb-4959-b392-ce2cf246a9d8)
    (at 74.8 38.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/04f454e1-55c5-49cc-a367-284659379cdf")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19a16410-63d2-43c6-8069-1b9cf33d1b70)
    )
    (fp_text value "470k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6677299e-6270-4ed8-832c-0fa26cc1bdd2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp d20a77e1-f873-41ed-ba35-792747ae2cbe)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0477633a-68ca-4065-9ef4-b8e752483b6b))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9731213-1bb8-4f5e-be70-718d5001952e))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fef26f0f-a30e-4bc4-8409-3543a1a3841b))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c7b94d8d-4f34-49c9-baff-255829f20986))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a32ac3ad-7b9d-481c-b5bc-87a014062b62))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 223c4ba4-be0c-40c4-9900-346556cb79a0))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c9e2401b-2614-4154-89bd-7b3d3420aa3a))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b6d20e3-1013-4223-984d-4642eb398788))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4e94435b-1918-46d0-962c-42a8d23f316f))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a220b67f-9306-496a-9a33-5c119585f52e))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 42 "Net-(Q5-C)") (pintype "passive") (tstamp 4d7e6776-d356-42be-bbc1-bbb1cd4486be))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 34 "Net-(Q1-B)") (pintype "passive") (tstamp e32106bf-9463-4890-96d9-0beff16a7963))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp c990840f-a9bb-4807-9e6b-124f2f53d4f8)
    (at 172.53 34.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/123d2b82-2043-4b75-83d5-5f1b4ddd38ce")
    (attr through_hole)
    (fp_text reference "Q4" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5cb6ae6d-833f-4fb9-8a8e-d300aecdca72)
    )
    (fp_text value "MPSA92" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 09d260c9-a394-48a0-a5b9-4e5a34c1e78b)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2a3354f-3fc9-4945-850a-84f48d4e279c)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 560309e7-0b28-4525-9977-2804da58489c))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c17490f-5daf-4a55-9d44-1ca7d5e66dad))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 14a56a94-a246-4a8a-b4a2-e19033e99035))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 58f93337-ebd4-487c-9f5a-82f32f2db5a7))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 03492c5b-c13f-4b31-9a98-64df669e41d0))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 76e5159b-5eaf-47b6-a7a2-6ea9debefe9e))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d3101b90-1215-48d6-a2c1-1a61c9fe9850))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d5bb1030-c4b5-4b73-91f0-6dfad51e35f2))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76f5ba59-615f-4af6-bbc1-3c458e591c19))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0679ed5d-8a64-4f26-8bc2-3b23a89fc7ed))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(Q4-C)") (pinfunction "C") (pintype "passive") (tstamp 5137a659-d94d-4822-b21e-1a7a594af7c8))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 40 "Net-(Q4-B)") (pinfunction "B") (pintype "input") (tstamp 1775aada-8d37-4c45-9dd2-7237723ca875))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "HT") (pinfunction "E") (pintype "passive") (tstamp f38c8e90-2119-49f1-bd27-76b74065a2ee))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp cfa2f940-08d4-4a1b-a579-a7ce4898d68b)
    (at 125.8 34.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/3dfc8938-fa1a-44c3-b4b3-6529b421aa3e")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 567009ff-e7ee-4b5c-a1bd-75d260907e78)
    )
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 60120e64-a1a6-45a4-bea1-4404a1f45989)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 58baf85c-fb87-4913-a56e-a9951cf1e1ec)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f7bea74c-d9c5-41de-991e-f307409dfd16))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2d2abb87-ba7c-432c-a30e-aaff67c66d20))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1a9fa327-8fd2-413e-8b15-3ec4c7880f3a))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5a5cc71a-9782-4cd7-b68f-fcd58d2d8fd5))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9388fc8d-8ce6-44ef-901a-748064ff53ff))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 885da296-a217-419c-9ebc-d6eeac6c5d50))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 20837781-58e4-46ef-aaae-42788c2f51c2))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56c81048-42c3-4aee-9486-0a09998995cf))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0c6a9fbd-2bfe-44ba-8bd7-a47f7f9f6bbc))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 13d0ac79-7b3a-411a-8896-288bb4785da8))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 30 "A_H01") (pintype "passive") (tstamp 3bc604b0-c33d-4419-a4ed-6caf0ee058ab))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 35 "Net-(Q2-C)") (pintype "passive") (tstamp 2a008e6d-0c61-4448-adc1-524208a595ec))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Kicad-VFD-Nixies-master:IN-14-mod" (layer "F.Cu")
    (tstamp d5cedd4a-057e-4e57-b6c3-c6b862405d13)
    (at 72.8 64.8)
    (descr "IN-14 Nixie")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/e0bf8b4e-aad5-4810-9aac-c49f5c94e72b")
    (attr through_hole)
    (fp_text reference "N1" (at 7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp 209b85d7-e9f6-461c-b7b6-55d6997f8097)
    )
    (fp_text value "IN-14" (at -7.62 8.89) (layer "F.SilkS")
        (effects (font (size 1.524 1.524) (thickness 0.15)))
      (tstamp f2a34446-47e6-49af-a236-8f89ae1e09bc)
    )
    (fp_line (start -1.27 -2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 9d97f449-2d63-4369-98d9-90b3d342a738))
    (fp_line (start 0 -3.81) (end -1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 64322000-e1d6-4fad-b33f-32d2b6ca0231))
    (fp_line (start 0 -3.81) (end 0 2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 70a85e9e-e0c3-47fe-af7d-4aa6365ee4c9))
    (fp_line (start 0 -3.81) (end 1.27 -2.54)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 5a858262-8de6-4d01-a158-c86a6110ab1e))
    (fp_line (start 0 2.54) (end 0 -3.81)
      (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 479f6540-1bcd-424e-a10a-6dce74d7b299))
    (fp_arc (start -8 0) (mid 0 -8) (end 8 0)
      (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp aa196e35-3bc3-4e20-81c9-7de6dd3b5087))
    (fp_circle (center 0 0) (end 9.0553 0)
      (stroke (width 0.127) (type solid)) (fill none) (layer "F.SilkS") (tstamp d5f09ad2-c6db-4272-8577-9af1a0c486f8))
    (pad "1" thru_hole circle (at 0 -6.477) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 27 "A_H10") (pinfunction "A") (pintype "bidirectional") (tstamp dd9c3a36-1529-4dde-a2c9-9fa40b0a1446))
    (pad "2" thru_hole circle (at 3.104 -5.752) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(N1-RHDP-Pad2)") (pinfunction "RHDP") (pintype "bidirectional") (tstamp b4099377-6270-405b-98bb-5c032996bba6))
    (pad "3" thru_hole circle (at 5.232 -3.973) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "/Horloge Nixie/K0") (pinfunction "0") (pintype "bidirectional") (tstamp 3373e10f-a646-4885-abbb-a6abc5ea8ad3))
    (pad "4" thru_hole circle (at 6.393 -1.307) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "/Horloge Nixie/K9") (pinfunction "9") (pintype "bidirectional") (tstamp 69e0dc36-701d-4ef6-9c32-d9a1378e638e))
    (pad "5" thru_hole circle (at 6.089 2.063) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "/Horloge Nixie/K8") (pinfunction "8") (pintype "bidirectional") (tstamp ee90043d-9b41-4824-949e-c565e62608d9))
    (pad "6" thru_hole circle (at 4.469 4.594) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 16 "/Horloge Nixie/K7") (pinfunction "7") (pintype "bidirectional") (tstamp 72a03f17-e63a-4f94-b707-bf05f0d492d6))
    (pad "7" thru_hole circle (at 1.822 6.213 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 17 "/Horloge Nixie/K6") (pinfunction "6") (pintype "bidirectional") (tstamp 1ed60726-78bd-4158-90c8-302c30588bb9))
    (pad "8" thru_hole circle (at -1.621 6.243 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 18 "/Horloge Nixie/K5") (pinfunction "5") (pintype "bidirectional") (tstamp 032efb9b-ff51-4126-9c3e-80ee72b68f70))
    (pad "9" thru_hole circle (at -4.348 4.846) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 19 "/Horloge Nixie/K4") (pinfunction "4") (pintype "bidirectional") (tstamp f74e7a27-72e1-4c9b-a124-453eb027514b))
    (pad "10" thru_hole circle (at -6.12 2.154) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 20 "/Horloge Nixie/K3") (pinfunction "3") (pintype "bidirectional") (tstamp 9163fd52-a6b3-455b-9766-8bd53bca8d2b))
    (pad "11" thru_hole circle (at -6.35 -1.27) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 21 "/Horloge Nixie/K2") (pinfunction "2") (pintype "bidirectional") (tstamp d44cc0c5-4e3c-48f2-9f6b-4044ad4e436d))
    (pad "12" thru_hole circle (at -5.08 -3.937) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "/Horloge Nixie/K1") (pinfunction "1") (pintype "bidirectional") (tstamp b64e4493-d871-41be-bda0-11664e574273))
    (pad "13" thru_hole circle (at -2.978 -5.725) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(N1-LHDP-Pad13)") (pinfunction "LHDP") (pintype "bidirectional") (tstamp 50c16e38-f002-49a6-8453-652b0c5bc8eb))
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp e5145a11-47fd-4c1c-86a3-3ef857374ff3)
    (at 167.07 34.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/f8a24ec2-4c2e-4169-ae3e-69c8f18a80cc")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2193ca56-6e3f-422f-9846-52b3b7ed411a)
    )
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7758c925-d82f-465b-bc9f-fbed944bb72f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 6cff34bf-032f-4281-9525-9ed2b6c2d388)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 72fafd44-cb71-465e-b19e-20452202de07))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b08b0b8a-2c09-459f-a506-e98a79ba8531))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp af9ed0a3-79f9-43ad-9706-b584c429841d))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp db110803-f483-4415-badd-a36ac32609a1))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp bcd0ce03-c9cc-4dcc-bf9c-f34a4d729f27))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9d18f8eb-43cf-4b60-ad90-355694bee45c))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 20f96f8c-51cc-4794-90db-e8e8e6c87219))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp af5a9e52-f54c-4d05-b180-09fb38b369ce))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 426e95bb-75be-4639-ba03-58abf80cac56))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7f635922-b79a-4626-918e-3361c1d52583))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 40 "Net-(Q4-B)") (pintype "passive") (tstamp bb8ca444-691b-4c38-92ee-bd617fc61259))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 10 "HT") (pintype "passive") (tstamp d47f467b-7a41-443e-bfdf-a8422d92c9c1))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "PCM_Espressif:ESP32-S3-DevKitC_Laurent" (layer "F.Cu")
    (tstamp e8f53336-f180-4bc1-833d-9b56be6103ef)
    (at 119.14 91.4 -90)
    (descr "ESP32-S3 general-purpose development board, based on ESP32-S3-WROOM-1 or ESP32-S3-WROOM-1U,It has all the ESP32-S3 pins exposed and is easy to connect and use.")
    (tags "ESP32-S3")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "ESP32-S3-DevKitC")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/2dc24073-c3ed-4178-abef-7de8f85194b1")
    (attr through_hole)
    (fp_text reference "U2" (at 12.7 -2.1 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0698edf9-375d-4481-a421-b42b2fa323a7)
    )
    (fp_text value "ESP32-S3-DevKitC" (at 11.42632 29.46128) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 69e2f3e8-0c83-4ef4-bdfe-2d803f126cb5)
    )
    (fp_text user "GPIO48" (at 24.13 38.1 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 0214e6e0-8ffc-411c-9d79-259db52c1a6f)
    )
    (fp_text user "GPIO14" (at 1.27 48.26 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 048e7cac-52b7-4619-ae58-e1e5ac69b1b5)
    )
    (fp_text user "GPIO20" (at 24.13 45.72 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 0cd7a7d1-d206-4a94-97a5-c908d07592e5)
    )
    (fp_text user "GPIO3" (at 1.27 30.48 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 0e1094b6-53c6-49bb-b2a7-acf3cfadc257)
    )
    (fp_text user "GPIO37" (at 24.13 25.4 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 172d387f-2da9-4e81-896d-415b839426d7)
    )
    (fp_text user "GND" (at 24.13 0 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 17c94def-bf44-4cce-a603-f7f2a5ed5034)
    )
    (fp_text user "GPIO44/U0RXD" (at 24.13 5.08 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 1c4019f2-b24f-47cd-8efb-76cb1a60b394)
    )
    (fp_text user "EN/RESET" (at 8.88632 5.07728 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 1f5f9a1a-1ff1-454a-bed2-354e8f05b102)
    )
    (fp_text user "3V3" (at 1.27 2.54 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 21f28454-7a80-4f47-9075-c88cf4ba9c51)
    )
    (fp_text user "GND" (at 24.13 50.8 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 23d8a57a-9196-45c1-b1fd-b276e56d930b)
    )
    (fp_text user "GPIO6" (at 1.27 12.7 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 30cad151-585e-4515-addd-66045a91c629)
    )
    (fp_text user "GPIO11" (at 1.27 40.64 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 372f3afc-ea01-4254-bedc-906b3c1112c0)
    )
    (fp_text user "GPIO18" (at 1.27 25.4 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 44e71d69-8176-4519-ad81-26123e73a6a1)
    )
    (fp_text user "GPIO4" (at 1.27 7.62 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 46044653-081f-48fe-924d-f95dc6ea0252)
    )
    (fp_text user "GPIO15" (at 1.27 17.78 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 46aa94e1-5f4a-424f-bf2c-7271f52b0153)
    )
    (fp_text user "GPIO1" (at 24.13 7.62 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 55d6863d-3c91-4dd6-9c7e-a19cb20cfe9c)
    )
    (fp_text user "GPIO38" (at 24.13 22.86 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 65575020-5f5a-466c-97af-74126f9b632d)
    )
    (fp_text user "GPIO16" (at 1.27 20.32 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 6957ada3-354e-4f05-9f5a-d32fedada077)
    )
    (fp_text user "GPIO42/MTMS" (at 24.13 12.7 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 6ef3680d-5561-4f26-944b-b09730b64b2b)
    )
    (fp_text user "GPIO0" (at 24.13 33.02 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 70e5c0fe-c929-4eee-a09c-ea91f34c56ea)
    )
    (fp_text user "GPIO7" (at 1.27 15.24 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 80bda145-7594-447a-9341-642569644bfe)
    )
    (fp_text user "GPIO8" (at 1.27 27.94 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 8195eea1-1501-4fe4-b54c-152bfe416de9)
    )
    (fp_text user "GPIO5" (at 1.27 10.16 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp 82bdddae-b19d-4ff3-a994-0ec704b75a8a)
    )
    (fp_text user "GPIO40/MTDO" (at 24.13 17.78 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 84c16838-d617-4f5a-bf5e-538e0d87bf3d)
    )
    (fp_text user "GPIO47" (at 24.13 40.64 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 87dcff9f-e597-4cee-8b0b-c3e16c22a555)
    )
    (fp_text user "GPIO36" (at 24.13 27.94 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp 9b532aad-2251-4775-8e22-82003f808bfb)
    )
    (fp_text user "GPIO19" (at 24.13 48.26 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp ad5a24cd-ef55-44ef-847f-35cfc367a7c2)
    )
    (fp_text user "5V" (at 1.52032 50.79728 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp aed3f275-64cc-4f52-aed7-fd368f3c2dd4)
    )
    (fp_text user "GPIO17" (at 1.27 22.86 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp b0bfdf70-dbf4-41fe-8594-8916e02563e2)
    )
    (fp_text user "GPIO10" (at 1.27 38.1 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp b24a9527-bfe7-461a-abd4-6eeadd744e08)
    )
    (fp_text user "GPIO46" (at 1.27 33.02 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp b99fa53d-8458-48df-9bca-030860370cdd)
    )
    (fp_text user "3V3" (at 1.27 0 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp c1a2810e-b152-4fa5-b045-01da47ee2d93)
    )
    (fp_text user "GPIO41/MTDI" (at 24.13 15.24 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp cc31f02c-534a-4ffc-bf50-736224884534)
    )
    (fp_text user "GPIO12" (at 1.27 43.18 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp cc3b5557-39bc-4780-bd69-002a8f7e6169)
    )
    (fp_text user "GND" (at 24.13 53.34 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp cc410fb2-3e7c-4478-b464-6833f549b142)
    )
    (fp_text user "GPIO39/MTCK" (at 24.13 20.32 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp e3e626b8-fe97-410f-8b42-50dd9fad0a22)
    )
    (fp_text user "GPIO9" (at 1.27 35.56 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp e4e2d19e-1c01-4f53-95ba-dc9c84bf9ef5)
    )
    (fp_text user "GPIO35" (at 24.13 30.48 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp e50ce6c6-3ef3-4082-b8c2-d2951f4e7fb8)
    )
    (fp_text user "GPIO21" (at 24.13 43.18 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp e9f0687c-c95f-4d7e-8016-62cf74f88fac)
    )
    (fp_text user "GND" (at 1.52032 53.33728 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp eadded73-b3eb-4298-9ab4-f17721d47ae4)
    )
    (fp_text user "GPIO43/U0TXD" (at 24.13 2.54 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp ee22429e-f94e-42cc-abec-b51cdcad3e98)
    )
    (fp_text user "GPIO13" (at 1.27 45.72 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify left))
      (tstamp efe09c35-44b9-4e6c-908f-540d26605ef3)
    )
    (fp_text user "GPIO2" (at 24.13 10.16 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp f679fa93-0c64-4853-9519-a6924a817f81)
    )
    (fp_text user "GPIO45" (at 24.13 35.56 -90 unlocked) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)) (justify right))
      (tstamp fb92b2f4-36f2-4819-bc92-de9449cd156f)
    )
    (fp_text user "REF**" (at -0.00368 -0.00272 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 65bab322-e3e0-4812-8cbe-522c087d960a)
    )
    (fp_line (start -1.5 55.114) (end 26.899999 55.114)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cfd2af9b-3bbf-4810-810b-51b9ba8cf101))
    (fp_line (start -1.499999 -1.1) (end -1.5 55.114)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e63f9436-daa2-4dfa-be76-b08dd5ebb129))
    (fp_line (start 2.46012 -7.01312) (end 22.98332 -7.01312)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c62e6914-84d9-4bc6-9207-3e6af0049823))
    (fp_line (start 2.46012 -1.12032) (end 2.46012 -7.01312)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 247a1679-1159-44a0-b1a7-8d8a87c69ff7))
    (fp_line (start 22.98332 -7.01312) (end 22.98332 -1.12032)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 98634b5d-c062-42ae-b4cd-858a0d9efa60))
    (fp_line (start 26.899999 55.114) (end 26.9 -1.1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6f4963d9-cda0-4ee3-a8b0-d645932c7933))
    (fp_line (start 26.9 -1.1) (end -1.499999 -1.1)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 52f30b0b-2055-4e67-bbcf-ca77d8d01dc3))
    (fp_line (start -1.25 -0.85) (end 26.65 -0.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 57654b5a-a778-46e2-b695-f9d30b94e59c))
    (fp_line (start -1.25 54.864) (end -1.25 -0.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 210d0592-f56a-4722-8ea2-199a00a89faa))
    (fp_line (start 26.65 -0.85) (end 26.65 54.864)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a6c795b4-db2a-423c-8a2c-2a68ba1897d5))
    (fp_line (start 26.65 54.864) (end -1.25 54.864)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 167d612e-a4e9-486f-804a-4ea01987d94a))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U2-3V3-Pad1)") (pinfunction "3V3") (pintype "passive") (tstamp 99639fe2-869d-4e7d-b108-fb86d1da4e96))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(U2-3V3-Pad1)") (pinfunction "3V3") (pintype "power_in") (tstamp c5b44675-77c6-49a8-a6e0-07574b1ca9a8))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(U2-CHIP_PU-Pad3)") (pinfunction "CHIP_PU") (pintype "input") (tstamp 6e00431e-c3de-4cd6-bbb9-ae68373c68f1))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 54 "BCD4") (pinfunction "GPIO4/ADC1_CH3") (pintype "bidirectional") (tstamp 0e484371-3ad9-4514-b53b-ae0fe7ac84ad))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 52 "M01") (pinfunction "GPIO5/ADC1_CH4") (pintype "bidirectional") (tstamp 126dc548-ea89-4b63-8fef-0443b839ec66))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 51 "M10") (pinfunction "GPIO6/ADC1_CH5") (pintype "bidirectional") (tstamp 48460513-94e6-443a-a522-83da01ca9f0c))
    (pad "7" thru_hole oval (at 0 15.24 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 50 "H01") (pinfunction "GPIO7/ADC1_CH6") (pintype "bidirectional") (tstamp 1fc2d15a-6b82-4558-b7cc-21ea5053ccbf))
    (pad "8" thru_hole oval (at 0 17.78 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(U2-GPIO15{slash}ADC2_CH4{slash}32K_P-Pad8)") (pinfunction "GPIO15/ADC2_CH4/32K_P") (pintype "bidirectional") (tstamp 0df4e738-64ac-459b-9e84-bd5f7f38c767))
    (pad "9" thru_hole oval (at 0 20.32 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 60 "unconnected-(U2-GPIO16{slash}ADC2_CH5{slash}32K_N-Pad9)") (pinfunction "GPIO16/ADC2_CH5/32K_N") (pintype "bidirectional") (tstamp e65eff06-f2a3-44d0-85fb-985e107df74c))
    (pad "10" thru_hole oval (at 0 22.86 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(U2-GPIO17{slash}ADC2_CH6-Pad10)") (pinfunction "GPIO17/ADC2_CH6") (pintype "bidirectional") (tstamp 9fe959a4-7bbb-4b60-98dd-fd6b766e3fba))
    (pad "11" thru_hole oval (at 0 25.4 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(U2-GPIO18{slash}ADC2_CH7-Pad11)") (pinfunction "GPIO18/ADC2_CH7") (pintype "bidirectional") (tstamp 8acceb55-5cae-4c25-9dc8-c4cac94be243))
    (pad "12" thru_hole oval (at 0 27.94 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 49 "H10") (pinfunction "GPIO8/ADC1_CH7") (pintype "bidirectional") (tstamp 34ab4ead-f276-42b8-b696-298fbf42b0c1))
    (pad "13" thru_hole oval (at 0 30.48 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 56 "BCD3") (pinfunction "GPIO3/ADC1_CH2") (pintype "bidirectional") (tstamp fa445b81-1b7e-4c71-8afc-d4d8cff48720))
    (pad "14" thru_hole oval (at 0 33.02 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(U2-GPIO46-Pad14)") (pinfunction "GPIO46") (pintype "bidirectional") (tstamp abcdcf89-fd20-4eee-a8e3-71402413e31c))
    (pad "15" thru_hole oval (at 0 35.56 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(U2-GPIO9{slash}ADC1_CH8-Pad15)") (pinfunction "GPIO9/ADC1_CH8") (pintype "bidirectional") (tstamp 43b967c5-0736-42ec-9827-93186bfadcc7))
    (pad "16" thru_hole oval (at 0 38.1 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(U2-GPIO10{slash}ADC1_CH9-Pad16)") (pinfunction "GPIO10/ADC1_CH9") (pintype "bidirectional") (tstamp 6469349c-404e-45aa-828f-e318d05b10b3))
    (pad "17" thru_hole oval (at 0 40.64 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 66 "unconnected-(U2-GPIO11{slash}ADC2_CH0-Pad17)") (pinfunction "GPIO11/ADC2_CH0") (pintype "bidirectional") (tstamp 98eede88-dc02-441f-90ae-49dc731d278f))
    (pad "18" thru_hole oval (at 0 43.18 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(U2-GPIO12{slash}ADC2_CH1-Pad18)") (pinfunction "GPIO12/ADC2_CH1") (pintype "bidirectional") (tstamp 6feba685-d03f-485a-beab-00582af1b04e))
    (pad "19" thru_hole oval (at 0 45.72 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(U2-GPIO13{slash}ADC2_CH2-Pad19)") (pinfunction "GPIO13/ADC2_CH2") (pintype "bidirectional") (tstamp b4d2c7df-f4dd-48a9-8f10-51181bfd7aa8))
    (pad "20" thru_hole oval (at -0.00368 48.25728 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(U2-GPIO14{slash}ADC2_CH3-Pad20)") (pinfunction "GPIO14/ADC2_CH3") (pintype "bidirectional") (tstamp ebd75c4d-f595-4056-92d3-d49c0250af8d))
    (pad "21" thru_hole oval (at -0.00368 50.79728 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "+5V") (pinfunction "5V") (pintype "power_in") (tstamp f723e58b-43f2-4723-a2bc-564e105cfd4e))
    (pad "22" thru_hole oval (at -0.00368 53.33728 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "passive") (tstamp af61ed67-bb56-41b4-9c77-74ae8afbf337))
    (pad "23" thru_hole oval (at 25.4 53.34 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "passive") (tstamp 225a76bf-4a90-46ca-8236-73ce558f2a64))
    (pad "24" thru_hole oval (at 25.4 50.8 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "passive") (tstamp fe7d8f37-1b5d-4563-8c3b-cf09ee4c00e8))
    (pad "25" thru_hole oval (at 25.4 48.26 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/Horloge Nixie/USB_D-") (pinfunction "GPIO19/USB_D-") (pintype "bidirectional") (tstamp 301fe7c5-df02-4552-99c2-b93098aabb37))
    (pad "26" thru_hole oval (at 25.4 45.72 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/Horloge Nixie/USB_D+") (pinfunction "GPIO20/USB_D+") (pintype "bidirectional") (tstamp 67c28bd8-4af4-427d-8d63-73dbdb4256c6))
    (pad "27" thru_hole oval (at 25.4 43.18 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 70 "unconnected-(U2-GPIO21-Pad27)") (pinfunction "GPIO21") (pintype "bidirectional") (tstamp 71932483-25e6-47c3-b37c-cce8b9a87feb))
    (pad "28" thru_hole oval (at 25.4 40.64 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(U2-GPIO47-Pad28)") (pinfunction "GPIO47") (pintype "bidirectional") (tstamp a7d1228b-cf90-4047-8189-10f108451be9))
    (pad "29" thru_hole oval (at 25.4 38.1 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(U2-GPIO48-Pad29)") (pinfunction "GPIO48") (pintype "bidirectional") (tstamp 38d41edd-773d-4d33-aa19-5b9d9f7e95b2))
    (pad "30" thru_hole oval (at 25.4 35.56 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 73 "unconnected-(U2-GPIO45-Pad30)") (pinfunction "GPIO45") (pintype "bidirectional") (tstamp efb57b62-aedc-4384-8177-77233eca1e33))
    (pad "31" thru_hole oval (at 25.4 33.02 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 74 "unconnected-(U2-GPIO0-Pad31)") (pinfunction "GPIO0") (pintype "bidirectional") (tstamp 4f472334-b379-4a62-8f5d-49bbc13a3fd7))
    (pad "32" thru_hole oval (at 25.4 30.48 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(U2-GPIO35)") (pinfunction "GPIO35") (pintype "bidirectional") (tstamp d99123f3-79dd-427e-9f96-cad9936d8f3e))
    (pad "33" thru_hole oval (at 25.4 27.94 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 76 "Net-(U2-GPIO36)") (pinfunction "GPIO36") (pintype "bidirectional") (tstamp 3475839c-39cf-4329-be92-bcea48fd48fa))
    (pad "34" thru_hole oval (at 25.4 25.4 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(U2-GPIO37)") (pinfunction "GPIO37") (pintype "bidirectional") (tstamp b6b23fbd-e1b4-451d-a630-f68a56beece4))
    (pad "35" thru_hole oval (at 25.4 22.86 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 78 "unconnected-(U2-GPIO38-Pad35)") (pinfunction "GPIO38") (pintype "bidirectional") (tstamp 407f4b74-b6a0-4ea4-889d-0b4ca0025839))
    (pad "36" thru_hole oval (at 25.4 20.32 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 79 "unconnected-(U2-GPIO39{slash}MTCK-Pad36)") (pinfunction "GPIO39/MTCK") (pintype "bidirectional") (tstamp 1ae651f7-3062-460d-be7f-7eacab3292ff))
    (pad "37" thru_hole oval (at 25.4 17.78 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 80 "unconnected-(U2-GPIO40{slash}MTDO-Pad37)") (pinfunction "GPIO40/MTDO") (pintype "bidirectional") (tstamp e0c3ca5f-1570-4d45-bffc-7a9230a00459))
    (pad "38" thru_hole oval (at 25.4 15.24 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "/Horloge Nixie/I2C_SCL") (pinfunction "GPIO41/MTDI") (pintype "bidirectional") (tstamp f3d49e83-9fe3-4be3-bf4b-982a40de30b2))
    (pad "39" thru_hole oval (at 25.4 12.7 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "/Horloge Nixie/I2C_SDA") (pinfunction "GPIO42/MTMS") (pintype "bidirectional") (tstamp 87e6da8a-523f-4694-9159-3e94c8bb4cd9))
    (pad "40" thru_hole oval (at 25.4 10.16 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 55 "BCD2") (pinfunction "GPIO2/ADC1_CH1") (pintype "bidirectional") (tstamp cbc740ff-8ed9-44e7-a138-b4e033385b84))
    (pad "41" thru_hole oval (at 25.4 7.62 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 53 "BCD1") (pinfunction "GPIO1/ADC1_CH0") (pintype "bidirectional") (tstamp c876b616-968b-42bf-a7c5-adac5d78cb59))
    (pad "42" thru_hole oval (at 25.4 5.08 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 81 "unconnected-(U2-GPIO44{slash}U0RXD-Pad42)") (pinfunction "GPIO44/U0RXD") (pintype "bidirectional") (tstamp 924a0de7-5287-4b35-8ebe-34bc33ecfbf1))
    (pad "43" thru_hole oval (at 25.4 2.54 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 82 "unconnected-(U2-GPIO43{slash}U0TXD-Pad43)") (pinfunction "GPIO43/U0TXD") (pintype "bidirectional") (tstamp 77a8d6e7-8911-4351-a0e5-3092d6e09c09))
    (pad "44" thru_hole oval (at 25.4 0 180) (size 1.2 2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 19100101-6a29-4504-bced-f0c13cdc0af1))
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tstamp e99a6403-4f57-4319-9654-4bc6a6cfc08a)
    (at 172.53 42.8)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "8A Ic, 400V Vce, Silicon Switching Power NPN Transistors, TO-220")
    (property "ki_keywords" "Switching Power NPN Transistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/0ca726e4-7b2d-4fba-9c3f-fa1046cb65f2")
    (attr through_hole)
    (fp_text reference "Q8" (at 1.27 -3.56) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 405ce65f-57af-43eb-88c0-084efdfbaa96)
    )
    (fp_text value "MPSA42" (at 1.27 2.79) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b6599fb5-5a1e-49af-bb86-3a548c92d7ec)
    )
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ccb9c127-049d-449f-803b-89c998079ce7)
    )
    (fp_line (start -0.53 1.85) (end 3.07 1.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d2c9ea1f-fda9-4645-aeaa-a3d1f3d8b925))
    (fp_arc (start -0.568478 1.838478) (mid -1.132087 -0.994977) (end 1.27 -2.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 87ffa3af-a7d2-46e2-84f3-f23da316f184))
    (fp_arc (start 1.27 -2.6) (mid 3.672087 -0.994977) (end 3.108478 1.838478)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d98ecc78-5d6b-4f17-a4b0-fdc446d7dbe2))
    (fp_line (start -1.46 -2.73) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ee1496b9-6b16-4d31-b3bc-2fa3fe1dac3b))
    (fp_line (start -1.46 -2.73) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0261d793-c9f1-4c02-a218-ff3d0e91ac2a))
    (fp_line (start 4 2.01) (end -1.46 2.01)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4a6350b3-4007-4121-aac6-2ad057f4e745))
    (fp_line (start 4 2.01) (end 4 -2.73)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9237dda7-fb7c-4cea-8644-b24652fcad89))
    (fp_line (start -0.5 1.75) (end 3 1.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 39c32dfd-0660-44c5-96a2-9c738078d1c0))
    (fp_arc (start -0.483625 1.753625) (mid -1.021221 -0.949055) (end 1.27 -2.48)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4def58d0-6d33-4ae3-899d-2244fa8dc28c))
    (fp_arc (start 1.27 -2.48) (mid 3.561221 -0.949055) (end 3.023625 1.753625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ae63dc77-63e0-46bd-bd96-13a73ab60f0b))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(Q8-B)") (pinfunction "B") (pintype "input") (tstamp 6c4129fc-d498-489f-a300-f85c4da4c885))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(Q8-C)") (pinfunction "C") (pintype "passive") (tstamp 51cede9b-f11c-4131-a593-fcaf7e04ca30))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "E") (pintype "passive") (tstamp 2c8cb671-c37f-4b9f-b142-cbda66f353eb))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tstamp f79f47fa-4cdb-4819-a2a7-dc1872aa2228)
    (at 141.8 33.8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "untitled.kicad_sch")
    (property "Sheetname" "Horloge Nixie")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/85850350-b5ad-4932-92cb-a375dee25730/f4277f74-9886-44e8-b205-9cac644dfc93")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0c62829-6366-48a6-a78b-366eae537513)
    )
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 28ec369b-d5e1-40b2-9920-389f918159e8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp bbd22600-df9d-4203-948c-a3e7ec6640d8)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fcb28359-c514-4ede-9924-a60438f08865))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 708da0b2-91ce-43d5-93b0-f368e2089117))
    (fp_line (start -1.85 -0.95) (end 1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cc6fa98a-1a27-4af5-b233-b5096865c619))
    (fp_line (start -1.85 0.95) (end -1.85 -0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 034174f6-d0fe-45af-b248-350282d38162))
    (fp_line (start 1.85 -0.95) (end 1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7ba23e55-d65f-4542-a194-da0a894a936e))
    (fp_line (start 1.85 0.95) (end -1.85 0.95)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c2a4b3e3-75fc-43f0-82d0-0d2d9ca2db11))
    (fp_line (start -1 -0.625) (end 1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e108f8d-767e-42b9-853b-61756ffb56d5))
    (fp_line (start -1 0.625) (end -1 -0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 51620fc1-ceeb-4a9c-9390-83c865366f9b))
    (fp_line (start 1 -0.625) (end 1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c15a1d5-9e4d-4925-8c85-4e42913c394d))
    (fp_line (start 1 0.625) (end -1 0.625)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2ca65f37-8796-4ac5-b15c-a8f3f91cdd46))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 38 "Net-(Q3-B)") (pintype "passive") (tstamp a17c4fdf-f0d4-449b-a6a4-ccc8a72971a6))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 10 "HT") (pintype "passive") (tstamp 5faa95ce-dc13-4d8f-b6a5-34fbfcb544ca))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tstamp feeddce8-11da-41b9-bdab-11f00f192777)
    (at 175.8 55.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fd563363-7a17-4f8c-87a2-d2679d06de9c)
    )
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fdf22a3d-14a9-404d-914d-53f6b4388b68)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19036cc9-b417-45c3-8465-55f9ee5ec199)
    )
    (fp_circle (center 0 0) (end 3.2 0)
      (stroke (width 0.15) (type solid)) (fill none) (layer "Cmts.User") (tstamp 65b7b46d-b04b-4b4a-99f7-6b70673492da))
    (fp_circle (center 0 0) (end 3.45 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp f8cc41a2-f219-4b9c-8458-7e47f98fa7f8))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "F&B.Cu" "*.Mask") (tstamp 31bf90e7-5aec-49f7-aa00-ba4d65d19694))
  )

  (gr_rect (start 50.8 50.8) (end 179.8 120.8)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 978ab02a-4d02-4f36-9c71-6b032c574b96))
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 10404ab6-f20f-48d5-a5b9-c84f81ea443d)
    (pts (xy 48.8 106.8) (xy 48.8 110.8))
    (height 3)
    (gr_text "4 mm" (at 43.8 108.8 90) (layer "Dwgs.User") (tstamp 10404ab6-f20f-48d5-a5b9-c84f81ea443d)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5))
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 22c28744-5d7e-4bf8-8048-23db71a5565d)
    (pts (xy 48.8 54.8) (xy 48.8 106.8))
    (height 3)
    (gr_text "52 mm" (at 44.65 80.8 90) (layer "Dwgs.User") (tstamp 22c28744-5d7e-4bf8-8048-23db71a5565d)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 33737eb9-0750-447a-8981-ee77596297d5)
    (pts (xy 42.8 110.8) (xy 42.8 50.8))
    (height -2)
    (gr_text "60 mm" (at 39.8 80.8 90) (layer "Dwgs.User") (tstamp 33737eb9-0750-447a-8981-ee77596297d5)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp 696cb32d-76f9-483d-93ea-19fa109940ca)
    (pts (xy 48.8 50.8) (xy 48.8 54.8))
    (height 3)
    (gr_text "4 mm" (at 43.8 52.8 90) (layer "Dwgs.User") (tstamp 696cb32d-76f9-483d-93ea-19fa109940ca)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5))
  )
  (dimension (type aligned) (layer "Dwgs.User") (tstamp f5243de0-5dc3-4a59-8fa6-89f61ca630e3)
    (pts (xy 50.8 126.8) (xy 180.8 126.8))
    (height 5)
    (gr_text "130 mm" (at 150.8 130.8) (layer "Dwgs.User") (tstamp f5243de0-5dc3-4a59-8fa6-89f61ca630e3)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 0))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5))
  )

)
